



Open DCB operation failed.
End of file encountered.

Invalid function input argument.
Invalid operation on target object.
Could not open job information (JCB) file.
Could not read job information (JCB) record number %d.
Could not update job information (JCB) record number %d.
Could not open job information (JDB) file.
Could not read job information (JDB) record.
Count or size mismatch has occurred while reading a system data file.
Could not allocate required memory (heap space).
A required system object or service was not found.
A request for an operating system resource (other than memory) has failed.
     
Error (%d) attaching to server %.80s.
Error (%d) logging into server %.80s as %.48s.
Error (%d) on drive %c.
Error (%d) accessing %.80s.
Error (%d) accessing server  - %.80s.
Error (%d) mapping a drive to %.80s.

Network connection ID is not valid (%d).
No drives available for mapping.
Error (%d) occurred during a file server bindery scan.
Unexpected error code received (%d).
Error (%d) unmapping drive %c.
A lock attempt has failed.      
    
An unlock attempt has failed.   





An unexpected error occurred while attempting to advertising an HSM service.
Network connection was terminated.
Error establishing a network connection.
Fatal resource error.
Fatal error occurred while attempting to find a server.
Fatal send error - connection is gone.
Server name is already in use.
Server does not respond.
No HSM message buffers are currently available.
No HSM messages are currently on the message queue.
SPX has not been loaded.
Message packet to be sent was too large.
Server name was not found.
Temporary error finding server.  A retry operation should be performed.
Too many network connections have been requested.
Unknown error establishing a network connection (%u).
Unknown error receiving a message packet (%u).
Unknown error finding server (%u).
Unknown error sending a message packet (%u).
Unknown error terminating a network connection (%u).




The HSM input Class value %d is out of range.
The HSM input Type value %d is out of range.
Unable to open file %.80s.
No volumes are configured as a system volume.  The minimum requirement is one.
Unable to write file %.80s.
An attempt to seek within file %.80s has failed.
An attempt to access configuration memory has failed.
An error has occurred in the configuration code.
Unable to contact secondary storage devices.
Unable to read file %.80s.
Error reading device description information from the Installation .INI file.
The input string was too long.
Links failed to initialize Network Services.
Links received a message packet out of sequence.
Links did not receive the message packet it expected.
Links could not find the requested HSM service.
The network connection was terminated normally.
Links did not receive a reply message.
A DOS error has occurred with error code %d.
A network error has occurred with error code %d.


Configuration conflict between Media Service and Configuration Service.
Memory allocation failed for a block of %d bytes.
The HSM handle %lx is not valid.
The HSM Class %hd is not valid.
The HSM Type %hd is not valid.
The HSM Group %hd is not valid.
Error encountered while scanning the Media Database during initialization.
A mismatch has occurred between what media object is mounted in a transport and what is recorded in the Media Database.  The mismatch is being corrected.
A requested state change for a media object isn't valid, based upon the current state of the media object.
HSM internal logic error:  Media Service could not find a free media object where one was expected.

During initialization Configuration Service reports a Class that Media Service hasn't configured.
During initialization Media Service has a Class configured that Configuration Service doesn't report.
During initialization Configuration Service reports a Group that Media Service hasn't configured.
During initialization Media Service configured a Group that Configuration Service didn't report.
During initialization Media Service and Configuration Service don't report the same number of slots for a Group.
An invalid request (%d) was received by an HSM work task.
HSM internal logic error:  Invalid state %d detected in an HSM work task.
Send of HSM mail failed with error %d.
Session constructor returned error %d.
Session error %d for HSM handle %lx returned.
Session add returned error %d.
Invalid HSM data control block (DCB) type %d detected.
An unexpected error was returned from Media Service.
HSM detected an invalid reply %d from an HSM work task.
An unexpected error was returned from List Service.
Unable to reschedule an job, job may need to be rescheduled using AVSTOMAN.
Unable to delete a record from file %.80s.
HSM internal logic error:  invalid function argument.

Record Management file %.80s not closed prior to HSM shutdown.
Record file %.80s opened with different %.80s value(s).
Record Management table out of space detected during open of file %.80s.
Error finding %.80s during %.80s operation.

Initialization of an HSM object or service (%.80s) failed.

Ran out of space on Novell file server volume %.80s.
Received unknown error %d from Device Service process file.




Error occurred while scanning list of Job Control Blocks (JCBs).
An HSM service function was requested that does not exist.  The function identifier was %d.


An open for an HSM service was requested when a session was already active. 
Unable to remove file %.80s.
Node %04X %08lX cannot be accessed in the Storage Catalog.

Could not find the Job Queue mail box.
Could not find the Hierarchy Manager mail box.
Error (%d) reading extended attribute information on %.80s.
Could not update JCB (job '%.80s'), JCB %d was in use.
Recall job '%.80s' failed (JCB %d).




Migrate job '%.80s' failed (JCB %d).


Could not open job information (JCB blocks) for job '%.80s' (JCB %d).
Could not open DCB blocks for DCB header %d while processing job '%.80s' (JCB %d).
Could not get handle for volume '%.80s' while processing job '%.80s' (JCB %d).
Could not get secondary storage media handle from catalog for file %.80s while processing job '%.80s' (JCB %d).

Could not connect to volume '%.80s' while processing job '%.80s' (JCB %d).
No filespecs found for job '%.80s' (JCB %d).
Could not add DCB header while processing job '%.80s' (JCB %d).
Could not add DCB filespec blocks to DCB header %d while processing job '%.80s' (JCB %d).
Could not update DCB header %d while processing job '%.80s' (JCB %d).
Could not update JCB header while processing job '%.80s' (JCB %d).
Could not update JCB while processing job '%.80s' (JCB %d).
A Link Service message block was too small for the message received.
Unable to establish a network connection with a file server.  HSM handle value was %08lX.
Invalid data has been detected in Storage Catalog %.128s.
File %.80s was not added to the Storage Catalog because of previous error.
Node %04X %08lX could not be deleted from the Storage Catalog because of a previous error.

Reference to a Storage Catalog path record %d could not be deleted.  The record usage count is %d.

Could not find Hierarchy Manager mailbox.
Could not get old file name from catalog for %.80s.
Cannot recall file %.80s because BAG information for the file cannot be retrieved.
Could not get volume handle for demand recall of file %.80s.
Error adding demand recall DCB for file %.80s.
Error updating demand recall DCB for file %.80s.
Error opening Data Control Blocks (DCBs) for demand recall of file %.80s.
Media handle %08lX for node %04X %08lX could not be set because of a previous error.
The primary database file appears to be corrupted and will no longer be used.
The backup database file appears corrupted and will no longer be used.
HSM internal logic error: encountered in File Mirroring Service.
Primary and mirrored files for %.80s contain invalid data.
Primary and mirrored files for %.80s contained different data.
Storage Catalog node %04X %08lX could not be deleted from the %08lX Media List.
Storage Catalog node %04X %08lX could not be added to the %04X Bag List.
The maximum number of unique paths for a server volume has been exceeded.
The specified volume does not have any file controls associated with it.
An unknown error occurred in the File Control Service.
The next entry in %04X Bag List could not be committed.  The node ID is %04X %08lX.
Could not delete temporary job information.
The Media List for media handle %08lX was not erased.
Could not get migrate class from the Configuration Service.
An unknown setting <%.80s> was detected in an HSM .INI file.


Unable to start an operating system process or thread.
Memory allocation failed (Device Service).
Device Service received a request to terminate a device driver that is not currently started.
Failed to open the HSM .INI file for the requested driver.
Failed to read the HSM .INI file for the requested driver.
Failed to read enough bytes from an HSM .INI file.
ASPI driver not present.
Got an unexpected message type in response to an HSM service request.
A Device Services protocol violation has been detected.
HSM device handle is bad or device does not exist.
The specified Device Service DEAMON name is bad or does not exist.
Device Service attempt to allocate memory failed.
The Device Service session or device is currently owned by another thread.
The Device Service session handle is invalid.
The Device Service endpoint 'type' is invalid
The Device Service endpoint 'type' (src or dest) is already assigned
The ESOS TSR program is not loaded.
Device Service unable to find a file (same as ENOENT).
Device Service could not access a file.
A request to start an HSM service cannot be performed:  the service is already running.
The requested HSM service is not currently started.
The Device Service request is not supported or is currently illegal for the device.
Too many Device Control Threads (DCTs) are active.
The specified device is already assigned to a Device Service session.
There is already a Device Control Thread (DCT) running for the specified device.
An HSM internal logic error has occurred.
Could not add record to an HSM system file.

Could not read an HSM system file record.
Could not get configuration data for volume %lx.
Could not get volume utilization for volume %lx.
Could not get file control information for volume %lx.
Could not open temporary file for volume sweep (volume %lx, file %d).
Could not get migrate media class.
Could not find Hierarchy Manager mailbox for job type %d.
Could not delete extended attributes for file <%.80s>.
Could not delete catalog entry for file <%.80s>.
Could not read sweep job data blocks for job <%.80s>, JCB %d.
A sweep job could not be completed.
Could not create placeholder file for file <%.80s>.
The media object mounted for writing is write protected.
Failed to create the Device Service session index file.
An unrecoverable error was encountered on a transport.
There is no media object in the source device.
There is no media object in the destination device.
Encountered unexpected end of media.
Physical end of media has been detected.
Media error detected.
Hardware error detected.
Could not find mailbox for the HSM Space Manager Task.
Error occurred while checking volume free space levels.
Could not get volume utilization for volume %lx.
Could not get volume utilization thresholds for volume %lx.
Error scanning configured servers for low space.
Error scanning configured server volumes for low space.
Could not connect to volume %.80s (%lx) to check free space level.
Error accessing critical migration list.
Node %04X %08lX could not be recalled from the Storage Catalog.
An error occurred during the transfer of Media List entries from %08lX to %08lX.
Node %04X %08lX could not be deleted from the %04X Bag List.
A new Backup Access Group (BAG) could not be created.
The %04X Bag could not be found.
An error occurred while accessing the Bag Info File.
Volume Totals: %lu files, %lu bytes
No shadow device was available for assignment.
An error occurred while accessing the %04X Bag List file.
An error occurred while accessing the %08lX Media List file.
Storage Catalog node %04X %08lX could not be added to the %08lX Media List.
The next entry in %08lX Media List could not be committed.  The node ID is %04X %08lX.

Could not open statistics database.

Could not read statistics record for HSM handle %08lx.
Could not open statistics database record for HSM handle %08lx.
Could not add statistics record for HSM handle %08lx.
Could not update statistics data for HSM handle %08lx (code = %d).

Statistics data for HSM handle %08lx is locked.
Bad HSM handle type for statistics operation (handle %08lx).
Out of space for the current user.
A request to suspend a data transfer stream was received after the stream was completed.
Restore-file job '%.80s' failed (JCB %d).
Restore-media job '%.80s' failed (JCB %d) for media %08lx.
Could not get out-of-space message from text database.
Could not get server/volume name from configuration for volume %08lx.
Server/volume '%.80s' is above the CRITICAL level, HSM could not find files to migrate which meet the migration criteria currently set for the volume.
A configured library has no transport associated with it.
A configured library has no robotic arm associated with it.
The minimum secondary storage and backup device configuration requirements do not exist.
The minimum number of migration volumes have not been configured.  The minimum requirement is %d.  The system will not start until the minimum configuration requirements are met.  See the Installation Guide for more information.
The minimum number of shadow volumes have not been configured.  The minimum requirement is %d.  The system will not start until the minimum configuration requirements are met.  See the Installation Guide for more information.
The minimum number of backup devices are not configured. The minimum requirement is %d.  The system will not start until the minimum configuration requirements are met.  See the installation guide for more information.
The minimum number of tape library devices have not been configured.  The minimum requirement is %d.  The system will not start until the minimum configuration requirements are met.  See the Installation Guide for more information.


Primary and mirrored files for %.80s contain different data.  Files must be corrected before HSM system activity can continue.
Mirrored file for %.80s contains invalid data.
Primary file for %.80s contains invalid data.
File mirroring operation error in file %.80s: primary code=%d, mirror code=%d.
Could not write to the required parameters file.
Recovery was required for the configuration database %.80s.  The last configuration changes may be lost.

Failed to recover configuration database error for file %.80s.

Could not update job information (JDB) record number %d.
Error occurred setting job status to RUNNING
Error occurred reading/updating job information
Error occurred building list of files for job
Error occurred accessing volume information in the Configuration Database
Error occurred building job information
Error occurred initializing sweep job information
Error scanning volume for eligible files for an HSM sweep job
No file(s) processed for file specification '%s'
No file(s) processed for volume '%.128s'
Warning: Job was interrupted and did not finish
Warning: Job was missed
Error occurred setting up data transfer connection for job
Warning: %s not found
Error occurred while processing file '%s'
Warning: %s has not been backed up
Warning: %s is too large to migrate
Warning: %s is too small to migrate
Warning: %s is EXECUTE-ONLY and cannot be migrated
Error reading message %d from the HSM Message Text Database.
No file(s) processed for the job
Primary and mirrored files for %.128s contained different data in record %ld.
Unable to rename file %.80s.
Server volume %lx is completely out of space, cannot migrate files.
Server volume is out of space, information for migrated files cannot be created
Device failed diagnostic test(s).
Library command failed because access door was open.
The library access door was opened and closed.
A Unit Attention message was received from the SCSI device.
The SCSI device aborted a command.
An unsupported error was received from a SCSI device.
SCSI error detected - key:%1x asc:%2x ascq:%2x.
The serial number was not found on the target media.
A label could not be found on a media object.
Failed to read the media header.
Backup Database %s is corrupted.  Primary copy does not match the mirror copy.
A new backup media volume tag could not be created.
Backup media volume tag %s could not be added to the Backup Database.
The reference to the volume tag for backup media %08lX could not be deleted.
The maximum number of backup tapes supported has been exceeded.
Could not delete record %ld in file %s.
A session mark for the backup device has been lost.  The session mark was for backup cartridge %08lX.  No action is required.
A reference for backup media handle %08lX could not be added to the Backup Database.
Error creating or accessing data transfer session mark on the media.
State of library import/export port is not what was expected.
Job: %.80s
File: %.80s
System startup
System shutdown
Volume: %.80s
Library: %.80s  Slot: %d
Storage volume: %.80s
Scan complete
Error reading message %d from the HSM Message Text Database.
Exabyte 8500 fault: key:%1x asc:%2x ascq:%2x fsc:%x
Media header block and stream header checksum do not match.
The vendor id in the MTF tape data block is not correct.
HSM internal logic error:  invalid argument for a function call.
----------------------------------------------------------------------------
                 RESULTS FOR JOB: %.80s
JOB TYPE:   %.80s
OWNER:      %.80s
SCHEDULED:  %.80s
START TIME: %.80s
RESULTS DETAIL LEVEL: %.80s
JOB INFORMATION:
   %s (+ subdirs)
   %s
%-60s %9lu bytes
RESULTS:
Volume %.80s
Volume %.80s (from media ID %08lX)

Job Completed: %.80s
Job Totals:    %lu files, %lu bytes
Job Totals:    %lu bytes
VOLUME SCAN INFORMATION FOR %.80s
   Target File Inactivity Period: %4d days
   File Inactivity Used:          %4d days
   Minimum Eligible File Size: %7lu bytes
   Volume Utilization (before sweep):     %2d%%
   Target Volume Utilization (OPT LEVEL): %2d%%
Volume Utilization (after sweep): %d%%
   Device %.80s, slot %d
   Media ID %08lX
   WARNING: No files available for critical migration
   WARNING: Could not reach target volume utilization (optimal level)
JOB CANCELED
Error trying to cancel HSM job (JCB) %d.
Log Reset
Could not allocate required memory for checking file(s) %.80s.
Invalid checksum for record %ld in file %.80s.
Error encountered while reading record %ld in file %.80s.
Error encountered while reading data block in file %.80s beginning at byte %ld.
Error encountered while seeking to byte offset %ld in file %.80s.
Primary and mirror files for %.80s are different sizes.
Primary file for %.80s has been updated more recently than mirror file.
Mirror file for %.80s has been updated more recently than primary file.
Sequence numbers in primary and mirror files for %.80s are inconsistent in record %ld.
Could not open temporary file %.80s in order to fix file %.80s.
Could not open file %.80s (attempting to copy to file %.80s).
Error encountered while reading data from %.80s (attempting to copy to file %.80s).
Error encountered while writing data to file %.80s (attempting to copy from file %.80s).
Error encountered while removing file %.80s.
Error encountered while renaming file %.80s to %.80s.
Error encountered while opening file %.80s.
File %.80s does not exist.
File %.80s does not end on a record boundary.
System error occurred while checking primary/mirror file(s) for %.80s.
Error detected in primary file for %.80s, mirror file was successfully copied to primary file.
Error detected in mirror file for %.80s, primary file was successfully copied to mirror file.
Volume %.80s (from library %.80s, slot %d)
Volume %.80s (from %.80s)
Failed to add volume "%.48s\%.16s:" to the system configuration database.
Could not create the statistics record for "%.48s\%.16s:".
Failed to mark the volume "%.48s\%.16s:" as configured.
Failed to create system subdirectory structure on configured volume "%.48s\\%.16s:".
Could not delete storage catalog files for volume "%.48s/%.16s:".
Failed to remove the volume "%.48s\%.16s:" from the system configuration database.
The volume "%.48s\%.16s:" was removed from the system configuration but attempts to remove the marker file failed.
The Bag List for Backup Access Group %04X was not erased.
   WARNING: No files found to migrate for sweep job
RESTARTING JOB
SYSTEM SHUTDOWN DETECTED
Error occurred setting system delay restart while processing shutdown job '%.80s' (JCB %d).
Error occurred setting system status while processing job '%.80s' (JCB %d).
Error occurred setting system restart time
Error occurred attempting to shut down system
BAG: %04X
Maximum number of supported HSM work tasks (%d) reached.
Error occurred scanning job information list (JDBs).
No files found
The system configuration cannot be initialized because the file %.80s cannot be found.
The system configuration cannot be initialized because the file %.80s cannot be read.
The system configuration cannot be initialized because the file %.80s cannot be opened.
The system configuration cannot be initialized because of a failure to obtain data within the file %.80s.
The system configuration cannot be initialized because there is not enough memory to process the file %.80s.
The system configuration cannot be initialized because an unexpected set of conditions was encountered while processing file %.80s.
The configuration service could not be initialized.  Check previous notices and the error log for causes.
The HSM Secondary Storage is full.
Job Failed: %.80s
Temporarily unable to migrate more files into HSM Secondary Storage.
Job Canceled: %.80s

The minimum number of optical library devices have not been configured.  The minimum number is %d.  The system will not start until the minimum configuration requirements are met.  See the Installation Guide for more information.
WARNING: No HSM data is stored on cartridge in library %.80s, slot %d, no action taken for restore media job
WARNING: No HSM data is stored on migration/shadow volume %.80s, no action taken for restore media job
WARNING: No HSM data is stored on media ID %08lx, no action taken for restore media job
Error occurred changing status of migration/shadow volume %.80s during restore media job.  Status should be manually changed using avmedman.
Error occurred changing status of media in library %.80s, slot %d.  Status should be changed manually using avmedman.
Error occurred changing status of media ID %08lx.  Status should be changed manually using avmedman.
Too many media IDs were specified for restore media job '%.80s' (media ID %08lx).
Error occurred rescheduling job '%.80s' (JCB %d).
A fault occurred in a system database.
SENSE: Key:%02x Asc:%02x Ascq:%02x VFC:%x
The drive can not determine the media type.
The drive detected media of wrong type (i.e. HSM found BACKUP media)
The target server requires encrypted passwords.
Setup the target server to allow unencrypted passwords.


The target server is not responding or does not have any available connection slots.
Bring the server up or free some connection slots and retry the operation.
The target server will not allow this user to login at this time.
This user should not have time restrictions for logging in.
The target server would not accept the HSM users password.
Update the users password.
The target server does not exist or has rejected the user name.
Make sure the target server is running and has this user configured.
The target server could not be found.
Make sure the target server is running.
The target servers bindery was locked.

Retry the operation.
The error code returned for this operation is unknown.
Call Technical Support.
The target server will not allow this user to login from this workstation.
Change the workstation restrictions for this user.
Error (%u) attempting to access volume %.80s.
The volume does not exist or is not mounted.
Make sure the volume is mounted and retry the operation.
The connection to the target server has failed.
Make sure the target server is running and check the physical connection.
The specified file or path could not be found.
Make sure that the file exists and the HSM user has rights to access it.
The specified path could not be found.
Make sure the path exists and the HSM user has rights to access it.
HSM user does not have supervisor rights to %.80s.
The HSM user must have supervisor equivalent rights to all managed servers.
Run SYSCON and change the HSM users security equivalence on the target server.
SENSE: Key:%02x Asc:%02x Ascq:%02x
SENSE: Key:%02x Asc:%02x Ascq:%02x HP:%04x DSP:%04x
Warning: %s cannot be restored at this time, backup tape is bad or missing
Error occurred getting backup tape ID for file %.128s while processing job %.40s (JCB %d).
Error occurred getting backup tape IDs for files in this job
The user %.48s does not have supervisor rights on the server %.48s.
Bad checksum on label of media in drive of %s.
Bad vendor id on label of media in drive of %s.
Bad label on media in drive of %s.
The media in the drive in %s could not be identified due to an internal database error.
The media in the drive in %s could not be identified due to a device error.
The program controlling %s has terminated because unknown media is in the drive. Please remove it.
The media in the drive in %s is unlabeled, and cannot be identified as HSM media.  Please remove this media from the drive.
Wrong HSM media found in the drive in %s. Expected serial number %ld but found %ld.
Could not verify the HSM media in the drive in %s due to an internal database error.
HSM media was found in the backup drive. Please remove it.
An external backup tape was found in the backup drive. Please remove it.
Backup tape %s is in the backup drive and may not be labeled. Please remove it.
A tape is in the picker of library %s. Return the tape to its slot and restart the system.
A tape is stranded in the drive of library %s. Manually eject the tape and restart the system.
The magazine of library %s failed to load. Check the library and restart the system.
The program controlling %s has terminated because the system is out of memory.
The program controlling %s has terminated because the device could not be reserved.
The program controlling the library %s has terminated because the device was unable to initialize.
The program controlling %s has terminated because it was unable to communicate with the device.
The program controlling %s has terminated because it failed to initialize the device.
Ran out of space during a Recall/Restore of file %s. 
  Migrated:    %lu files, %lu bytes
  Premigrated: %lu files, %lu bytes
%-60s %9lu bytes
RESULTS: (files followed by (+) have been premigrated)
Error occurred sending DCB %d (type %d) to Hierarchy Manager (code %d).
The minimum number of library devices have not been configured for the system.  The minimum number is %d.  The system will not start until the minimum requirements are met.  See the Installation Guide for more information.
Restore media failed, ran out of space on the destination media. Use larger media.
The device was unable to verify the data just written.
The requested service - %s/%s - could not be located.
The specified HSM server does not have that service installed.
This is a non-fatal error - system operation should continue normally.

The HSM user is not a console operator on the target server.
Use Syscon to make the HSM user a console operator on all managed servers.
Error (%u) encountered writing placeholder EA data for %.80s.
The maximum percentage of disk space allowed for EA data has been allocated.
Use the SET command at the target server to increase the percentage of space allowed for extended attributes. 
The target file has the maximum allowed number of extended attributes.
Use the SET command at the target server to increase the number of extended attributes per file.
Error starting %.80s service.
The mailbox could not be found.
The HSM name could not be identified.
Failed to communicate with %.80s service.
The service could not be located.
No action is required.
The file is marked execute only.
The path given is a directory name.
The file was modified since it was moved into the HSM system.
Cannot make %.80s a placeholder.
The job status information file (JCB) contains invalid data in record number %d.
The job description information file (JDB) contains invalid data in record number %d.

The DOS driver failed to connect to a server.
An error was encountered during a read, write or seek on the shadow device.
An error was encountered during and attempt to open the shadow device. Check 'MEDIA.OBJ' on the volume.

Could not get minimum size of file for migration for server/volume %.80s while processing job '%.80s' (JCB %d).
Placeholder created for premigrated file %s 
Unable to access the data on the media in device %.80s slot %d.
Unable to access shadow volume %.80s.
Unable to access volume %.80s.
Use AVRECMAN to manually discard files from the HSM.
Error occurred attempting to automatically discard files from the HSM.
HSM automatically discarded files from the lowest storage layer.

An attempt to write to media failed.
Failed to read from DOS file <%s>: errno - %d
Failed to write to DOS file <%s>: errno - %d
Failed to position correctly in DOS file <%s>: errno - %d
Failed to open DOS file <%s>: errno - %d
Failed to read from shadow drive: errno - %d
Failed to write to shadow drive: errno - %d
Failed to position in shadow drive: errno - %d
A failure occurred during an attempt to read from the media.
An error has occurred on the source device.
An error has occurred on the destination device.
The media in the source device is bad.
The media in the destination device is bad.
Could not get file rules information for server/volume %.80s while processing job %.80s (JCB %d).
Warning: %s matched file rules
Check the error log for more specific failure information.
Set the system status to offline, then online, to restart space level monitor activity on the volume.
Critical migrate jobs are failing on volume %.80s.
Encountered an error while accessing the data on volume %.80s. Review the error log for the specific error.
Encountered an error while accessing the data on the media mounted on device %.80s. Review the error log.
Warning: %s is a compressed or sparse file and cannot be migrated
Encountered an error on the backup device.  See error log for specific error.
Encountered an error while writing to volume %.80s. Review the error log.
Encountered an error accessing the media on device %.80s. Review the error log.
A valid backup media was detected when a blank or HSM media was expected.
Warning: %s is overflowed, retrieve file using restore-file job
The job was canceled because the file server was in use by the backup system.
%.8s of %.48s by %.48s
The device <%s> on adapter <%d> at SCSI address <%d> is not responding because its driver <%s> is not running.
The device <%s> on adapter <%d> at SCSI address <%d> is not responding to software requests.
The mount was canceled.
Error occurred retrieving catalog information for file.
Unable to Recall/Restore '%s'. The placeholder has changed since the file was migrated.
The media in drive %s is not able to be identified due to a media error.
Make sure that the SYS: volume is mounted and a backup is not active.
Volume Utilization (after critical migrate): %d%%
%s could not be written because (errno %d) the user is out of space or is no longer administered.
The HSM Secondary Storage remains full because one or more media is in a BAD state. Use AVMEDMAN to correct any BAD media.
DISCARDING BAG: %04X


The HSM Secondary Storage does not have enough space for restoring the overflowed data.
<Y> Yes  
<N> No  
<Esc> Cancel
HSM %s requires administrator attention.
  
-------
Migrate
Recall
Sweep
Demand Recall
Crit Migrate
Relocate
Partial Backup
Backup
File Restore
Media Restore
Replace Media
Remove Media
Add Cartridge
Discard Files
Retire Files
Change Status
View Info
Premig Sweep
Sched Shutdown
System Startup
System Shutdown
Auto Discard
Network Backup
Restore Bag
Unknown Log Entry
-------
Start
Restart
Complete
MISSED
FAILED
INCOMPLETE
CANCEL
Unknown status
%02d/%02d/%02d %02d:%02d:%02d
%-17.17s  %-10.10s  %-15.15s  %.180s
Add Server
Add Volume
Delete Server
Delete Volume
Add HSM Volume 
Add HSM Opt Lib
Add HSM Tape Lib
Add HSM Backup 
Delete HSM Vol
Del HSM Opt Lib
Del HSM Tape Lib
Del HSM Backup
Add HSM MRU Dev
Del HSM MRU Dev
%s
System shutdown could not be completed because HSM utilities were running.
The connection to the domain server (%s) has been lost.
Restore the domain server and HSM will automatically restart.
The user GUEST may not have a password for HSM to send notification messages to users on this server.
Notify service has deleted all old notices. 
The database was from a previous version of HSM software.

%.80s could not be contacted.
The machine could not be located.
Make sure the HSM software is running and the server name is specified correctly.
Failed to append data because new data is not member of the data set on mounted media.
The HSM backup rotation configuration is invalid.  Please use AVBAKMAN to view and correct this problem.
HSM overflowed files from the lowest storage layer.
Error occurred attempting to overflow files from HSM.
Files must be backed up on all backup sets.
Id: %d BAG: %04X
Id: %d Hard Disk
Id: %d Optical
Id: %d Discard Oldest Files
Id: %d Overflow Oldest Files
Id: %d Stop Migration
Oldest media is currently being used in the system.
Id: %d
MRU
Backup Rotation
Media Replaceable Unit (MRU) Creation Needed
Creating a MRU requires manually changing backup media. Are you ready to create the MRU now?
Backup Set Rotation Needed
Changing the Backup Set requires manually changing the backup media. Are you ready to change the Backup Set now?
HSM %.80s already uses some or all of the keys in use here.
You may not use keys on more than one system.
Purchase and install unique keys on each system.
User: %.48s on connection %u%.128s
WARNING:  A request to delete managed volume %s from the HSM configuration has been processed.  The volume had migrated data that is no longer accessible.
The job was canceled because the product evaluation time period has expired.
Load backup cartridge. Choose one: %s
Failed to get element status for slot %u in library %s.
Failed to set the media state for slot %u in library %s.

HSM encountered errors accessing the media database.
MRU creation failed, ran out of space on the destination media. Use larger media.
Please close the door on library %s to proceed.
Failed to execute driver %.80s.
The file was not found or failed to load.
Check that the file exists and is in the hsm\exe directory.
Unable to Demand Recall '%.128s'. The placeholder has changed since the file was migrated.
The file or directory could not be located.
The argument list was too large.
The executable format was incorrect.
The file handle was not valid.
There was not enough memory available to complete the action.
Access to the file was denied.
The action could not be completed because the file exists.
The action would cause a cross-device link.
Invalid arguments were passed.
The applications internal file table is full.
The system file table is full.
The volume is out of space or the file owner has space restrictions.
The argument was too large.
The result of the operation was too large.
The operation failed because it would have caused a deadlock.
The file or record was in use by another process.
A file server internal error occurred.
The file server could not be located.
Verify that the file or directory exists and is accessible.

Check the integrity of the executable files and re-install any bad ones.
Unload any unnecessary applications or increase the available memory.
Make sure that the HSM user has supervisor access to all servers.


Make sure the volume has available space and that the file owner has not exceeded any space restrictions.
Retry the operation.  If the error is persistent please call Technical Support.
Check the target servers system error log.  There may be hardware problems.
Verify that the target server is running and is accessible.
The connection to the target server was lost.
Check the target server and the network connections.
Unable to locate oldest media for the OPTICAL layer. Verify at least two pieces of media are configured for the OPTICAL layer. Check cartridges with AVMEDMAN.
Unable to locate oldest media for the TAPE layer. Verify at least two pieces of media are configured for the TAPE layer. Check cartridges with AVMEDMAN.
Unable to locate oldest media for the MIGRATION VOLUME layer.
Internal transfer buffer corruption detected.
Update Install
Version %d.%2d.%c
See Install Log
Media in drive %s is not formatted for 1024 bytes per sector.
The HSM is disabled because there is no space on the %.80s volume.
The HSM cannot add to or update its database files.
Create some space on the volume.  Then shutdown and restart the HSM.
Record Manager cannot write data to an HSM system file because there is no space on the volume.
SKIPPED BAG: %04X
An error occurred trying to Restore BAG %04X to HSM Secondary Storage. If the BAG is backed up on multiple sets, try a different backup media.
HSM could not restore %d BAGs to Secondary Storage. Check the Error Log for additional information.
The file was open by another client when HSM attempted to access it.
You may retry the operation or ignore the error.
Files on volume %.80s cannot be migrated.  The AVSTOR.$$$ file on the volume contains the name %.80s which does not match the name of this HSM (%.80s).
If the HSM server has been renamed, use AVSETUP.NLM to correct the HSM name for the volume.  Otherwise, call Technical Support.
The AVSTOR.$$$ file on the volume is missing.
Restore the AVSTOR.$$$ file from primary network backup.
Files on volume %.80s cannot be migrated at this time.  An error occurred accessing the AVSTOR.$$$ file on the volume.
Check user permissions on the AVSTOR.$$$ file and/or check for network connection errors.
Job %.40s could not migrate files for volume %.80s.  Check previous errors in the error log for more information.
WARNING: Files cannot be migrated from volume %.80s.  See the error log for more information.
Critical migrate job could not migrate files for volume %.80s.  Check previous errors in the error log for more information.
An error occurred while scanning managed volumes for server %.80s to verify HSM information (error code: %d).
An error occurred while scanning managed servers to verify HSM information (error code: %d).
Could not get volume configuration information for %.80s/%.80s (error code: %d).
Network services internal connection limit has been exceeded. 
No more SPX connections are available. 
See your network documentation to configure the system parameters. 
The server is not responding to a connection request.
An unexpected error was encountered.
The catalog entry for file %.80s (%04x:%08lx) could not be found while processing job %.80s (JCB %d). Node information for this file is either missing or invalid.
Warning: Catalog entry for %s could not be found or is invalid, retrieve file using primary network backup
The catalog file %s cannot be opened.
Another process is currently accessing the catalog, or has accessed the catalog and left it locked from use by other processes.
Use the Novell MONITOR program to determine which user process has the catalog open.  Wait for that process to complete its access, or terminate it.  If the catalog is not currently open, down the server and restart it.
A label could not be written to the media.
The application has requested more IPX sockets than are available on the workstation.
The HSM ID was not set in the system information table.
Premigration Sweeps: OFF
Critical migrate jobs: OFF
Failed (%u) to determine if block-suballocation is enabled for %s.
HSM operation will continue.
This is a non-fatal error.
The media has a bad format or no format.
Require file backup: OFF
System Offline
System Online

Files on volume %.80s cannot be migrated.
The AVSTOR.SCF file on the volume is missing.  Note:  this is normally a hidden file.
Restore the AVSTOR.SCF file to the volume from primary storage backup, then execute the Rebuild Storage Catalog function in the Database Recovery Manager program.
Cannot recall file %.80s because it was migrated to a different HSM server.
Cannot recall file %.80s because it is overflowed to backup media that is not currently mounted.
NETWORK BACKUP DETECTED
HSM Backup Disabled
The program controlling the library %s has terminated because the device is requesting manual intervention. 
Please register your system and then increase the HSM Secondary Storage capacity.

