pcANYWHERE32 for Windows 95 and Windows NT		version 7.50
Copyright 1996 Symantec Corp.  All Rights Reserved.          5/22/96

Release Notes:

Install / Uninstall

*	Because Windows NT allows varying access to protected files 
	and services, installing/uninstalling pcANYWHERE32 should be 
	performed by a user with administrator privileges.

*	Users of Microsoft Windows NT3.51 with Service Pack #4 - to 
	properly install pcANYWHERE32, use the following steps:

	1. In the SYSTEM32 sub-folder of your Windows NT folder, 
	   rename SMSS.EXE to SMSS.OLD.
	2. Copy SMSS.EXE located on "pcANYWHERE32 Disk 1" to the 
	   SYSTEM32 sub-folder.
	3. Restart Windows NT.
	4. Run pcANYWHERE32 setup program.

	For more information, please contact Microsoft Windows NT 
	product support or look for article #Q148485 at:
	http://www.Microsoft.com/kb

Network Installations

*	Administrators installing pcANYWHERE32 NT workstations onto a
	network drive need to alter the "Add Be A Host" template 
	before workstation users begin to create host session 
	items.  The default template setting "Run as a Service" 
	should be unchecked if host items files are stored on the 
	network.  Host files will not launch if "Run as a Service"
	is checked.

*	In order to access Administrator options, a workstation install
	must be performed on the Administrator's machine.  If the /A 
	option is invoked without first installing a workstation, you 
	will not be prompted for an Administrator password.

*	If host or caller files are located on a network drive, you 
	will not have access to the "Launch host at startup" feature.

TCP/IP

*	The following registry items effect the ability to browse 
	networks for pcANYWHERE32 TCP/IP hosts:

	TCPIPBrowseDelay -
	Allows the user to set the delay used when creating the 
	remote's browse list.  For a RAS connection, start with a 
	setting of 11.  If the complete host list is not received over 
	a WAN connection, start this value at 1 and increase until the 
	entire host list is displayed.

	DisplayInHostList - 
	This item can be altered for pcANYWHERE32 hosts that do not 
	wish to appear in a remote's browse list, when the remote is 
	scanning the network.  The default for this setting is 1.  
	To keep the host from being displayed on a browse list, assign 
	the registry key a value of zero.  Currently, this item only 
	applies to TCP/IP hosts.

	These items may be added to the registry by:

	1.  Running the edit registry utility (REGEDIT.EXE)
	2.  Editing the key:

 HKEY_LOCAL_MACHINE\SOFTWARE\Symantec\pcANYWHERE\CurrentVersion\System

	3.  Creating a new DWORD value with the browse option name
	4.  Assigning the appropriate value

Multiple Remotes

*	The Multiple Remote Sessions feature is not supported using an 
	IPX connection type under Microsoft Windows 95.

Simultaneous Remote Control/File Transfer

*	Simultaneous file transfer and remote control is only supported
	when connecting to hosts pcANYWHERE 7.5 or later.

AutoXfer(tm)

*	An AutoXfer can be scheduled to run whenever is convenient for 
	you.  Follow these easy steps to create an unattended file 
	transfer:

	1. Using pcANYWHERE file manager, add files you wish to copy to
	   an AutoXfer procedure.

	2. Assign this procedure to a remote control object

	3. Make sure the automated procedure is set to "end session 
	   when finished"

	4. Launch a scheduling program, such as Norton Program 
	   Scheduler or Microsoft System Agent

	5. Assign the remote control session object (ex. DIRECT.CHF) to
	   run whenever you like

*	When connecting to a pcANYWHERE32 host under NT, the host user 
	must already be logged-in before a successful AutoXfer can take
	place.

OLE

*	pcANYWHERE Host objects do not support OLE when they are "Run 
	as a service."  Uncheck this feature when launching host 
	objects embedded within other applications or run from the file
	manager.

*	The OLE service must be installed and activated under Windows 
	NT 3.51 before installing pcANYWHERE32.

CAPI

*	AVM/A1 cards running the North American CAPI drivers
	(Windows 3.x) do not support channel bonding.  Checking 
	"Attempt Channel Bonding" in pcANYWHERE32 may produce 
	unpredictable results.  Future AVM drivers may correct this 
	problem.

Host Operation

*	Under Security Options, the feature "Prompt to confirm 
	connection" will only function for those callers that are not
	SuperUsers (i.e. have individual callers privileges defined).

NT Host Service

*	For optimal performance under Windows NT 3.51, it is 
	recommended that pcANYWHERE32 NT Hosts are configured to 
	"Run as a Service".

*	SPX host objects are currently not supported with the Novell 
	NetWare Client for Windows NT installed.  This also applies to 
	pcANYWHERE32 gateways where SPX is the inbound device type.

Remote Control

*	Users experiencing slow performance connecting to a pcANYWHERE 
	7.5 host with a previous version of pcANYWHERE (5.x or 2.x) 
	should disable the remote's cache file.  This will improve the 
	remote's performance.

NT Remote Control

*	Those who see a performance decrease when opening a DOS window 
	on a pcANYWHERE32 NT Host can improve the speed by altering NT 
	tasking, located under System in the Control Panel.  The 
	default setting should be changed from "Best Foreground 
	Application Response Time", to "Foreground and Background tasks
	equally responsive".

*	For users experiencing problems remotely sending certain
	keystrokes to a pcANYWHERE32 NT Host, try pressing the NumLock,
	Shift, ALT or CTRL keys.

*	To enable remote file transfer support with NetWare volumes, 
	your Novell NetWare password should be the same as your 
	Windows NT password.

pcANYWHERE Access Server

*	When making pcANYWHERE32 connections to a pcANYWHERE Access 
	Server Host to perform file transfer, click "Remote Control" 
	and start the file transfer after the connection has been made.	
 
Logging onto NT with pcANYWHERE 2.0x and Lower

*	Owners of previous versions of pcANYWHERE may now take 
	advantage of the pcANYWHERE32 feature "Send CTRL-ALT-DEL".  
	Pressing CTRL-ALT-D while connected to a pcANYWHERE32 host 
	will emulate this feature.

Data Conversion

*	When converting pcANYWHERE configuration files under Windows 
	NT, please note that all newly created session items with IPX
	as the connection type will be changed to SPX. 

*	If enabled, the master password from a previous installation
	of pcANYWHERE 2.0x should be disabled before converting files.

*	Data files configured as "Shared" under a previous 
	Administrator installation of pcANYWHERE cannot be converted 
	to pcANYWHERE32.

Script Language

*	The script command LOAD CONFIG is no longer supported.  Use the
	commands LOAD ONLSVCINFO or LOAD HOSTINFO instead.

*	Scripts may be executed from the command line by typing the 
	following line:

	AWREM32.EXE <scriptname>

	Make sure both the path and .SCR extension are given.

International

*	When specifying TCP/IP host names to connect to, lowercase 
	extended ASCII characters (e.g. "ö") cannot be used, or the 
	name will not appear on a list of available hosts.

Modems

*	If you experience connection problems using modems under WIN95,
	try lowering the default FIFO buffer settings, or changing the 
	default data rate.  These options are found in the modem's 
	connection property page, under the headings "port settings" 
	and "maximum speed".

8250 and 16550A UARTS
*	It is recommend that users of slower PCs, who typically have a 
	8250 UART chip on their serial card, upgrade their card to one 
	containing the 16550A UART chip.  This will prevent 
	communication errors at higher data rates.

Remote Networking

*	After successfully configuring a Remote Networking item, a 
	pcANYWHERE32 remote control item named "RAS" is created in the 
	remote control window.  This item is not to be used for
	your dial-up networking connections.  Click Remote Networking
 	and choose the appropriate item.

3D Accelerated Video Cards

*	If you experience problems with a 3D accelerator card, such 
	as the Matrox Millenium, you may need to disable some of the 
	cards advanced accelerator features.  (For the Matrox 
	Millenium, you must disable the PowerGDI Acceleration option.)

Security

*	Do not restrict access to the pcANYWHERE installation directory
	by setting callers' security privileges to "No Access". Callers
	must be given read-access to these files.

*	Drive Security is not supported by pcANYWHERE32 under Windows 
	NT.  If you need security, use an NTFS partition and allocate 
	rights to users with the Administrative Tools included in NT.

WinFax and pcANYWHERE32 Hosts

*	In order for WinFax to give control of an incoming telephone 
	call to a waiting pcANYWHERE32 host, the WinFax feature 
	"call discrimination" must be enabled.  For more information,
	consult your WinFax User Manual

*	If using Delrina's Wincomm Suite follow procedure below:

	How to use Winfax 7.0 to call discriminate between fax and 
        data calls.
     
     	SETUP: When using Delrina's Wincomm Suite:
        	1.  In Winfax, click on "Setup" drop down menu and 
                    then click on "Receive".
                2.  Enable "Call discrimination" 
                3.  Enable "Automatically answer incomming calls" 
                4.  Click on OK.
     
        	If using Delrina's Winfax 7.0 standalone:
                1.  Run regedit
                2.  Edit the key 
     
     HKEY_CURRENT_USER\Software\Delrina\Commsuite\7.0\Modems\Modem#
		
		3.  Set "DataCapable" to 1.
                4.  Set "CallDiscriminationSupport" to one of the 
                    values below:

                    Value     Description
                      1         FAE...ATO  (recommended value) 
                      2         FAA...ATO
                      3         FAE
                      4         FAA
                      values that are not supported in the October 
                      31,1995 release but are in later releases are:
                       9         FCLASS=1 FAE...ATO
                       10        FCLASS=2 FAA...ATO
                       11        FCLASS=1 FAE
                       12        FCLASS=2 FAA

                5.  Close regedit
                6.  In Winfax, click on "Setup" drop down menu and 
			then click on "Receive".
                7.  Enable "Automatically answer incomming calls" 
                8.  Click on OK.
     
                Check the TELEPHON.INI that is in the WINDOWS directory
                Make sure that the handsoff section is as follows:
                    [HandoffPriorities]
                    RequestMakeCall=DIALER.EXE
                    datamodem=wfxmod32.exe,
                    unknown=
                    g3fax=wfxmod32.exe,
     
 	Run Winfax or the Commbar utiltiy.  Run pcANYWHERE32 host.  
	Winfax Win fax 7.0 answers the call.  If it is a fax call, 
	Winfax 7.0 will handle it.  If it is a data call, Winfax 
	7.0 will hand the call off to pcANYWHERE32.





                                                                                                                                                 
                                                                                                                                                 
                                                                                                                                                 
                                                                                                                                                 
                                                                                                                                                 
                                                                                                                                                 
                                                                                                                                                 
                                                                                                                                                 
                                                                                                                                                 
