/* Install *A*ll files or only the *P*rogram executables and support files */
@DefineDisk
   @Label = "DISK 8 OF 12"

   @If (( 'B' [= @Group) || ('K' [= @Group ))
      @F README @O @Outdrive:@Subdir@Subdir3\README
      @F WHATS.NEW @O @Outdrive:@Subdir@Subdir3\WHATS.NEW
      @F RNDRSTAR.TXT @O @Outdrive:@Subdir@Subdir3\RNDRSTAR.TXT

      @BeginLib PROGRAMS.RED
	 @F 1024-1.FNT @O @Outdrive:@Subdir@Subdir3\BIN\1024-1.FNT
	 @F 1024-2.FNT @O @Outdrive:@Subdir@Subdir3\BIN\1024-2.FNT
	 @F 1024-3.FNT @O @Outdrive:@Subdir@Subdir3\BIN\1024-3.FNT
	 @F 1024-4.FNT @O @Outdrive:@Subdir@Subdir3\BIN\1024-4.FNT
	 @F 640.FNT @O @Outdrive:@Subdir@Subdir3\BIN\640.FNT
	 @F 800.FNT @O @Outdrive:@Subdir@Subdir3\BIN\800.FNT
	 @F AALIAS.EXE @O @Outdrive:@Subdir@Subdir3\BIN\AALIAS.EXE
	 @F DEFAULT.CFG @O @Outdrive:@Subdir@Subdir3\BIN\DEFAULT.CFG
	 @F DEFAULT.RSC @O @Outdrive:@Subdir@Subdir3\BIN\DEFAULT.RSC
	 @F FLI2VGA.EXE @O @Outdrive:@Subdir@Subdir3\BIN\FLI2VGA.EXE
	 @F ORIGINAL.COL @O @Outdrive:@Subdir@Subdir3\BIN\ORIGINAL.COL
	 @F PATCH_RS.EXE @O @Outdrive:@Subdir@Subdir3\BIN\PATCH_RS.EXE
	 @F PLAYFLC.EXE @O @Outdrive:@Subdir@Subdir3\BIN\PLAYFLC.EXE
	 @F RENDER2.EXE @O @Outdrive:@Subdir@Subdir3\BIN\RENDER2.EXE
	 @F RS2.COM @O @Outdrive:@Subdir@Subdir3\BIN\RS2.COM
	 @F RS2.COM @O @Outdrive:@Subdir\RS2.COM
	 @F RS2EPS.EXE @O @Outdrive:@Subdir@Subdir3\BIN\RS2EPS.EXE
	 @F RS2PCX.EXE @O @Outdrive:@Subdir@Subdir3\BIN\RS2PCX.EXE
	 @F RS2SVGA.EXE @O @Outdrive:@Subdir@Subdir3\BIN\RS2SVGA.EXE
	 @F RS2TGA.EXE @O @Outdrive:@Subdir@Subdir3\BIN\RS2TGA.EXE
	 @F RSEDIT.EXE @O @Outdrive:@Subdir@Subdir3\BIN\RSEDIT.EXE
	 @F RSHELL.COL @O @Outdrive:@Subdir@Subdir3\BIN\RSHELL.COL
	 @F RSHELL.EXE @O @Outdrive:@Subdir@Subdir3\BIN\RSHELL.EXE
         @F 16X16.CMF @O @Outdrive:@Subdir@Subdir3\DEFAULT\16X16.CMF
         @F 16X16.PAL @O @Outdrive:@Subdir@Subdir3\DEFAULT\16X16.PAL
         @F 32X8.PAL @O @Outdrive:@Subdir@Subdir3\DEFAULT\32X8.PAL
         @F 4X64.CMF @O @Outdrive:@Subdir@Subdir3\DEFAULT\4X64.CMF
         @F 4X64.PAL @O @Outdrive:@Subdir@Subdir3\DEFAULT\4X64.PAL
         @F 8X32.CMF @O @Outdrive:@Subdir@Subdir3\DEFAULT\8X32.CMF
         @F 8X32.PAL @O @Outdrive:@Subdir@Subdir3\DEFAULT\8X32.PAL
         @F NEWTEXT.MAT @O @Outdrive:@Subdir@Subdir3\DEFAULT\NEWTEXT.MAT
         @F OLDRS1.MAT @O @Outdrive:@Subdir@Subdir3\DEFAULT\OLDRS1.MAT
         @F RS2-X24.MAT @O @Outdrive:@Subdir@Subdir3\DEFAULT\RS2-X24.MAT
         @F STANDARD.CMF @O @Outdrive:@Subdir@Subdir3\DEFAULT\STANDARD.CMF
         @F STANDARD.MAT @O @Outdrive:@Subdir@Subdir3\DEFAULT\STANDARD.MAT
         @F STANDARD.MLF @O @Outdrive:@Subdir@Subdir3\DEFAULT\STANDARD.MLF
         @F STANDARD.PAL @O @Outdrive:@Subdir@Subdir3\DEFAULT\STANDARD.PAL
         @F RS2SVGA.DOC @O @Outdrive:@Subdir@Subdir3\DOC\RS2SVGA.DOC
         @F DCAD8.PAL @O @Outdrive:@Subdir@Subdir3\DEFAULT\DCAD8.PAL
         @F DCAD16.PAL @O @Outdrive:@Subdir@Subdir3\DEFAULT\DCAD16.PAL
      @EndLib
   @EndIf

@EndDisk

@If (( 'B' [= @Group ) ||
     ( 'S' [= @Group ) ||
     ( 'T' [= @Group ))

   @Chain ("DISK 9 OF 12")

@EndIf

@Finish

   @Cls

	@If ('B' [= @Group || 'K' [= @Group)
		@InsertPatchRc("PATCH","PATCH")   
		@SetCfgFont("PATCH")               
		@PatchRsCom("@Outdrive:@Subdir","@Outdrive:@Subdir@Subdir3\\bin","")
	@ElseIf ('R' [= @Group)                    
		@InsertPatchRc("PATCH","PATCH")
		@SetCfgFont("PATCH")
	@ElseIf ('I' [=@Group || 'J' [=@Group )
		@InsertPatchRc("PATCH","PATCH")
	@EndIf

        @Cls
	@ChDrive@OutDrive
        @ChDir "@Subdir"

        @If (('A'[=@Group) || ('D'[= @Group ))
           @Mkdir ("@OutDrive:\\@Subdir\\LYR")
           @Mkdir ("@OutDrive:\\@Subdir\\PLT")
           @Mkdir ("@OutDrive:\\@Subdir\\SYM")
           @Mkdir ("@OutDrive:\\@Subdir\\TPL")
        @EndIf


   @If (1004 [= @Option)
        The DataCAD Configuration Utility will now be run.  This is
        where you should select your display device, digitizer (if any),
        plotter, etc.

	@pause

      @If (@Spawn ("CONFIG"))
      @EndIf

   @EndIf
   @Cls

        The installation has been successfully completed.
        To run DataCAD, type RUNDCAD at the DOS prompt and
        press <Enter>.

	Note:  Please be sure you have installed your mouse
	       manufacturer's supplied driver according to
	       their instructions prior to running DataCAD.

	Thank-you for choosing DataCAD!

	@pause
@EndFinish
