Foray PPP Client Installation Instructions


You should start with Windows for Work Groups with Networking DISABLED.
If your workstation produces "insufficient" memory messages, see the bottom of
this file for instructions on how to load files high.


1.0  INSTALL LAN WORKPLACE

     For more complete instructions on the LAN WorkPlace installation program,
     refer to the LAN WorkPlace manual. The steps and order of steps may vary
     with the version of LAN WorkPlace you use.

     1.1  From the DOS prompt, start the LAN WorkPlace installation program.

          1.1.1  Insert Disk 1 in your floppy drive.

          1.1.2  Change your drive to "a" by typing "a:" and pressing "enter".

          1.1.3  Type "install" at the "a:\>" prompt to initiate the program.

     1.2  The LAN WorkPlace installation program will present a screen which asks
          you to have information about your network configuration ready.

          1.2.1  You will need to know, among other things, what kind of IP
                 addressing your network adminstrator has employed and the IP
                 address of your IP Router and Domain Name Server.  If you
                 have the appropriate information, press the "ESC" key to
                 continue.

          1.2.2  If you do not know how your network configured, you should
                 abort the install, review the LAN WorkPlace manual, and find
                 the appropriate information before continuing.  If you need
                 more information, follow the screen instructions to abort the
                 install.

    1.3   The LAN WorkPlace installation program will prompt you to choose
          what parts of the LAN WorkPlace stack to install.  Select support
          for ODI LAN Workstation Services, LAN WorkPlace TCP/IP Support and
          LAN WorkPlace DOS support and LAN WorkPlace for Windows Applications option.

    1.4   Press "ESC" to continue.

    1.5   Click on "Yes" to save changes.  

    1.6   The LAN WorkPlace installation program will prompt you to choose
          which drive to install LAN WorkPlace on.

    1.7   The LAN WorkPlace installation program will prompt you to specify
          a target directory. Unless you specify another directory, LAN
          WorkPlace will create the \net directory and install to "c:\net".
          Accept default or change target directory. Press "ESC" to continue.

    1.8   The LAN WorkPlace installation program will ask you whether your
          workstation boots from a file server. Unless your workstation
          does not have a hard drive, the answer will likely be "No".
          If you select "No", press enter (and continue). If you select "Yes",
          see your system administrator for details.

    1.9   The LAN WorkPlace installation program will ask you whether you
          want to update system files. Choose "Yes".

    1.10  Press the "ESC" key to continue. 

    1.11  When the LAN WorkPlace installation program prompts you to
          install a driver, choose the option, "None of these". (Foray PPP
          Client will install its own driver on your workstation.)

    1.12  The LAN WorkPlace installation program will ask whether you want
          to install the SLIP/PPP Driver on your workstation.  Choose "Yes".

    1.13  Press the "ESC" key to continue.

    1.14  The LAN WorkPlace installation program will ask your whether TCP/IP
          parameters are provided by a BootP Server. Choose "No."

    1.15  When you are prompted to enter the IP address for your workstation,
          enter 1.1.1.1.  Press "Enter".  The Foray PPP Client Setup program
          will allow you to change this parameter.

    1.16  When the LAN WorkPlace installation program asks you whether your
          subnets, enter "No".

    1.17  When the LAN WorkPlace installation program asks you whether your
          network uses an IP Router, enter "No".

    1.18  When the LAN WorkPlace installation program asks whether your
          network has a domain name server, answer "Yes" or "No".

    1.19  If the answer is "Yes", enter the Domain Name.

    1.20  Enter the Domain Name Server Address.

    1.21  The LAN WorkPlace installation program (version 4.1) will ask you
          to select the workstation you are using from a list. Choose the
          appropriate option.

    1.22  The LAN WorkPlace installation program (version 4.1) will ask you
          the name of the server you log into.  Enter the appropriate name.

    1.23  The LAN WorkPlace installation program will ask you to provide your
          username.  Enter the appropriate name.

    1.17  The LAN WorkPlace installation program will also ask to provide
          a user name to use with R-utilities.  Enter the appropriate name.

  
2.0 INSTALL NETWARE CLIENT

    2.1   Return to the DOS prompt.

    2.2   Insert Disk 1 in floppy drive.

    2.3   Type "A:", if you are using drive A, and enter. 
          You should have moved from the C: prompt to the A: prompt

    2.4   Type "Install" and press "Enter".

    2.5   Choose option "5".  Press "Enter".

    2.6   Choose "TechSmith Corporation Enterprise Wide PPP".

    2.7   Press "ESC" to save your selection.

    2.8   Select item "6" and press "Enter".

    2.9   Complete Setup.

    2.10  Reboot Machine.

    2.11  Start Windows.  

    2.12  Ignore networking errors and warnings.
 

3.0 INSTALL THE PPP CLIENT

    3.1   Start Windows.

    3.2   Insert disk in floppy drive.

    3.3   From program manager open "File" menu.

    3.4   Select "Run".

    3.5   Type "a:setup". Press "Enter".

    3.6   Complete Setup. (If you already have Enterprise Wide you will want to 
          install the PPP Client to a different directory.)

    3.7   Choose "Yes" to view the README.1ST file.


4.0 USE THE FORAY CONTROL PANEL TO FINALIZE NETWORK SETUP.

    The first time you run the Foray PPP Client, the setup program 
    will prompt you to configure the modem and driver.

    4.1  Click on the Enterprise Wide PPP Client Icon. 

    4.2  Click "OK" on the "Info" screen.

    4.3  Click "OK" on the "Control Panel Info" screen.

    4.4  Select a "modem".

    4.5  Select a "com port". (Remember, if you have a serial mouse, it should 
         be on com1 and the modem on com2!)

    4.6  Select the "baud rate". (If you don’t have a 16550 uart, choose 19,200.
         If you do not choose a baud rate the 19,200 default will be applied.)

    4.7  Click "Next".

    4.8  In the Driver Setup Screen select LAN Workplace and leave 
         "Address Assignment" at "Automatic".

    4.9  Click "Next".

    4.10 If you want to look at the changes made in your configuration 
         files do it now, and, when you are done, click "Next".

    4.11 Click OK on Foray PPP Client info screen.

    4.12 If you do not have a Windows Permanent Swap File you will see a 
         screen asking you to set one up.  Click "Yes".

    4.13 This screen tells you to reboot after you are done. Click "OK".

    4.14 In the Enhanced screen, click "Virtual Memory".

    4.15 In the Virtual Memory, click "Change".

    4.16 Insure that the setting is for permanent memory, and click "OK".

    4.17 Click "YES" to the "Are You Sure?" screen.

    4.18 Click "Continue" to go back to windows, then exit windows and reboot.
 

5.0 USE FORAY CONTROL PANEL FOR USER AND PHONEBOOK SETUP

    5.1  Choose Setup/User from the Foray Control Panel Menu.

    5.2  Enter User Information.

         5.2.1  Enter the User ID (identification) which your remote server 
                will recognize.
  
         5.2.2  Enter the password which your remote server will recognize.
  
         5.2.3  Click "Allow passwords to be saved in setup file" checkbox.

     5.3 Choose Phonebook Information from the Foray Control Panel menu.

     5.4 Enter the name of your PPP Server. 

     5.5 Enter Phone number information:

	 5.5.1 Click on the "Default PPP Server" checkbox.

	 5.5.2 Click on the check "Automatic Dial".

	 5.5.3 Click on the "Save" button.

     5.6 Choose Actions/Connect and /Dial from the Foray Control Panel menu.


6.0  REGISTER THE PRODUCT

-------------------------------

MEMORY OPTIMIZATION

Optimizing Your Workstation’s Memory for Foray PPP Client

If you are not running a memory manager and your workstation produces 
"insufficient memory" messages when you execute programs, you can 
edit your workstation’s configuration files to make your pc’s use 
of memory more efficient.

If  you do not have enough memory to run your DOS editor, you must 
unload some files from memory before you begin.  We suggest that 
unloading two files,  VLM.EXE  and IPXODI.COM,  from conventional 
memory will help solve this problem.  

To unload these files from conventional memory, type the name of 
each file, a space and a "u"  at the DOS prompt:

c:\>vlm.exe u

c:\>ipxodi.com u

-----------------

Editing Your CONFIG.SYS file

In your CONFIG.SYS file, you can add lines which will tell workstation 
to load certain application files "high" or above the level of 
conventional memory.   If you are not already using a memory manager, 
the following lines must be present to allocate memory high: 

dos = high,umb

device = c:\dos\himem.sys

device = c:\dos\emm386.exe noems

To change your memory allocation, follow these steps.

·	Change to your root directory by typing 

        c:

        at the DOS prompt.

·	Open your CONFIG.SYS file with your DOS editor by typing 

        edit config.sys

·	Add the necessary lines to the text.

·	Save your changes.

·	Exit the file.

·	Reboot the machine to effect this change.

-------------------------------------------------

Editing Your AUTOEXEC.BAT file

Once your workstation allocates "high" memory,  you must specify, in 
your AUTOEXEC.BAT file, which files you want loaded high.  We suggest 
loading high these files from the Foray PPP Client bundle:  

·	LSL.COM

·	IPXODI.COM

·	VLM.EXE

·	NETX.EXE.

Please note that attempting to load EWPPP.EXE  high does not 
improve use of memory on your workstation.

To load files into high memory, edit your AUTOEXEC.BAT in the 
following way: 

·	Change to your root directory by typing 

        c:

        at the DOS prompt.

·	Open your AUTOEXEC.BAT file with your DOS editor by typing 

        edit autoexec.bat.

·	Find each program file listed above.

·	Insert the load high command and a space in front of the program 
        file you want to load high.  For example, when you find the 
        program file

        c:\foray\lsl.com

        change the syntax to

        lh c:\foray\lsl.com

·	Save your changes.

·	Exit the file.

·	Reboot the machine to effect this change.

--------------------------------------------------

Editing Your NET.CFG file

If editing your CONFIG.SYS  and AUTOEXEC.BAT does not free up enough 
conventional memory, you can also edit NET.CFG.   We suggest that you find 
the Netware DOS Requester section of this file and add two lines to it:

load low conn = off

load low ipxncp = off 

These lines will load IP and IPX stacks into high memo

To edit your NET.CFG file, follow these steps.

·	Change to the directory in which your active NET.CFG file resides.  
        If you have not installed Novell before using the Foray PPP Client, 
        the NET.CFG will be in your FORAY directory.

·	Open your NET.CFG file with your DOS editor by typing 

        edit net.cfg

·	Find the Netware DOS Requester section in the file. 

·	Add the following lines under the Netware DOS Requester heading:

        load low conn = off

        load low ipxncp = off 

·	Save your changes.

·	Exit the file.

·	Reboot the machine to effect this change.

--------------------------------------------------

Tips for Configuring Your Workstation

·	IFSHLP.SYS is a device driver that is needed for Microsoft Networking 
        under Windows for Workgroups  (but not in Windows 3.1). When the user 
        runs Network Setup, Network Setup fails to install IFSHLP.SYS in some 
        circumstances.  You are missing this file in your CONFIG.SYS, if you 
        receive the following message in a dialogue box:

        "The Windows for Workgroups network was not started.  Check your 
        configuration, or run Setup again to set up Windows for Workgroups 
        properly.  The Windows for Workgroups network driver was unable to load."

·	To add IFSHELP.SYS to your CONFIG.SYS file, open the CONFIG.SYS with 
        your DOS editor and add the following line at the bottom of the file text:

        device = c:\windows\ifshelp.sys

·	Reboot the machine to effect this change.

          
