Colorado Backup for Windows 95 (By Cheyenne Software)
		 3.00 Release
	       December 10, 1996


This document contains important information about network
backups. It also includes information about installing the
HP Colorado T1000e tape drive and using our software on
computers with the new "Green" power-management feature.

Please contact our QICFAX service for the latest information
regarding our products.  QICFAX phone numbers are listed in
the back of your Colorado Backup manual.

SEE THE FOLLOWING INFORMATION ABOUT:
- Novell 2.x - 3.x network backup
- Novell 4.x network backup
- Windows95 network/Windows for Workgroups network backup
- Windows NT network backup
- Installing the HP Colorado T1000e tape drive
- Power-Management (GREEN) Computers
- Issues with the Scheduler
- Disaster Recovery with the ADAPTEC 1510 SCSI Card

NOVELL 2.x - 3.x NETWORK BACKUP

  To backup Novell 2.x - 3.x servers, use either:
  - Colorado Backup for DOS
    (reboot from DOS)
       or
  - Colorado Backup for Windows
    (reboot to DOS, then Windows 3.x)

  *DO NOT USE* Colorado Backup for Windows 95 to
   back up a Novell 2.x or 3.x server.

  To back up Win95 workstations, use Microsoft's Windows
  95 built-in Cheyenne ARCserve Client software (if the
  appropriate server application is installed on the server).
  See QICFAX document #2421 for more information.

  See +++ note below.


NOVELL 4.x NETWORK BACKUP

  Your Colorado PowerDAT or PowerTape (SCSI) tape drive
  must be installed on the server. IDE tape drives are
  not supported on the server.

  To back up Novell 4.x servers, use NLM software.

  To back up Win95 workstations, use Microsoft's Windows
  95 built-in Cheyenne ARCserve Client software (if the
  appropriate server application is installed on the server).
  See QICFAX document #2421 for more information.

  *DO NOT USE* Colorado Backup for DOS, Colorado Backup
  for Windows (Windows 3.x), or Colorado Backup for
  Windows 95 to backup a Novell 4.x server.

  See +++ note below.


WINDOWS 95 NETWORK BACKUP
WINDOWS FOR WORKGROUPS NETWORK BACKUP

  Colorado Backup for Windows 95 (CBW95) supports
  Win95 Network and Windows for Workgroups networks.

  IMPORTANT: CBW95 will back up *ONLY* the Win95 registry
  of the PC to which the tape drive is attached; the Win95
  registry of a remote PC will not be backed up.

  REMEMBER: Certain Windows 95 system files will always
  appear "in use."

  See +++ note below.


WINDOWS NT NETWORK BACKUP

  Your Colorado PowerDAT or PowerTape (SCSI) tape drive
  must be installed on the server.

  To back up NT servers, use Microsoft's built-in Windows
  95 NT drivers or appropriate 3rd party software.
  See QICFAX document #5225 for more information.

  To backup Win95 workstations, use Microsoft's Windows
  95 built-in Arcada Backup Exec Client for NT software
  (if the appropriate server application is installed on
  the server). See QICFAX document #2421 for more infor-
  mation.

  See +++ note below.
------------------------------------------------------------
+++ NOTE:
Currently,  there are no plans to include additional
network support in future versions of Colorado Backup for
Windows 95 software.
------------------------------------------------------------

INSTALLING THE HP COLORADO T1000e TAPE DRIVE

Special instructions for installing the HP Colorado T1000e
in Windows 95:

1. Power down your computer.

2. Power up your computer.

3. Install the T1000e's data cable.

4. Install the T1000e's power cable.

5. Insert a tape into the drive.

6. Follow the Installation Guide's directions for Installing
   the Software.

If you are having problems:
A. Click the Uninstall icon.
B. Right-click on the My Computer icon.
C. Click the Device Manager tab.
D. Verify that the HPTAPE and TAPEDRIVE sections are deleted.
E. Go to step one above.


POWER-MANAGEMENT (GREEN) COMPUTERS

If your computer has a power-management feature that shuts off
your computer after xx minutes since the last keyboard input...
you may experience problems with certain operations that exceed
the time limit.

Turn off the power-management feature when:

- running a long operation, such as formatting a tape

- running a full-system backup

- running a scheduled operation, such as an unattended
backup in the middle of the night

Check your computer's manual to find out how to turn off or
change the time limit of the power-management feature.

ISSUES WITH THE SCHEDULER

When you run a scheduled job when Colorado Backup is running,
you will recieve a message that the backup failed because 
only one instance of Colorado Backup can be run at a time.

To avoid recieving this error when scheduling jobs, insure that 
Colorado Backup is not running at the times you specify for 
scheduled backups.

DISASTER RECOVERY WITH THE ADAPTEC 1510 SCSI CARD

If your disaster recovery diskettes are unable to detect your Adaptec 1510 SCSI card, 
you may need to edit the DEVICE= line of the config.sys file.  Instructions are contained
within the config.sys file for selecting all the proper settings for the card.  To edit the
config.sys file on your disaster recovery disk, type the following at a DOS prompt within 
Windows 95.
				
				Edit A:\Config.sys


