=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-
   Adaptec EZ-SCSI 4.01a Setup Information

   (c) Copyright Adaptec, Inc.  1995-1996

=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-


=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-
Welcome to Adaptec EZ-SCSI 4.01a
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-

This readme is divided into 3 sections: Windows 95/NT, Windows 3.x
and DOS. Each section contains instructions on getting started, 
and specific tips for that Operating System(s). 
At the end of this file you will find a section on how to contact
Adaptec.

=-=-=-=-=-=-=-=-=

Windows 95 and NT

=-=-=-=-=-=-=-=-=

This section contains information on the following for
the above operating systems:

   A.) Getting Started
   B.) Help on installing Windows 95 from a SCSI CD-ROM
   C.) Help on installing NT on a SCSI hard drive


A.) Getting Started
===================

   Insert the "Adaptec EZ-SCSI Setup Disk" into your floppy drive 
   and run SETUP.EXE.
   Follow the instructions.

   When the Adaptec EZ-SCSI installation is complete, please select the
   "EZ-SCSI README" option for additional information.
  

B.) Help on Installing Windows 95 from a SCSI CD-ROM
====================================================

   1. Run DOS Install as explained in the DOS section, and
   reboot. All the drivers needed to view your CD-ROM 
   drive will be loaded in config.sys, and you will be able
   to install Windows 95.
   (This of course assumes you had DOS already loaded on your
   system so that EZ-SCSI could load MSCDEX. If this file
   is not available you will be prompted for it by EZ-SCSI)

   2. Take note of the lines containing aspi*dos.sys and aspicd.sys
   in config.sys, and MSCDEX in autoexec.bat.
   
   3. Install Windows 95

   4. Say yes when it asks you should it create an emergency
   repair diskette for you. 

   5. When installation is complete you should copy the lines 
   noted in step 2 above into config.sys and autoexec.bat
   on this emergency diskette. This disk will allow you to
   reboot your system in an emergency and
   access your CD-ROM to restore Windows 95.

D.) Help on Installing NT on a SCSI hard drive
==============================================

   If you do a floppyless install of NT 3.51 from 
   your SCSI CD-ROM using winnt /b, you may run into
   a blue screen the first time the NT Installer
   reboots your system. The reason for this is the
   installer cannot find your SCSI harddrive.
   You must reboot again, and just after the banner for
   NT appears, you have 2 seconds within which to
   press F6. This will pop up the screen that allows
   you to specify your SCSI host adapter. You should 
   specify Other and insert the EZ-SCSI setup floppy
   when it requests one. Then continue with the rest
   of the installation.
   
   This trick is also useful, if during installation
   you want NT to use the host adapter driver on the 
   EZ-SCSI setup disk instead of the usually older 
   embedded driver.


=-=-=-=-=-=-=-=-=-=-=

    Windows 3.1x

=-=-=-=-=-=-=-=-=-=-=


   Getting Started
   ===============

   Insert the "Adaptec EZ-SCSI Setup Disk" into your floppy drive 
   and run SETUP.EXE.
   Follow the instructions.

   When the Adaptec EZ-SCSI installation is complete, please select the
   "EZ-SCSI README" option for additional information.


=-=-=-=-=-

   DOS

=-=-=-=-=-

   Getting Started
   ===============

   Insert the EZ-SCSI 4.01 Disk number 2 into your floppy drive, 
   change to your floppy's drive letter, and run DOSINST.BAT.  
   For example:

        C:\> A: 
        A:\> DOSINST <Enter>

        Follow the instructions.




=-=-=-=-=-=-=-=-=-=
CONTACTING ADAPTEC
=-=-=-=-=-=-=-=-=-=

Technical Support:

  Automated Technical Support:      U.S. and Canada:  (800) 959-7274
  ----------------------------      International:    (408) 945-2550
  o  Interactive FAX Service
  o  On-line Questions & Answers         
   
  Live Technical Support:           U.S. , Canada &
  -----------------------           International:    (408) 934-7274
  o  M-F: 6:00am to 5:00pm  Pacific Standard Time

Literature Hotline:                                    (800) 934-2766
   o M-F: 6:00am to 5:00PM Pacific Standard Time

Software Ordering (U.S.A. and Canada):                 (800) 442-7274
   o M-F: 6:00am to 5:00pm Pacific Standard Time

International Software Ordering:                       (408) 957-7274
   o M-F: 6:00am to 5:00pm Pacific Standard Time

Bulletin Board Service (BBS):                          (408) 945-7727
   o 24 hours a day (up to 28800 bps, using 8 data bits,
                     1 stop bit, no parity)

CompuServe Support                                         GO ADAPTEC

The Microsoft Network (MSN)                                GO ADAPTEC

World-Wide Web                                 http://www.adaptec.com

FTP (login as user "anonymous")                       ftp.adaptec.com

Internet E-Mail support                           support@adaptec.com

          