SYMANTEC LOCALISATION GROUP IRELAND

README.TXT
Copyright (c) 1996 Symantec Corp. All Rights Reserved.

NORTON COMMANDER FOR WINDOWS 95/NT

Welcome to Norton Commander for Windows 95/NT
------------------------------------------
Please read this document carefully. It contains important information
not included in the documentation.

     Topics covered in this document include:
	
	* NT Workstation Users Information
	* Key Commands Changed from Previous Versions
	* Troubleshooting
	* Commander Link File Transfer
	

NT Workstation Users Information
------------------------------------------------- 

- To map a network drive, please follow the instructions for NT Server users. The Path drop-down listbox will not display all previously attached servers and areas, however.
	

Keys changed from previous versions.
------------------------------------

- ALT+F6 has been changed to ALT+F9. (ALT+F6 is used by Windows 95 and
cannot be used by Commander.)

- Editor:
Shortcut keys ALT+F6 (Count) and ALT+F8 (Goto) have been changed to F6
and F8.
Save As has been changed to ALT+F then A.

- Configurable Speed Search Keys:
You can configure how Norton Commander interprets the keyboard - as in
previous versions of Norton Commander or as in Windows 95. The new
default for speed search is CTRL+ALT. To change your keyboard
interpretation, choose Configuration from the Commands menu. On the
Compatibility tab of the Configuration Options dialog, selecting the
<ALT> option changes speed search to work as in previous version of
Norton Commander.

- Command History:
CTRL+UP-Arrow and CTRL+DOWN-Arrow offer the ability to go back and forth,
selecting commands from the command line history. These replace the old
CTRL+X and CTRL+E keys.


Troubleshooting
----------------------
Q: Why do I get a Sharing Violation error?
A: You may get this error if you tried to perform an operation on a
file that is being used by another application.

Q: Why can't I view any files?
A: Norton Commander utilizes the Microsoft Quick View or the Inso Quick
View Plus viewer. If neither of these are installed on your system,
Commander will use its own internal text viewer. Consult your Windows 95
Installation Guide, or see the online help about obtaining Quick View
Plus. Also see the end of this document.

Q: How do I remove the NC Scheduler from my taskbar?
A: The NC Scheduler must be shut down first. If you want to turn the NC
Scheduler off permanently, choose Shut Down from the NC Scheduler
Options menu.
 
Q: When I drag an .EXE or .COM file to the other panel, why does it not
copy the file?
A: When you drag a single .EXE or .COM file to another location,
Windows 95 assumes that you are creating a shortcut. To copy the files,
hold down the CTRL key while dragging files.
	
Q: Why have I lost my templates in the Filter/Cleanup Filter dialogs? 
A: The Norton Commander registry entries have been corrupted somehow.
To fix this, shut down Norton Commander and run the NC.REG file, which
is found in the Norton Commander directory. This will restore your Norton
Commander registry back to its default.

Q: Why can't I associate a file extension with more than one application?
A: Norton Commander now only supports one association per extension.

- See Troubleshooting in the online help for additional information on
errors you might come across.


Incomplete Installation
------------------------
"Setup has found an incomplete installation. This
is probably due to installing or uninstalling a
Symantec product without restarting your system.
Please reboot your computer to complete the
previous installation before running setup again."

If you see this message, the installation did not complete successfully.
This is caused by Setup finding ~SYMINST.EXE and _SYMINST.BAT in the
Windows directory. To complete the installation remove these files
from the Windows directory and restart Setup.

This also applies to the uninstall process.


Commander File Transfer
--------------------------
	
	<> Pin layout of the cables.

	You must use a Commander Link Cable to link two computers 
	together. 


	<> Problems Linking.
	If you have problems linking two machines, you should try the 
	following simple method.

	(1) Join two machines using the Commander Link cable
            (Serial/Parallel)
	(2) Turn the Status bar on.
	(3) From the Commands menu (on both machines), choose Scan for 
	    Connection.
	(4) The Status bar will indicate that the machine is scanning. 
	(5) When a connection is made the Status bar indicates
	    this with : "Link: LPT#/COM#".
	(6) Once connection has been made, the menu item 'Link' in the 
	    Left/Right menu on both machines becomes enabled. 
	(7) Select Link from the Left/Right menu and you will see 
	    the other machine in that panel.

	<> Problems with Long File Names and the Link.
	   You can only copy LFNs across the Link if the Target Drive
           supports them.
		
	<> Pin layout of the serial cables.

	    9 - 9 Serial           9 - 25 Serial         25 - 25 Serial
					          
	    2 ======= 3             2 ======= 2	         2 ======== 3
	    3 ======= 2             3 ======= 3	         3 ======== 2
	    4 ======= 6             4 ======= 6	         4 ======== 5
	    5 ======= 5             5 ======= 7	         5 ======== 4
	    6 ======= 4             6 ======= 20         6 ========20
	    7 ======= 8             7 ======= 5	         7 ======== 7
	    8 ======= 7             8 ======= 4	        20 ======== 6
	
	<> Pin layout of the parallel cable.

	                            1 ======= 7
				    2 ======= 15
				    3 ======= 13
				    4 ======= 12
				    5 ======= 10
				    6 ======= 11
				    7 ======= 1
				    8 ======= 14
				    9 ======= 16
				   10 ======= 5
				   11 ======= 6
				   12 ======= 4
				   13 ======= 3
				   14 ======= 8
				   15 ======= 2
				   16 ======= 9
				   17 ======= 17
				   18 ======= 18
				   19 ======= 19
				   20 ======= 20
				   21 ======= 21
				   22 ======= 22
				   23 ======= 23
				   24 ======= 24
				   25 ======= 25



---------------------------------END------------------------------
