                        Sentinel Driver
                          Version 2.1
                     Installation Procedure
 
1. Under the Microsoft Windows NT Main group, select Control Panel.

2. In the Control Panel group, select Drivers.

3. When the driver list appears, select the ADD button.

4. Choose "Unlisted or Updated" from the Driver list and select the OK button.

5. Place the EZ-Setup diskette in the floppy disk drive, specify its location and
   select OK.

6. Select the Sentinel x86-based driver and select OK.

7. The Sentinel Driver and associated files are copied to the hard disk.
   The file SNTI386.DLL and SENTTEMP.HLP will be copied into
   \%SYSTEMROOT%\SYSTEM32.  The file SENTTEMP.HLP will be copied to
   SENTINEL.HLP.  The file SENTTEMP.SYS will be copied to the file
   \%SYSTEMROOT%\SYSTEM32\DRIVERS\SENTINEL.SYS.
  %SYSTEMROOT% is the directory where Microsoft Windows NT has been
   installed.

8. The Sentinel Driver setup program is automatically started.  Configure
   the Sentinel Driver for your computer.  The Help button can be selected
   for configuration information.

9. Restart your computer as directed at the end of the installation 
   procedure.
