GHOST and GHOST Utilities
Copyright (C) 1998 Symantec Corporation
All Rights Reserved

See WHATSNEW.GHO for a list of changes in this version.

GHOST (General Hardware Oriented System Transfer) is a system
cloning application which eases the task of upgrading hard
drives and/or replicating many systems on a concurrent basis.
For program details please refer to the V5MANUAL.PDF
documentation supplied with this package.


List of Files

    The GHOST Upgrade package consists of the following files:

    BUGFORM.TXT  - Form for submitting bug reports.
    ERROR.TXT    - List of common errors and solutions.
    GHOST.EXE    - This is it, the one that does all the work.
    GHOSTFAQ.TXT - Frequently Asked Questions.
    LICENSE.TXT  - Pricing and Licensing information.
    README.TXT   - Introductory information.
    SWITCHES.TXT - A listing of command line switches.
    UPGRADE.TXT  - Directions for "binding" your new GHOST.
    V5MANUAL.PDF - The GHOST manual in Adobe Acrobat format.
    WHATSNEW.TXT - Latest enhancements and bug fixes.

    If you did not receive all these files please contact GHOST
    Technical Support via electronic mail at support@ghosthelp.com.


Documentation and Support

    Full documentation is provided in the V5MANUAL.PDF file. If
    you do not have the Adobe Acrobat Reader required to read PDF
    files, you can download it from:
    http://www.adobe.com/prodindex/acrobat/readstep.html

    Technical Support information is available online at
    http://www.ghosthelp.com.


System Requirements

    SYSTEM
    ------
    Processor         - Minimum 386SX -> 486 or above recommended
    RAM               - 4MB (8MB for NTFS) -> 16 MB recommended
    Operating System  - DOS 5.0 or above
    Monitor           - VGA
    Pointing Device   - None required -> MS Compatible recommended

    FEATURES
    --------
    Peer to Peer LPT/Parallel Port Connection - Laplink or
    equivalent cable. Bi-directional parallel port with EPP or ECP
    compatibility on each PC.

    Peer to Peer NetBIOS Connection - Ethernet or Token Ring
    Network Interface Card. Established Network connection which
    includes one of the following:
    - Crossover Ethernet cable (pins 1236 to 3612)
    - Coaxial cable
    - Standard cables with HUB or MAU
    Additional Network software required (These components are
    available from http://www.ghosthelp.com):
    - LSL.COM
    - MLID ODI driver (Your Network card's ODI driver)
    - IPXODI.COM
    - NetBIOS.EXE

    SCSI Tape Drive - Loaded DOS ASPI driver. SCSI tape drive.
    Tape media.

    Multicast - Ethernet or Token Ring NIC. Established Network
    connection. NIC Packet drivers and/or NDIS2.01 NIC driver.
    Optional Multicast-enabled router. Optional BOOTP/DHCP
    software.

    Removable Media - Removable media drive and media. Media
    drivers required to use in DOS.

    CD-ROM Usage - CD-ROM Writer. CD-ROM Writer's disk creation
    software (Mastering Software).

    Mapped Network Drive - Network interface card. Established
    network connection. DOS Network software client to provide
    mapped drives.
