EDA.Client.v3.23.Cracked-iNW


                      EDA Client is the communications subsystem that initiates and sustains
                      synchronous or asynchronous communications between connected client
                      and server environments. EDA Client identifies and manages all network
                      communications during queries, interprets and packages the application
                      queries appropriately for transportation to each target EDA Server
                      environment, and provides data compression and decompression for
                      enhanced performance in data transfer. 

                      EDA Client shields applications and EDA Servers from the details
                      associated with sending or receiving information across proprietary
                      communications networks. It also optimizes server responsiveness and
                      fault tolerance and improves data transfer rates between EDA clients
                      and servers. 

                      EDA Client supports most major network protocols, such as TCP/IP, LU
                      6.2, SPX, NetBIOS, and LU 0, and is available on the following
                      platforms: Windows, Windows NT, Macintosh, OS/2, MVS, UNIX,
                      CICS, VM, OpenVMS, Tandem, and AS/400. 

unzip and run setup  ...  eNJOY =]



