
    .             /\                                  /\
    . /\_________/  \ _______/\    _____/\ _______/\ /  \ ___________/\_____/\
    : \     ____/    \\____    \  /   ___//    ____//    \\___     ___/   ___/
    | /    ___/ \____/ /  /    / /   __/\ \       \ \____/   /     | /   __/\    
    |/      |   /    \/   \    \/        \/\___    \/    \  /      |/        \   
    / ______|  /_____ \____\    \________ \______  /_____ \/______ |\________ \  
    \/-[  xx/03  ]---\/-----\____\-------\/------\/------\/-------\|-------+ \/
    [PERMIT/Client NT 4.0 v1.10.021]=========================>99/09/20

	Operating system:  Windows NT 4.0 (workstation)
	Cpu: P90
	Ram: 24mb
	Hdd: 10mb

	With an increased number of remote users traveling the
	globe, organizations are finding it harder to provide
	secure connectivity to their corporate network that is
	more flexible and cost effective than traditional remote
	access.
	With PERMIT/Client(TM) software, remote users are able to
	remain securely connected to their corporate LAN anytime,
	anywhere. PERMIT/Client secures network traffic for a
	single workstation running Win 95/98, Win NT 4, or
	Mac OS 7.1 (or later). TimeStep ’s client software supports
	multiple IPSec tunneling modes for different connection
	types as well as two-factor user authentication, using the
	RADIUS protocol.

	PERMIT/Client Features

	Encryption:     DES, 3-DES, RC5, CAST, Blowfish,
	                IDEA (optional)

	Authentication: Certificate-based with RSA signatures,
	                shared secret, IKE-XAUTH secured RADIUS,
        	        ACE/SecurID, NT domain, NDS, and TACACS+

	Integrity:      HMAC-MD5, HMAC-SHA-1

	Key management: features IKE (formerly ISAKMP/Oakley),
	                Diffie-Hellman

	Protocol
	support:        TCP/IP, IPSec ESP/AH, LDAP

	Security
	standards:      IPSec, IKE, IKE-XAUTH, X.509v3, RSA

	Connection
	types:          PPP, Ethernet, Token Ring, cable modem,
        	        xDSL, ISDN

	Certification:  ICSA-IPSec

	Key Benefits of Permit/Client

	Transparency PERMIT/Client, a network layer security solution,
	is fully transparent, securing communications invisibly to the
	user and applications. The integrated PKI provides automated
	certificate enrollment, revocation, and updating eliminating
	the need to manually download certificates and CRLs.

	Simple enterprise-wide deployments
	With preconfigured installations, predefined policy, remote
	address management, and multiple connection profiles,
	PERMIT/Client allows administrators to quickly deploy users
	even over their corporate intranets.

	Interoperability
	PERMIT/Client is an interoperable IPSec-compliant solution
	that is IPSec-certified by the International Computer Security
	Association (ICSA).

	Flexibility
	TimeStep provides flexibility for your users by supporting
	various IPSec tunneling modes including tunneling private
	addresses over public networks. With Dedicated Tunneling, one
	secure tunnel is created back to the IP-VPN gateway ensuring
	all traffic is subject to the corporation’s firewall policy.
	TimeStep’s Virtual Tunneling, which hides both the source AND
	destination address of packets, enables mobile users to login
	to their privately addressed corporate network, from any ISP,
	and surf the Internet simultaneously.    