                                   /;    ;\
                               __  \\____//
                              /{_\_/   `'\____
                              \___   (o)  (o  }
        ________________________/          :--'   MOOO!
   ,-"'`@@@@@@@@     @@@@         \_    `__\
  ;:(  @@@@@@@@@      @             \___(o'o)
  :: )  @@@@        @@@@        ,'@@(  `===='
  :: : @@@@@:        @@         `@@@:
  :: \  @@@@@:     @@@@@)    (  '@@@'
  ;; /\      /`,  @@@@@@@\   :@@@@@)
  ::/  )    {____------___:  :~`,~~;
 ;;'`; :   )              :  / `; ;
;;;; : :   ;              :  ;  ; :
    )_ \__;     ";"       :_ ;  \_\       `,','
    :__\  \   * `,'*      \  \  :  \   *  8`;'*  *
        `^'    \ :/        `^'  `-^-'   \v/ :  \/ 

---

INDPENDENT COWS PRESENTS:
EMULive Active Theatre Version 3.9.50
(C) EMULive Imaging Corporation 

--

Picks up all the live or prerecorded action from
 EMULive Servers. 20 Channel "surfable" remote 
control offers online and offline dialing directories, 
high-speed broadcast recording & playback with 
fast-forward/rewind, text chat, encryption, file 
transfer, HDTV style video aspect ratio, VU meter, 
volume controls and much more. Video viewport is 
fully resizable and can be blown up full screen at 
any resolution. Requires a 8MB Pentium PC with 
Windows95 or WindowsNT. 16-BITsound card, MMX CPU 
and accelerated video hardware are recommended, 
but are not required. Operates at 1200bps to 
2Mbps+ over TCP/IP networks including LAN's, 
WAN's, Intranets and the Internet. On a mid-range 
PC, Active Theatre is capable of playing back at 
30FPS with near-CD quality synchronized sound. 

Author: EMULive Imaging Corporation 

GREETING: MAYBITCH @£$@£$£@$£@$@£$@$£@£$@£$@£$£@$£$£
	  ZEWMAH!"#¤/)¤#/!)/)"#¤/)#¤	  
 ICH LIEBE DICH:: "#%(SFD
	  

