/*
 * INSTALL.DAT
 *
 * Project: NewWorld Operating Environment (NWOE)
 * Version: Beta
 *
 * This INSTALL.DAT was automatically generated by DDB
 */

@DefineProject
	@Name = "NWOE"
	@Version = "2.0"
	@Subdir = "\\NEWWORLD"
	@Requires @HardDisk
	@OutDrive = C
@EndProject

@If (@CPU < 286)
	NWOE requires an 80286, 80386SX, 80386, 80486 ... to run
	@Abort
@Endif

@DefineVars
	@Qstring @MFMDevice = ""
	@Qstring @ADPDevice = ""
	@Qstring @ABIOSDevice = ""
	@Qstring @CDDevice = ""
@EndVars



@Display
	@Cls

	About to install: 

	NewWorld Operating Environment (NWOE) version @Version

	on your computer system and verify the integrity of the
	distribution disk(s).  You may press the [Esc] key at any time to
	abort the installation.

	You will be asked several questions about your computer hardware.

	Each question has a default answer.  If the default answer is
	correct, press the ENTER key in response to the question.
	Otherwise, type the answer or use  and  keys to higlight your
	choice and then press the ENTER key.

	If you make a mistake while typing, press the BACKSPACE key
	and then retype the answer.

	@Pause
@EndDisplay

@GetOutDrive
	@Cls

	On which disk drive do you wish to install @Name?

@EndOutDrive

@GetSubdir
	@Cls
	Now you need to specify the disk destination subdirectory.  The
	subdirectory is the location on your disk where the @Name system
	will be installed.  If you don't know what a "subdirectory" is, you
	probably need not worry about it, and should hit the enter key to
	accept the default directory.






	@Prompt = "Which subdirectory ([Enter] = @Subdir) ?"
@EndSubdir

@GetOption
	@Cls

	Select your DVI hardware configuration:











	@Option 3 = "ActionMedia-AT Board with NTSC Monitor"
	@Option 4 = "ActionMedia-AT Board with VGA Monitor"
	@Option 5 = "ActionMedia II-AT Board with PAL Monitor"
	@Option 6 = "ActionMedia II-AT Board with NTSC Monitor"
	@Option 7 = "ActionMedia II-AT Board with VGA Monitor"
	@Option 10 = "ActionMedia II-MCA Board with PAL Monitor"
	@Option 8 = "ActionMedia II-MCA Board with NTSC Monitor"
	@Option 9 = "ActionMedia II-MCA Board with VGA Monitor"
	Please select the DVI hardware configuration that you have
	in your system.  You must know what type of DVI card you have
	as well as what type of monitor you have connected to it.

	If you are not sure which DVI card you have contact your 
	hardware vendor.

@EndOption

/*
**	Set up default config options for the DS1 cards
*/
@If(3 [= @Option || 4 [= @Option)
	@DefineVars
		@Qstring @AudCode = "~"
		@Qstring @DefPort = "/P0x2E0"
		@Qstring @DefVPort = "/P2E0"
		@QString @DefIntlvl = "/L9"
		@QString @DefAIntLvl = "~"
		@QString @DefSIntLvl = "~"
		@QString @DefvAIntLvl = "~"
		@QString @DefvSIntLvl = "~"
	@EndVars
@Endif

@If (3 [= @Option || 4 [= @Option)
	@DefineVars
		@QString @ucode = "ucode"
	@EndVars
@Endif


/*
**	Set up default config options for the DS2 cards
*/
@If(5 [= @Option || 6 [= @Option || 7 [= @Option) 
	@DefineVars
		@Qstring @AudCode = "2105.bin"
		@Qstring @DefPort = "/P0x2E4"
		@Qstring @DefVPort = "/P2E4"
		@QString @DefIntlvl = "/L9"
		@QString @DefvAIntLvl = "/A0xB"
		@QString @DefvSIntLvl = "/S0xA"
		@QString @DefAIntLvl = "/AB"
		@QString @DefSIntLvl = "/SA"
		@QString @ucode = "ucode2"
	@EndVars
@Endif

/*
**	Set up defaults for conf options for MCA DS2 boards
*/
@If(8 [= @Option || 9 [= @Option || 10 [= @Option) 
	@DefineVars
		@Qstring @AudCode = "2105.bin"
		@Qstring @DefPort = "/P0xc000"
		@Qstring @DefVPort = "/Pc000"
		@QString @DefIntlvl = "/L9"
		@QString @DefvAIntLvl = "/A0xB"
		@QString @DefvSIntLvl = "/S0xA"
		@QString @DefAIntLvl = "/AB"
		@QString @DefSIntLvl = "/SA"
		@QString @ucode = "ucode2"
	@EndVars
@Endif
@If (3 [= @Option || 4 [= @Option) 

@GetOption
	Enter the base memory address of your VRAM window.  64K is required.








	@Option 1100 = "C000"
	@Option 1101 = "D000"
	@Option 1102 = "E000"

	A 64K EMS window is required for access to the DVI Video Ram.
	Please select the base address in host memory which will
	Correspond to this area.  Make sure that there are no conflicts
	with other devices installed.
@EndOption
@Endif

/*
**	For DS2 cards, only a 32k window is required.
*/
@If (5 [= @Option || 6 [= @Option || 7 [= @option || 8 [= @Option || 9 [= @Option || 10 [= @Option)

@GetOption
	Enter the base memory address of your VRAM window.  32k is required.










	@Option 1100 = "C000"
	@Option 1103 = "C800"
	@Option 1101 = "D000"
	@Option 1104 = "D800"
	@Option 1102 = "E000"
	@Option 1105 = "E800"

	A 32K EMS window is required for access to the DVI Video Ram.
	Please select the base address in host memory which will
	Correspond to this area.  Make sure that there are no conflicts
	with other devices installed.
@EndOption
@Endif

@If (1100 [= @Option)
	@DefineVars
		@QString @DefWindow = "/W0xC000"
		@QString @DefVWindow = "/WC000"
	@EndVars
@ElseIf (1103 [= @Option)
	@DefineVars
		@QString @DefWindow = "/W0xC800"
		@QString @DefVWindow = "/WC800"
	@EndVars
@ElseIf (1101 [= @Option)
	@DefineVars
		@QString @DefWindow = "/W0xD000"
		@QString @DefVWindow = "/WD000"
	@EndVars
@ElseIf (1104 [= @Option)
	@DefineVars
		@QString @DefWindow = "/W0xD800"
		@QString @DefVWindow = "/WD800"
	@EndVars
@ElseIf (1102 [= @Option)
	@DefineVars
		@QString @DefWindow = "/W0xE000"
		@QString @DefVWindow = "/WE000"
	@EndVars
@ElseIf (1105 [= @Option)
	@DefineVars
		@QString @DefWindow = "/W0xE800"
		@QString @DefVWindow = "/WE800"
	@EndVars
@EndIf

/*
**	If this is a microchannel machine, skip the questions on
**	hard disks and cd-roms
*/
@If (8 [= @Option || 9 [= @Option || 10 [= @Option)
@GetOption
	@Cls

	Would you like to install the ABIOS Screaming Device Driver
	in your autoexec.bat?




	@Option 2001 = "No"
	@Option 2000 = "Yes"


	The ABIOS screaming device driver is optimized to play motion
	video by bypassing DOS I/O and generally gives better performance
	than DOS.  Select "Yes" to install this device driver.
@EndOption

@If (2000 [= @Option)
	@GetString @ABIOSDevice
	The ABIOS driver command line has the following format:

	c:v c:v ... 

		Where:	c	is the drive letter of first logical drive 
				on the physical disk
	                v	is the physical DOS drive number

	For example, a PC that has 2 MFM hard disks with the first drive 
	having drive letters C:, E:, and F: and the second drive has D: and G:, 
	the following command line would be used:
			     
			C:0 D:1

	For additional information refer to the installation notes.

	@EndString	   		
@Endif
/*
**	If AT base machine, check for MFM, ADAPTEC and CD-ROM drivers
*/
@Else

@GetOption
	@Cls

	Do you have one or more MFM compatible hard drives in your
	system?




	@Option 1001 = "No"
	@Option 1000 = "Yes"


	If you have one or more MFM compatible hard drives and you plan
	to play motion video from one of them, select "Yes", otherwise
	select "No".  
@EndOption

@If (1000 [= @Option)
	@GetString @MFMDevice
	The MFM driver command line has the following format:

	c:v c:v ... 

		Where:	c	is the drive letter of first logical drive 
				on the physical disk
	                v	is the physical DOS drive number

	For example, a PC that has 2 hard disks with the first drive 
	having drive letters C:, E:, and F: and the second drive has D: and G:, 
	the following command line would be used:
			     
			C:0 D:1

	For additional information refer to the installation notes.

	@EndString	   		
@Endif

@GetOption
	@Cls

	Do you have one or more Adaptec/SCSI compatible hard drives in your
	system?




	@Option 1011 = "No"
	@Option 1010 = "Yes"


	If you have one or more Adaptec compatible hard drives and you plan
	to play motion video from one of them, select "Yes", otherwise
	select "No".  
@EndOption

@If (1010 [= @Option)
	@GetString @ADPDevice
	The Adaptec disk driver command line has the following format:

	c:vtl c:vtl ... 

		Where:	c	is the drive letter of first logical drive 
				on the physical disk
	                v	is the DOS drive number
			t	is the SCSI target number of the disk
			l	is the SCSI unit number of the disk

	For example a PC that has 1 SCSI disk drive with drive letters C:
	and D: would use the following command line:
			     
			C:000

	If your system contains both an MFM disk as physical drive 0
	and a scsi disk as physical drive 1 starting with logical drive D:
	The command line is:

			D:100

	For additional information refer to the installation notes
	@EndString	   		
@Endif


@GetOption
	@Cls
	
	Do you have a CD drive connected to your DVI card?





	@Option 1021 = "No"
	@Option 1020 = "Yes"


	If you have a CD player connected to your DVI card and would like
	to use it for playing motion video, select "Yes".  Otherwise,
	select "No".

	If you select "Yes", low level drivers will be installed to allow
	MSCDEX.exe to access the CD drive as a standard DOS device.  However,
	MSCDEX.exe is NOT part of this distribution package and must
	be aquired separately.  If you do not have MSCDEX.exe, select
	"No".

@EndOption

@If (1020 [= @Option)
	@GetString @CDDevice
	Specify the drive letter for the  CD player. If the CD player is 
	given the driver letter Z by mscdex type "Z:". You must enter the
	drive letter and the colon, but not the quotes.




	@EndString	   		
@Endif

@Endif


@DefineDisk
	@Label = "Disk #1"

	@BeginLib NWOE.001
		@File SAMP256.IMV @Size 3900 @Out IM\SAMP256.IMV
		@File SAMP256.IMU @Size 3900 @Out IM\SAMP256.IMU
		@File SAMP256.IMY @Size 61500 @Out IM\SAMP256.IMY
		@File ULTRA.118 @Size 3932 @Out FONT\ULTRA.118
		@File V15TO32.BIN @Size 911 @Out UCODE2\V15TO32.BIN
		@File V16TO32.BIN @Size 911 @Out UCODE2\V16TO32.BIN
		@File V32TO15.BIN @Size 995 @Out UCODE2\V32TO15.BIN
		@File V32TO16.BIN @Size 995 @Out UCODE2\V32TO16.BIN
		@File VBLEND.BIN @Size 1576 @Out UCODE2\VBLEND.BIN
		@File VBLENDM.BIN @Size 2034 @Out UCODE2\VBLENDM.BIN
		@File VCHECK.BIN @Size 883 @Out UCODE2\VCHECK.BIN
		@File VCHECKA.BIN @Size 883 @Out UCODE2\VCHECKA.BIN
		@File VCLEAR.BIN @Size 584 @Out UCODE2\VCLEAR.BIN
		@File VCLUT.BIN @Size 6463 @Out UCODE2\VCLUT.BIN
		@File VCOLOR.BIN @Size 3324 @Out UCODE2\VCOLOR.BIN
		@File VCOPY.BIN @Size 3997 @Out UCODE2\VCOPY.BIN
		@File VCOPYM.BIN @Size 1294 @Out UCODE2\VCOPYM.BIN
		@File VCOPYMAP.BIN @Size 1333 @Out UCODE2\VCOPYMAP.BIN
		@File VCOPYMSK.BIN @Size 1679 @Out UCODE2\VCOPYMSK.BIN
		@File VCOPYPL.BIN @Size 1305 @Out UCODE2\VCOPYPL.BIN
		@File VCOPYSK.BIN @Size 1272 @Out UCODE2\VCOPYSK.BIN
		@File VD080003.BIN @Size 20051 @Out UCODE2\VD080003.BIN
		@File VD080004.BIN @Size 20051 @Out UCODE2\VD080004.BIN
		@File VD080005.BIN @Size 20331 @Out UCODE2\VD080005.BIN
		@File VD080128.BIN @Size 4805 @Out UCODE2\VD080128.BIN
		@File VD080192.BIN @Size 5672 @Out UCODE2\VD080192.BIN
		@File VD080193.BIN @Size 7742 @Out UCODE2\VD080193.BIN
		@File VD080194.BIN @Size 2380 @Out UCODE2\VD080194.BIN
		@File VD080195.BIN @Size 12390 @Out UCODE2\VD080195.BIN
		@File VD160001.BIN @Size 1333 @Out UCODE2\VD160001.BIN
		@File VD160002.BIN @Size 1683 @Out UCODE2\VD160002.BIN
		@File VDIFF.BIN @Size 1368 @Out UCODE2\VDIFF.BIN
		@File VDIGIPL.BIN @Size 1141 @Out UCODE2\VDIGIPL.BIN
		@File VDTOI16.BIN @Size 1668 @Out UCODE2\VDTOI16.BIN
		@File VDTOV16.BIN @Size 494 @Out UCODE2\VDTOV16.BIN
		@File VE080128.BIN @Size 16080 @Out UCODE2\VE080128.BIN
		@File VE160001.BIN @Size 4264 @Out UCODE2\VE160001.BIN
		@File VE160002.BIN @Size 6448 @Out UCODE2\VE160002.BIN
		@File VE320192.BIN @Size 5566 @Out UCODE2\VE320192.BIN
		@File VE320193.BIN @Size 9514 @Out UCODE2\VE320193.BIN
		@File VE320194.BIN @Size 3368 @Out UCODE2\VE320194.BIN
		@File VE320195.BIN @Size 5160 @Out UCODE2\VE320195.BIN
		@File VE32A192.BIN @Size 5846 @Out UCODE2\VE32A192.BIN
		@File VE32A193.BIN @Size 9724 @Out UCODE2\VE32A193.BIN
		@File VEDGEFIX.BIN @Size 2929 @Out UCODE2\VEDGEFIX.BIN
		@File VELLIPSE.BIN @Size 3569 @Out UCODE2\VELLIPSE.BIN
		@File VFADE.BIN @Size 2638 @Out UCODE2\VFADE.BIN
		@File VFILTER.BIN @Size 3954 @Out UCODE2\VFILTER.BIN
		@File VFISH.BIN @Size 3886 @Out UCODE2\VFISH.BIN
		@File VFISHSIZ.BIN @Size 2731 @Out UCODE2\VFISHSIZ.BIN
		@File VFLOOD.BIN @Size 2686 @Out UCODE2\VFLOOD.BIN
		@File VFLOODU.BIN @Size 116 @Out UCODE2\VFLOODU.BIN
		@File VFLOODW.BIN @Size 116 @Out UCODE2\VFLOODW.BIN
		@File VIDLE.BIN @Size 578 @Out UCODE2\VIDLE.BIN
		@File VIMAGE.BIN @Size 5976 @Out UCODE2\VIMAGE.BIN
		@File VINT.BIN @Size 144 @Out UCODE2\VINT.BIN
		@File VINTERP.BIN @Size 692 @Out UCODE2\VINTERP.BIN
		@File VISCALE.BIN @Size 6784 @Out UCODE2\VISCALE.BIN
		@File VJUMP.BIN @Size 228 @Out UCODE2\VJUMP.BIN
		@File VKTEXT8.BIN @Size 2940 @Out UCODE2\VKTEXT8.BIN
		@File VLINE.BIN @Size 1356 @Out UCODE2\VLINE.BIN
		@File VMIRROR.BIN @Size 116 @Out UCODE2\VMIRROR.BIN
		@File VMOSAIC.BIN @Size 1156 @Out UCODE2\VMOSAIC.BIN
		@File VPARM.BIN @Size 536 @Out UCODE2\VPARM.BIN
		@File VPOLY.BIN @Size 116 @Out UCODE2\VPOLY.BIN
		@File VPOLY2D.BIN @Size 18884 @Out UCODE2\VPOLY2D.BIN
		@File VPOLY2DC.BIN @Size 116 @Out UCODE2\VPOLY2DC.BIN
		@File VPOLY2DS.BIN @Size 116 @Out UCODE2\VPOLY2DS.BIN
		@File VPOLY2DT.BIN @Size 116 @Out UCODE2\VPOLY2DT.BIN
		@File VRANGE.BIN @Size 1113 @Out UCODE2\VRANGE.BIN
		@File VRECT.BIN @Size 1564 @Out UCODE2\VRECT.BIN
		@File VREPLAC2.BIN @Size 2114 @Out UCODE2\VREPLAC2.BIN
		@File VREPLACE.BIN @Size 1474 @Out UCODE2\VREPLACE.BIN
		@File VRETURN.BIN @Size 522 @Out UCODE2\VRETURN.BIN
		@File VROUND.BIN @Size 3299 @Out UCODE2\VROUND.BIN
		@File VSCALE.BIN @Size 9234 @Out UCODE2\VSCALE.BIN
		@File VSKEW.BIN @Size 1436 @Out UCODE2\VSKEW.BIN
		@File VSWITCH.BIN @Size 696 @Out UCODE2\VSWITCH.BIN
		@File VTESTH.BIN @Size 688 @Out UCODE2\VTESTH.BIN
		@File VTESTPC.BIN @Size 2208 @Out UCODE2\VTESTPC.BIN
		@File VTESTV.BIN @Size 1328 @Out UCODE2\VTESTV.BIN
		@File VTEXT1.BIN @Size 1772 @Out UCODE2\VTEXT1.BIN
		@File VTEXT2.BIN @Size 1942 @Out UCODE2\VTEXT2.BIN
		@File VUNCLUT.BIN @Size 2496 @Out UCODE2\VUNCLUT.BIN
		@File VV8TOV8.BIN @Size 522 @Out UCODE2\VV8TOV8.BIN
		@File VWAITLN.BIN @Size 792 @Out UCODE2\VWAITLN.BIN
		@File VWARP2D.BIN @Size 116 @Out UCODE2\VWARP2D.BIN
		@File KCOPY.BIN @Size 3266 @Out UCODE2\KCOPY.BIN
		@File VD080129.BIN @Size 18816 @Out UCODE2\VD080129.BIN
		@File VD080006.BIN @Size 28787 @Out UCODE2\VD080006.BIN
		@File 2105.BIN @Size 8448 @Out UCODE2\2105.BIN
		@File VE080129.BIN @Size 28453 @Out UCODE2\VE080129.BIN
		@File VD080200.BIN @Size 11676 @Out UCODE2\VD080200.BIN
		@File VD080020.BIN @Size 24615 @Out UCODE2\VD080020.BIN
		@File MCINIT.BCH @Size 3860 @Out UCODE2\MCINIT.BCH
		@File VK16.BIN @Size 2814 @Out UCODE2\VK16.BIN
		@File VK24.BIN @Size 2814 @Out UCODE2\VK24.BIN
		@File VD080021.BIN @Size 25777 @Out UCODE2\VD080021.BIN
		@File V15TO32.PA @Size 897 @Out UCODE\V15TO32.PA
		@File V16TO32.PA @Size 897 @Out UCODE\V16TO32.PA
		@File V32TO15.PA @Size 981 @Out UCODE\V32TO15.PA
		@File V32TO16.PA @Size 981 @Out UCODE\V32TO16.PA
		@File VBLEND.PA @Size 1548 @Out UCODE\VBLEND.PA
		@File VBLENDM.PA @Size 1978 @Out UCODE\VBLENDM.PA
		@File VCHECK.PA @Size 869 @Out UCODE\VCHECK.PA
		@File VCHECKA.PA @Size 869 @Out UCODE\VCHECKA.PA
		@File VCLEAR.PA @Size 584 @Out UCODE\VCLEAR.PA
		@File VCLUT.PA @Size 6281 @Out UCODE\VCLUT.PA
		@File VCOLOR.PA @Size 3226 @Out UCODE\VCOLOR.PA
		@File VCOPY.PA @Size 3619 @Out UCODE\VCOPY.PA
		@File VCOPYM.PA @Size 1182 @Out UCODE\VCOPYM.PA
		@File VCOPYMAP.PA @Size 1221 @Out UCODE\VCOPYMAP.PA
		@File VCOPYMSK.PA @Size 1567 @Out UCODE\VCOPYMSK.PA
		@File VCOPYPL.PA @Size 1277 @Out UCODE\VCOPYPL.PA
		@File VCOPYSK.PA @Size 1146 @Out UCODE\VCOPYSK.PA
		@File VD080003.PA @Size 20051 @Out UCODE\VD080003.PA
		@File VD080004.PA @Size 20051 @Out UCODE\VD080004.PA
		@File VD080005.PA @Size 20135 @Out UCODE\VD080005.PA
		@File VD080128.PA @Size 4749 @Out UCODE\VD080128.PA
		@File VD080192.PA @Size 5616 @Out UCODE\VD080192.PA
		@File VD080193.PA @Size 7672 @Out UCODE\VD080193.PA
		@File VD080194.PA @Size 5698 @Out UCODE\VD080194.PA
		@File VD080195.PA @Size 12292 @Out UCODE\VD080195.PA
		@File VD160001.PA @Size 1305 @Out UCODE\VD160001.PA
		@File VD160002.PA @Size 1641 @Out UCODE\VD160002.PA
		@File VDIFF.PA @Size 1130 @Out UCODE\VDIFF.PA
		@File VDIGIPL.PA @Size 1127 @Out UCODE\VDIGIPL.PA
		@File VDTOI16.PA @Size 1654 @Out UCODE\VDTOI16.PA
		@File VDTOV16.PA @Size 494 @Out UCODE\VDTOV16.PA
		@File VE080128.PA @Size 15590 @Out UCODE\VE080128.PA
		@File VE160001.PA @Size 4194 @Out UCODE\VE160001.PA
		@File VE160002.PA @Size 6350 @Out UCODE\VE160002.PA
		@File VE320192.PA @Size 5566 @Out UCODE\VE320192.PA
		@File VE320193.PA @Size 9514 @Out UCODE\VE320193.PA
		@File VE320194.PA @Size 3368 @Out UCODE\VE320194.PA
		@File VE320195.PA @Size 5160 @Out UCODE\VE320195.PA
		@File VE32A192.PA @Size 5846 @Out UCODE\VE32A192.PA
		@File VE32A193.PA @Size 9724 @Out UCODE\VE32A193.PA
		@File VEDGEFIX.PA @Size 2775 @Out UCODE\VEDGEFIX.PA
		@File VELLIPSE.PA @Size 3387 @Out UCODE\VELLIPSE.PA
		@File VFADE.PA @Size 2610 @Out UCODE\VFADE.PA
		@File VFILTER.PA @Size 3926 @Out UCODE\VFILTER.PA
		@File VFISH.PA @Size 3886 @Out UCODE\VFISH.PA
		@File VFISHSIZ.PA @Size 2731 @Out UCODE\VFISHSIZ.PA
		@File VFLOOD.PA @Size 2658 @Out UCODE\VFLOOD.PA
		@File VFLOODU.PA @Size 116 @Out UCODE\VFLOODU.PA
		@File VFLOODW.PA @Size 116 @Out UCODE\VFLOODW.PA
		@File VIDLE.PA @Size 578 @Out UCODE\VIDLE.PA
		@File VIMAGE.PA @Size 5962 @Out UCODE\VIMAGE.PA
		@File VINT.PA @Size 144 @Out UCODE\VINT.PA
		@File VINTERP.PA @Size 692 @Out UCODE\VINTERP.PA
		@File VISCALE.PA @Size 7106 @Out UCODE\VISCALE.PA
		@File VJUMP.PA @Size 228 @Out UCODE\VJUMP.PA
		@File VKTEXT8.PA @Size 2814 @Out UCODE\VKTEXT8.PA
		@File VLINE.PA @Size 1328 @Out UCODE\VLINE.PA
		@File VMIRROR.PA @Size 116 @Out UCODE\VMIRROR.PA
		@File VMOSAIC.PA @Size 1156 @Out UCODE\VMOSAIC.PA
		@File VPARM.PA @Size 536 @Out UCODE\VPARM.PA
		@File VPOLY.PA @Size 116 @Out UCODE\VPOLY.PA
		@File VPOLY2D.PA @Size 18492 @Out UCODE\VPOLY2D.PA
		@File VPOLY2DC.PA @Size 116 @Out UCODE\VPOLY2DC.PA
		@File VPOLY2DS.PA @Size 116 @Out UCODE\VPOLY2DS.PA
		@File VPOLY2DT.PA @Size 116 @Out UCODE\VPOLY2DT.PA
		@File VRANGE.PA @Size 1085 @Out UCODE\VRANGE.PA
		@File VRECT.PA @Size 1382 @Out UCODE\VRECT.PA
		@File VREPLAC2.PA @Size 2086 @Out UCODE\VREPLAC2.PA
		@File VREPLACE.PA @Size 1460 @Out UCODE\VREPLACE.PA
		@File VRETURN.PA @Size 522 @Out UCODE\VRETURN.PA
		@File VROUND.PA @Size 3187 @Out UCODE\VROUND.PA
		@File VSCALE.PA @Size 9206 @Out UCODE\VSCALE.PA
		@File VSKEW.PA @Size 1436 @Out UCODE\VSKEW.PA
		@File VSWITCH.PA @Size 696 @Out UCODE\VSWITCH.PA
		@File VTESTH.PA @Size 688 @Out UCODE\VTESTH.PA
		@File VTESTPC.PA @Size 2208 @Out UCODE\VTESTPC.PA
		@File VTESTV.PA @Size 1328 @Out UCODE\VTESTV.PA
		@File VTEXT1.PA @Size 1576 @Out UCODE\VTEXT1.PA
		@File VTEXT2.PA @Size 1648 @Out UCODE\VTEXT2.PA
		@File VUNCLUT.PA @Size 2314 @Out UCODE\VUNCLUT.PA
		@File VV8TOV8.PA @Size 536 @Out UCODE\VV8TOV8.PA
		@File VWAITLN.PA @Size 792 @Out UCODE\VWAITLN.PA
		@File VWARP2D.PA @Size 116 @Out UCODE\VWARP2D.PA
		@File VD080006.PA @Size 28549 @Out UCODE\VD080006.PA
		@File VK24.PA @Size 2814 @Out UCODE\VK24.PA
		@File VK16.PA @Size 2814 @Out UCODE\VK16.PA
		@File MCINIT.BCA @Size 3874 @Out UCODE\MCINIT.BCA
		@File VD080020.INT @Size 24405 @Out UCODE\VD080020.INT
		@File NWSAMP.AVS @Size 138224 @Out AV\NWSAMP.AVS
		@File NWAVDRV.SYS @Size 392 @Out BIN\NWAVDRV.SYS
		@File REGISTER.EXE @Size 44284 @Out BIN\REGISTER.EXE
		@File NWED.EXE @Size 9137 @Out BIN\NWED.EXE
		@File AVD1ATNT.EXE @Size 44699 @Out BIN\AVD1ATNT.EXE
		@File DS1SCSI.SYS @Size 15500 @Out BIN\DS1SCSI.SYS
		@File AVD1ATVG.EXE @Size 45773 @Out BIN\AVD1ATVG.EXE
		@File NWDSK.EXE @Size 8079 @Out BIN\NWDSK.EXE
		@File AVD2ATPL.EXE @Size 42001 @Out BIN\AVD2ATPL.EXE
		@File MFMDRVR.EXE @Size 20761 @Out BIN\MFMDRVR.EXE
		@File ADPDRVR.EXE @Size 22601 @Out BIN\ADPDRVR.EXE
		@File NPLAY.EXE @Size 54425 @Out BIN\NPLAY.EXE
		@File GRTST.EXE @Size 45215 @Out BIN\GRTST.EXE
		@File DS2VRAM.SYS @Size 6805 @Out BIN\DS2VRAM.SYS
		@File DS1VRAM.SYS @Size 5814 @Out BIN\DS1VRAM.SYS
		@File DSCDDRVR.EXE @Size 23403 @Out BIN\DSCDDRVR.EXE
		@File DS2DIAG.SYS @Size 8526 @Out BIN\DS2DIAG.SYS
		@File KEYON.EXE @Size 41543 @Out BIN\KEYON.EXE
		@File KEYOFF.EXE @Size 41543 @Out BIN\KEYOFF.EXE
		@File BRANDX.EXE @Size 13865 @Out BIN\BRANDX.EXE
		@File SLIDESHO.EXE @Size 52177 @Out BIN\SLIDESHO.EXE
	@EndLib
@EndDisk


@DefineDisk
	@Label = "Disk #2"

	@BeginLib NWOE.002
		@File SLIDESHO.EXE @Size 1 @AppendTo BIN\SLIDESHO.EXE
		@File DS2SCSI.SYS @Size 15492 @Out BIN\DS2SCSI.SYS
		@File ABIOSDVR.EXE @Size 29311 @Out BIN\ABIOSDVR.EXE
		@File AVD2ATNT.EXE @Size 48627 @Out BIN\AVD2ATNT.EXE
		@File AVD2ATVG.EXE @Size 49225 @Out BIN\AVD2ATVG.EXE
		@File AVD2AT42.EXE @Size 48637 @Out BIN\AVD2AT42.EXE
		@File NEWWORLD.PRO @Size 3322 @Out NEWWORLD.PRO
	@EndLib
@EndDisk



@SetConfig
	@AskOverwrite /* alternatively @DiskProto */
	@Device = "@OutDrive:\\@SubDir\\bin\\nwavdrv.sys"
	@Buffers = 20
	@Files = 20
/*
**	If the user wishes to use  the cd...
*/
	@If (1020 [= @Option)
		@If ( 3 [= @Option || 4 [= @Option)
			/* use DS1, or integrator driver */
			@Device = "@OutDrive:\\@SubDir\\bin\\ds1vram.sys @DefVWindow @DefVPort @DefIntlvl"
			@Device = "@OutDrive:\\@SubDir\\bin\\ds1scsi.sys"
		@ElseIf ( 5 [= @Option || 6 [= @Option || 7 [= @Option)
			/* use DS2 driver */
			@Device = "@OutDrive:\\@SubDir\\bin\\ds2vram.sys @DefVWindow @DefVPort @DefIntlvl @DefAIntLvl @DefSIntLvl"
			@Device = "@OutDrive:\\@SubDir\\bin\\ds2scsi.sys"
		@Endif
	@Endif

@EndConfig

@SetAutoexec
	@AskOverwrite /* alternatively @DiskProto */
	@Path = "@OutDrive:@Subdir\\bin"
	@Verbatim "set Nw=@OutDrive:\\@SubDir"
	@If (3 [= @Option)
		@Verbatim "@OutDrive:\\@SubDir\\bin\\AVD1ATNT"
	@ElseIf (4 [= @Option)
		@Verbatim "@OutDrive:\\@SubDir\\bin\\AVD1ATVG"
	@ElseIf (5 [= @Option || 10 [= @Option)
		@Verbatim "@OutDrive:\\@SubDir\\bin\\AVD2ATPL"
	@ElseIf (6 [= @Option || 8 [= @Option)
		@Verbatim "@OutDrive:\\@SubDir\\bin\\AVD2ATNT"
	@ElseIf (7 [= @Option || 9 [= @Option)
		@Verbatim "@OutDrive:\\@SubDir\\bin\\AVD2ATVG"
	@Endif

	@If (1000 [= @Option)
		/* install hard disk driver */
		@Verbatim "@OutDrive:\\@SubDir\\bin\\MFMDRVR @MFMDevice"
	@Endif


	@If (1010 [= @Option) 
		/* install the adaptec driver */
		@Verbatim "@OutDrive:\\@SubDir\\bin\\ADPDRVR @ADPDevice"
	@Endif

	@If (1020 [= @Option)
		@If (3 [= @Option || 4 [= @Option || 5 [= @Option ||
			 6 [= @Option  || 7 [= @Option)
			@Verbatim "@OutDrive:\\@SubDir\\bin\\DSCDDRVR"
		@Endif
	@Endif

	@If (2000 [= @Option) 
		/* install the abios driver */
		@Verbatim "@OutDrive:\\@SubDir\\bin\\ABIOSDVR @ABIOSDevice"
	@Endif

			
@EndAutoexec


@Finish
	@ChDrive @InDrive
	@ChDir "\\"
	@System "@OutDrive:\\@SubDir\\bin\\register"
	@System "@OutDrive:\\@SubDir\\bin\\brandx @OutDrive:\\@SubDir\\bin\\av*.exe"
	@System "del @OutDrive:\\@SubDir\\bin\\register.exe"
	@System "del @OutDrive:\\@SubDir\\bin\\brandx.exe"
	@ChDrive @OutDrive
	@ChDir "@SubDir"
	@System "copy newworld.pro newworld.ini >nul"
	@System "bin\\nwed newworld.ini \@DEFINTLVL\@ @DefIntlvl \@DEFPORT\@ @DefPort \@DEFWINDOW\@ @DefWindow"
	@System "bin\\nwed newworld.ini \@DRIVE\@ @OutDrive: \@DIR\@ @SubDir \@AUDCODE\@ @AudCode"
	@System "bin\\nwed newworld.ini \@DEFSINTLVL\@ @DefvSIntLvl \@DEFAINTLVL\@ @DefvAIntLvl"
	@System "bin\\nwed newworld.ini \@UCODE\@ @ucode"
	@System "del ucode\\*.bin"
	@System "del ucode\\*.bch"
	@System "ren ucode\\*.pa *.bin"
	@System "ren ucode\\*.bca *.bch"

	@If (3 [= @Option || 4 [= @Option || 5 [= @Option || 6 [= @Option  || 7 [= @Option)
		@System "bin\\nwdsk MfmDrvr @MFMDevice AdpDrvr @ADPDevice dscddrvr @CDDevice >>newworld.ini"
	@Endif

	@If (8 [= @Option  || 9 [= @Option || 10 [= @Option)
		@System "bin\\nwdsk AbiosDvr @ABIOSDevice >>newworld.ini"
	@Endif

	@Cls
	Installation is complete. Reboot you machine to allow the changes
	in config.sys and autoexec.bat to take affect.
	@Pause
@EndFinish
