
OS/2 2.1 Special Edition for Use with Windows Version 3.1 - INSTALLATION README
_______________________________________________________________________________

   Thank you for purchasing a copy of OS/2* 2.1 Special Edition.
   This product is designed for licensed users of Microsoft**
   Windows** Version 3.1 product.  After the installation of
   this product, your system will allow you to run DOS, Windows,
   and OS/2 applications.  Throughout the documentation provided
   with this product, all references to WIN-OS/2* apply to running
   your Windows Version 3.1 programs under the special edition.

     This document provides you with information
     you need before you install OS/2* 2.1 Special Edition.
     It contains helpful hints found in our testing
     as well as updates and corrections to the
     "OS/2 2.1 Installation Guide".

     Use the information in conjunction with the
     "OS/2 2.1 Installation Guide", the "OS/2 2.1
     Using the Operating System" manual, and the
     "OS/2 2.1 Special Edition for Use with Windows
     Version 3.1 Installation Guide".

     Do NOT install this product over OS/2 2.1.
     Installation of OS/2 2.1 Special Edition over
     OS/2 2.1 is not supported.

     Do NOT install OS/2 2.1 over this product.
     Installing OS/2 2.1 over OS/2 2.1 Special Edition
     is not supported.  If you install OS/2 2.1 over
     OS/2 2.1 Special Edition, you might lose the ability
     to use the Dual Boot or Boot Manager feature to
     start Windows Version 3.1.  You will need to
     re-install Windows Version 3.1, and you might need
     to re-install some of your Windows programs.

     The "OS/2 2.1 Special Edition for Use with Windows
     Version 3.1 Installation Guide" INCORRECTLY states
     that you cannot install OS/2 2.1 Special Edition over
     previous versions of OS/2.  You CAN install this product
     over previous versions of OS/2.  However, if you install
     this product over previous versions of OS/2 you must have
     Windows 3.1 installed on your system to run Windows
     applications.

     If you are installing OS/2 2.1 Special Edition over a
     product release such as OS/2 1.3, OS/2 2.0, OS/2 2.0
     with the Service Pak, DOS, or DOS and Windows**, it is
     recommended that you do not reformat the OS/2 partition.

     Do not install this product over Windows**
     for Work Groups.  Installing this product over
     Windows for Work Groups is not supported.

     To install OS/2 2.1 Special Edition, the original
     device drivers, fonts, and specific language information
     shipped with Windows 3.1 are required.
     You will use these files to update your Windows 3.1
     configuration to match your OS/2 configuration.
     Listed below is information to assist you.

       o   Some computer manufacturers ship Windows 3.1 diskettes
           with the computer.  Use those diskettes when requested
           during the installation process.

       o   Some computer manufacturers preinstall the Windows 3.1
           diskette images on the hard disk and provide authorization
           to use a utility to create the Windows 3.1 diskettes.  If
           you are authorized to do so, and you have not done so, create
           the Windows 3.1 diskettes and use those diskettes when
           requested during the installation process.

       o   Some computer manufacturers ship the Windows 3.1 device
           drivers on a directory on the hard disk.  The installation
           process will install the device drivers, fonts, and language
           specific information from that directory and you will not be
           prompted for diskettes.

       o   If you have an Ultimedia preinstalled system,
           or you installed Windows Version 3.1 from your
           Ultimedia System CD-ROM, do the following when
           prompted for the Windows Version 3.1 diskettes:

             1.  Insert the Ultimedia System CD-ROM into the drive.
             2.  Change to the directory containing Windows 3.1 on
                 your CD-ROM.
                 For example, type:

                         D:\WINSETUP

             3.  Continue with the installation process.

       o   If Windows 3.1 was installed from 3.5-inch diskettes, you
           must have the 3.5-inch Windows 3.1 diskettes.  If Windows 3.1
           was installed from 5.25-inch diskettes, you must have the
           5.25-inch Windows 3.1 diskettes.

       o   If you have updated the device drivers, fonts, or specific
           language information from those shipped on the Windows 3.1
           diskettes, or from those on your preinstalled system, you might
           be overwriting these files.

     If you are installing OS/2 2.1 Special Edition over an
     existing OS/2 2.0 system in which you have application
     programs on the desktop, you should not elect to migrate
     these applications during your installation.  Your
     current application set will continue to be available
     to you after installation.

     If you have a version of the OS/2 2.1 Special Edition beta
     installed, you need to reformat the OS/2
     partition.  Installing OS/2 2.1 Special Edition
     over a previous beta version is not supported.
     Do not use any OS/2 system files (such as
     OS2.INI or OS2SYS.INI) from a previous
     beta version.

   ****************IMPORTANT!*****************

     If you have a DOS or Windows Compression product installed
     before installing OS/2 2.1 Special Edition,
     check the documentation that came with your disk
     compression program to make sure it is compatible
     with the OS/2 operating system.  If the disk
     compression program is incompatible with the OS/2
     operating system, you will not be able to use the
     compressed drive while running OS/2 2.1 Special Edition,
     or the installation of OS/2 2.1 Special Edition
     might fail.

     If you have a DOS system with compression
     activated, do one of the following:

       1.  Decompress the disk where DOS and/or
           Windows Version 3.1 is installed.

       2.  Select a different partition to
           install OS/2 2.1 Special Edition.

       3.  Format the disk partition and reinstall
           DOS and Windows without compression.

     If you are installing OS/2 2.1 Special Edition on
     a non-Micro Channel (MCA) system, change the
     settings in your CMOS to the following:

       o   Turbo/System Speed should be OFF/Slow
       o   Caching (External) should be OFF
       o   ROM Shadowing (System and Video) should be OFF

     These settings affect the way that OS/2 2.1 Special Edition installs.
     Failure to change these settings might result in OS/2 2.1 Special Edition
     not installing at all; installing and then booting to a Trap 2;
     or what seems to be a good install and later having unexplainable
     random Traps (from a few days to a few months later).

     To improve system performance after you have installed
     this version of the OS/2 operating system, all of the
     above settings can be changed back without causing
     damage to OS/2 2.1 Special Edition.

   *******************************************

DOS 3.1 AND 3.2 USERS
_____________________

   DOS Versions 3.1 and 3.2 will create only one partition
   with a maximum size of 32MB.  If both DOS and
   Windows Version 3.1 are already in the partition,
   OS/2 2.1 Special Edition might not fit in the same partition.

   To solve this problem, allow OS/2 2.1 Special Edition
   to create additional partitions at installation time.
   A minimum of 20MB is required for the installation
   of OS/2 2.1 Special Edition.

   NOTE:  When you start from DOS, the partitions created
   with OS/2 2.1 Special Edition cannot be accessed.

DOS 3.3 USERS
_____________

   DOS Version 3.3 allows multiple partitions no larger than
   32MB.  Although OS/2 2.1 Special Edition allows partitions
   larger than 32MB, in order for DOS to access the contents
   of the partition, do not create a larger partition.  This
   allows DOS to access the contents of the partition.

   Also, for optimum performance, put DOS Version 3.3 and Windows
   Version 3.1 in one partition and OS/2 2.1 Special Edition
   in another partition.

SCSI-BASED CD-ROM SUPPORT
_________________________

   The majority of SCSI-based CD-ROM drives and
   adapters are supported by OS/2 2.1 Special Edition.
   ("SCSI-based" refers to the small computer
   system interface (SCSI), a standard
   input/output interface used by personal
   computers.)

   A complete list of the CD-ROM drives and SCSI
   adapters tested on OS/2 2.1 Special Edition
   can be found in the "Hardware Support"
   chapter of the "OS/2 2.1 Using the Operating System"
   manual.  (Note that Panasonic** MC521 support is not
   shipped with OS/2 2.1 Special Edition.  Please
   contact Panasonic to receive this support.)


OBTAINING ADDITIONAL CD-ROM SUPPORT

   If, after reviewing the list in "OS/2 2.1 Using
   the Operating System", you find that your
   CD-ROM drive or SCSI adapter is not supported
   within OS/2 2.1 Special Edition, you can contact the
   manufacturer and obtain an OS/2 Adapter Device
   Driver (.ADD) file.  After you receive the .ADD
   file, follow the instructions in the "Before
   You Begin" section of the "OS/2 2.1
   Installation Guide" to add this file to
   Diskette 1.

   As an alternative, you can create installation
   diskettes from the diskette images that are on
   the OS/2 2.1 Special Edition CD, if you have
   DOS support for your CD-ROM drive.

   If support for your CD-ROM was not properly
   installed during initial installation of
   OS/2 2.1 Special Edition, then you will need
   to use the Selective Install program located
   in the System Setup folder to reinstall the
   CD-ROM support appropriate for your CD-ROM.

CREATING DISKETTES FROM THE OS/2 2.1 SPECIAL EDITION CD

   You use the LOADDSKF utility program to create
   the diskettes.  (LOADDSKF.EXE is in the
   \DISKIMGS directory of the CD. LOADDSKF can be
   run from either the DOS or OS/2 operating
   system.)

   In the following sections, you will see lists
   of the product diskettes for OS/2 2.1 Special Edition
   and the actual diskette names as they exist on the CD.
   For each diskette image file, use LOADDSKF to
   expand the image to its own diskette.  (Note
   that you must use formatted diskettes for this
   procedure.)

   For example:

      cddrive:\DISKIMGS\LOADDSKF cddrive:\DISKIMGS\OS2\size\disk_name b:

   where:

       cddrive is the drive letter of the CD-ROM

       size is 35 for 3.5-inch diskettes or 525
       for 5.25-inch diskettes

       disk_name is the diskette image file name
       (for example, DISK0.DSK, PMDD1.DSK.)

       b is the drive letter of your diskette
       drive (A: or B:)

   After you create all the diskettes (16 for
   3.5-inch diskettes or 19 for 5.25-inch
   diskettes), insert the DISK0 diskette in drive
   A:, restart your system, and follow the
   instructions to install OS/2 2.1 Special Edition.


List of 3.5-Inch Diskette Images


   DISKIMGS\OS2\35\DISK0.DSK -- INSTALLATION Diskette
   DISKIMGS\OS2\35\DISK1.DSK -- Diskette 1 of 11
   DISKIMGS\OS2\35\DISK2.DSK -- Diskette 2 of 11
   DISKIMGS\OS2\35\DISK3.DSK -- Diskette 3 of 11
   DISKIMGS\OS2\35\DISK4.DSK -- Diskette 4 of 11
   DISKIMGS\OS2\35\DISK5.DSK -- Diskette 5 of 11
   DISKIMGS\OS2\35\DISK6.DSK -- Diskette 6 of 11
   DISKIMGS\OS2\35\DISK7.DSK -- Diskette 7 of 11
   DISKIMGS\OS2\35\DISK8.DSK -- Diskette 8 of 11
   DISKIMGS\OS2\35\DISK9.DSK -- Diskette 9 of 11
   DISKIMGS\OS2\35\DISK10.DSK -- Diskette 10 of 11
   DISKIMGS\OS2\35\DISK11.DSK -- Diskette 11 of 11
   DISKIMGS\OS2\35\PMDD1.DSK --  Printer Drivers Diskette 1 of 2
   DISKIMGS\OS2\35\PMDD2.DSK --  Printer Drivers Diskette 2 of 2
   DISKIMGS\OS2\35\DISP1.DSK --  Display Drivers Diskette 1 of 2
   DISKIMGS\OS2\35\DISP2.DSK --  Display Drivers Diskette 2 of 2


List of 5.25-Inch Diskette Images

   DISKIMGS\OS2\525\DISK0.DSK - INSTALLATION Diskette
   DISKIMGS\OS2\525\DISK1.DSK - Diskette 1 of 13
   DISKIMGS\OS2\525\DISK2.DSK - Diskette 2 of 13
   DISKIMGS\OS2\525\DISK3.DSK - Diskette 3 of 13
   DISKIMGS\OS2\525\DISK4.DSK - Diskette 4 of 13
   DISKIMGS\OS2\525\DISK5.DSK - Diskette 5 of 13
   DISKIMGS\OS2\525\DISK6.DSK - Diskette 6 of 13
   DISKIMGS\OS2\525\DISK7.DSK - Diskette 7 of 13
   DISKIMGS\OS2\525\DISK8.DSK - Diskette 8 of 13
   DISKIMGS\OS2\525\DISK9.DSK - Diskette 9 of 13
   DISKIMGS\OS2\525\DISK10.DSK - Diskette 10 of 13
   DISKIMGS\OS2\525\DISK11.DSK - Diskette 11 of 13
   DISKIMGS\OS2\525\DISK12.DSK - Diskette 12 of 13
   DISKIMGS\OS2\525\DISK13.DSK - Diskette 13 of 13
   DISKIMGS\OS2\525\PMDD1.DSK -  Printer Drivers Diskette 1 of 2
   DISKIMGS\OS2\525\PMDD2.DSK -  Printer Drivers Diskette 2 of 2
   DISKIMGS\OS2\525\DISP1.DSK -  Display Drivers Diskette 1 of 2
   DISKIMGS\OS2\525\DISP2.DSK -  Display Drivers Diskette 2 of 2

   If you want to create diskettes for the
   Multimedia support that is part of OS/2 2.1 Special Edition,
   note that the images are located in the
   \DISKIMGS\MMPM2 directory. Use LOADDSKF to
   expand each image to its own diskette.  For
   example:

       cddrive:\DISKIMGS\LOADDSKF cddrive:\DISKIMGS\MMPM2\size\disk_name b:

   where:

       cddrive is the drive letter of the CD-ROM

       size is 35 for 3.5-inch diskettes or 525
       for 5.25-inch diskettes

       disk_name is the diskette image file name
       (for example, DISK1.DSK)

       b is the drive letter of your diskette
       drive (A: or B:)

   NOTE: Use previously formatted diskettes for
   the target (b:).


List of 3.5-Inch Multimedia Diskette Images

   DISKIMGS\MMPM2\35\DISK1.DSK - Diskette 1 of 2
   DISKIMGS\MMPM2\35\DISK2.DSK - Diskette 2 of 2


List of 5.25-Inch Multimedia Diskette Images

   DISKIMGS\MMPM2\525\DISK1.DSK - Diskette 1 of 3
   DISKIMGS\MMPM2\525\DISK2.DSK - Diskette 2 of 3
   DISKIMGS\MMPM2\525\DISK3.DSK-  Diskette 3 of 3

   When you do a selective install to update your system
   from VGA to SVGA, your system attempts to write to the
   CD-ROM.  Therefore, you must create the diskette images
   for the display drivers before performing the selective
   install.

HARDWARE CONSIDERATIONS
_______________________

   If you have a Quantum hard card, you must make
   a modification to the BASEDEV=IBM1S506.ADD line
   in the CONFIG.SYS file of Diskette 1 before you
   install OS/2 2.1 Special Edition.  The BASEDEV
   statement should be modified as follows:

       BASEDEV=IBM1S506.ADD /A:1 /IRQ:11

   (These are the default settings for the Quantum
   hard card.)

   If you have added a device driver statement to
   the CONFIG.SYS file on diskette 1 and later
   migrate your old CONFIG.SYS file, make sure
   there are not two copies of this statement in
   your file.  If you have two copies of this
   statement in your file, REM one statement out.

   If you have a Logitech** TrackMan**, select one
   of the two Logitech mouse choices during
   installation.


INSTALLING OS/2 2.1 SPECIAL EDITION FROM A CD ON
AN IBM THINKPAD ATTACHED TO A DOCKING STATION
________________________________________________

   If you are installing OS/2 2.1 Special Edition on an IBM*
   ThinkPad* 700, 700C, 720, or 720C attached to a
   3550 Docking Station, you need to replace the
   ABIOS files on the OS/2 Installation Diskette
   with files from the Reference Diskette.  Do the
   following:

       1.  Detach the ThinkPad from the Docking
           Station.

       2.  Create a Reference Diskette (if you have
           not already done so) by following the
           documentation that came with the ThinkPad.

       3.  Make a copy of the OS/2 Installation
           Diskette.

       4.  Insert the original OS/2 Installation
           Diskette into drive A.

       5.  Turn on the computer.  If it is already on,
           press Ctrl+Alt+Del.

       6.  When you are prompted to do so, remove the
           Installation Diskette, insert Diskette 1,
           and press Enter.

       7.  When the Welcome screen is displayed, press
           Esc to display the command prompt.

       8.  Insert the copy of the Installation
           Diskette into drive A.

       9.  Type:

                 DEL *.BIO

           and press Enter.

      10.  Remove the copy of the Installation
           Diskette, and insert the Reference Diskette
           you created in step 2 into drive A.

      11.  If your computer has more than one diskette
           drive, insert the copy of the Installation
           Diskette into drive B.  Otherwise, in the
           next two steps, you will be prompted to
           insert diskettes into both drive A and
           drive B.  When you are asked to insert a
           diskette into drive A, insert the Reference
           Diskette.  When you are asked to insert a
           diskette into drive B, insert the copy of
           the Installation Diskette.

      12.  Type:

                 COPY A:\*.BIO B:\

           and press Enter.

      13.  Type:

                 COPY A:\ABIOS.SYS B:\

           and press Enter.

      14.  Power off the ThinkPad and return it to the
           Docking Station.

      15.  Restart the installation procedure by
           inserting the copy of the Installation
           Diskette into drive A.


INSTALLING OS/2 2.1 SPECIAL EDITION USING RIPL
______________________________________________

   When installing OS/2 2.1 Special Edition using the IBM LAN
   Server 3.0 Remote Installation Program Load (RIPL), the
   OS/2 2.1 Special Edition version of RIPLINST.EXE is dependent
   upon the OS/2 2.1 Special Edition version of UNPACK.EXE.
   Therefore, if you are using the OS/2 2.1 Special Edition version
   of RIPLINST.EXE on a client machine with OS/2 version 2.0 or lower,
   then you must copy the UNPACK.EXE file to the client machine.  To do
   this, do the following:

       1.  Insert OS/2 2.1 Special Edition Diskette 2 into drive A

       2.  At an OS/2 command prompt type:

               copy a:\unpack.exe \os2\unpack.exe

       After copying the file to the client machine, you can now
       execute the OS/2 2.1 Special Edition version of the
       RIPLINST.EXE program.

       o   When installing IC06163 to a LAN Server supporting
           Remote IPL (RIPL), you must first obtain a special
           utility package from the IBM Service and Support
           Center.  To obtain this tool, you must request
           the LAN SERVER RIPL package for IC06163.


VIDEO CONSIDERATIONS
____________________

   The following information pertains to video
   support for OS/2 2.1 Special Edition.


INSTALLING SUPER VGA (SVGA) SUPPORT

   After the VGA installation is complete, follow
   the procedure "Changing Your Setup or Adding
   Features" in Appendix A of the "OS/2 2.1
   Installation Guide".


INSTALLING S3 SUPER VGA (SVGA) SUPPORT

   For more information on how to install S3** SVGA support,
   refer to the S3 README.

CID INSTALL UPDATE FOR S3 256 COLOR DISPLAY DRIVERS

   If you want to install the S3 256 color display driver
   using CID installation, add the following statements to
   your LCU command file.  The following information provides
   a guide to help you update your LCU command file.

   /*****************************************************/
   /*               PRODUCT DATA SECTION                */
   /*****************************************************/

                         .
                         .
                         .

   x.s3video256 = 15
   x.15.name='S3 Video 256 color'
   x.15.statevar = 'CAS_' || x.15.name
   x.15.instprog = 'x:\img\s3_256\S3INST.CMD',
                   ' x:\img\s3_256 ' || bootdrive
   x.15.rspdir   = ''
   x.15.default  = ''

   =======================================================
   S3INST.cmd needs to be modified before it can by used.
   Use a text editor to REM out the PAUSE statement.
   =======================================================

   /*---------------------------------------------------*/
   /*         NUMBER OF PROGRAMS SET UP IN THE          */
   /*               PRODUCT DATA SECTION                */
   /*---------------------------------------------------*/

   NUM_INSTALL_PROGS = 15

   /*****************************************************/
   /*                  INSTALL SECTION                  */
   /*****************************************************/
                         .
                         .
                         .

       when OVERALL_STATE = 2 then do
         if RunInstall(x.s3video256) == BAD_RC then exit
         Call CheckBoot
       end
                         .
                         .
                         .

   end
   exit


INSTALLATION ON SPECIFIC VIDEO ADAPTERS

   In the "OS/2 2.1 Installation Guide",
   instructions are given for configuring the
   ATI** Graphics Ultra Pro.  These instructions
   state that the monitor type for 640 x 480 must
   be configured to IBM DEFAULT.  Note that this
   setting might be referred to as 60Hz rather
   than IBM DEFAULT.

   The Radius XGA display adapter is supported on
   PS/2* Models 35 and 40 and PS/ValuePoint* 486
   systems.  If you are using the display adapter
   on a PS/ValuePoint system, the VPXGA.EXE
   utility is required.  For a copy of this
   utility program, check your Radius installation
   diskette or contact Radius.

   The OS/2 2.1 Special Edition operating system cannot
   restore the state of a Sigma Legend** display adapter
   after you switch sessions or video modes.
   Also, the Sigma Legend video adapter might
   cause the system to stop when using 1024 x 768
   x 256 color mode.  Use only 640 x 480 or 800 x
   600 mode with this adapter.


CORRECTION TO INSTALLATION GUIDE APPENDIX B
___________________________________________

   Appendix B of the "OS/2 2.1 Installation Guide"
   presents information on how to respond to
   messages that begin with "TRAP".  The
   information in the appendix pertains only to
   TRAP0002 messages.



EXTENDED SERVICES (ES) 1.0
__________________________

       o   If you installed OS/2 2.1 Special Edition
           on a system that already had Extended Services
           installed, you need to replace the existing
           ESSTART.CMD file with the ESSTART.BAK file that was
           installed by OS/2 2.1 Special Edition.  (The ESSTART.BAK
           file is located in the OS2\INSTALL subdirectory.)
           First rename ESSTART.CMD to ESSTART.OLD.
           Then rename ESSTART.BAK to ESSTART.CMD.

       o   If you are installing Extended Services
           over OS/2 2.1 Special Edition for the first
           time (that is, there is no Extended Services
           on the workstation), or if you are installing
           Extended Services from diskettes, rename
           the existing ESSTART.CMD file from the
           Extended Services Diskette 1.  Then, copy
           the file ESSTART.BAK from the \OS\INSTALL
           directory to Extended Services Diskette 1.
           Finally, rename the ESSTART.BAK file
           ESSTART.CMD, and begin the installation of
           Extended Services.



NOTICES AND TRADEMARKS
__________

   If you want to run Windows programs on the OS/2 desktop, with
   OS/2 2.1 Special Edition, you agree that you are a current
   licensee of Microsoft Windows Version 3.1 software.  You also
   agree to abide by all the conditions of the Microsoft Windows
   Version 3.1 license agreement.

   In order for OS/2 2.1 Special Edition to work properly,
   you need to have the original copies of Windows Version 3.1
   files on your system.  During installation you will be
   prompted for your original Windows diskettes.  This process
   replaces any modified code from your original copy of
   Windows, leaving you with one and only one copy of Windows on
   your system.  If you have changed any of your Windows file names
   or have made any additional unauthorized copies, you must dispose
   of them accordingly, leaving you one copy of Windows on your hard
   file.

   Your Windows system configuration will be updated to
   match your selected OS/2 2.1 system configuration.
   As a result of this update, your existing Windows
   device drivers might be overwritten.
   Also, if you install any other manufacturer's
   enhanced device drivers on your system, they might
   be overwritten.  Be sure to verify with the license
   agreement that came with the other manufacturer's
   device driver that it can be used with OS/2 Special Edition.

   The following terms, denoted by an asterisk (*)
   in this README, are trademarks or registered
   trademarks of the IBM Corporation in the United
   States or other countries:

    IBM
   -----------------------------------------------
    OS/2
   -----------------------------------------------
    PS/2
   -----------------------------------------------
    PS/ValuePoint
   -----------------------------------------------
    ThinkPad
   -----------------------------------------------
    XGA
   -----------------------------------------------

   The following terms, denoted by a double
   asterisk (**) in this README, are trademarks of
   other companies as follows:


    Trademark:            Owner:
   --------------------------------------------------------------
    Adaptec               Adaptec, Inc.
   --------------------------------------------------------------
    ATI                   ATI Technologies, Inc.
   --------------------------------------------------------------
    Legend                Sigma Designs Inc.
   --------------------------------------------------------------
    Logitech              Logitech, Inc.
   --------------------------------------------------------------
    Panasonic             Matsushita Electric Industrial Co., Ltd.
   --------------------------------------------------------------
    S3                    S3 Incorporated
   --------------------------------------------------------------
    TrackMan              Logitech, Inc.
   --------------------------------------------------------------
    Windows               Microsoft Corporation
   --------------------------------------------------------------

   IBM DISCLAIMS ALL WARRANTIES, WHETHER EXPRESSED
   OR IMPLIED, INCLUDING WITHOUT LIMITATION,
   WARRANTIES OF FITNESS AND MERCHANTABILITY WITH
   RESPECT TO THE INFORMATION IN THIS DOCUMENT.
   BY FURNISHING THIS DOCUMENT, IBM GRANTS NO
   LICENSES TO ANY RELATED PATENTS OR COPYRIGHTS.

   Copyright IBM Corporation, 1993, all rights
   reserved.
