USING 16-BIT VGA CARDS
======================

 Some 16-bit VGA cards can cause upper memory block conflicts that
 result in a NO HOST ADAPTER FOUND error. This is a problem with 
 some 16-bit cards and 8-bit memory-mapped cards, and is not specific 
 to CorelSCSI.

 To eliminate the conflict, you can

 - set the memory address on your card to E000 if your computer 
   allows cards to use memory above E000

 - use your VGA card in 8-bit mode. For instructions about how to
   use your card in 8-bit mode, see the user manual for your 
   16-bit VGA card.
