NOTICE TO MEMORY MANAGER USERS
==============================

 If you're using memory managers, you must exclude the SCSI card 
 address in the CONFIG.SYS file. Excluding the SCSI card address
 range prevents address conflicts between the memory manager and
 the SCSI card.

 For example, if you're using the QEMM memory manager and
 a SCSI card that covers the address range from d800 to dbff,
 you would specify the following in your CONFIG.SYS file:

      DEVICE=C:\QEMM\QEMM386.SYS x=d800-dbff
 
 If you're using the EMM386 memory manager and
 a SCSI card that covers the address range from d800 to dbff,
 you would specify the following in your CONFIG.SYS file:

      DEVICE=C:\EMM386\EMM386.SYS x=d800-dbff

 If you're using the 386MAX memory manager and
 a SCSI card that covers the address range from d800 to dbff,
 you would specify the following in your CONFIG.SYS file:

      DEVICE=C:\386MAX\386MAX.SYS RAM=d800-dc00
