NOTICE TO DR-DOS USERS
======================

 Prior to DOS version 4, you were limited to cartridge partition
 sizes of 32 MB or less. For example, if you used a 1 GB rewritable
 cartridge, you were required to divide it into several smaller 
 partitions. To resolve this problem, CorelSCSI provided a "patch"
 program. A patch lets DOS recognize a partition size larger than
 32 MB. Most users won't need to use the patch program. 
 
 If you're using DR-DOS 5 or 6, your operating system automatically
 adjusts to different physical sector sizes. However, if you have 
 cartridges formatted under DOS version 3.x or earlier, you can 
 read them only if they were formatted with a power of two sector
 size; for example, 2048, 4096, 8192, or 16384 bytes.
