INSTALLING CORELSCSI WINDOWS UTILITIES 
======================================

 The CorelSCSI Windows utilities section (on page 27), in the 
 CorelSCSI "Installation Manual" refers to INSTALL.EXE. However,
 INSTALL.EXE has been renamed to SETUP.EXE.
 
 To install the CorelSCSI Windows utilities, you must Run SETUP.EXE 
 from the installation diskette.

 Note: To use the CorelSCSI Windows utilities, you must have Run
       INSTALL.EXE from DOS first. Doing so would install the 
       CD-ROM device driver and DOS CD-ROM utilities.

FOR MICROSOFT WINDOWS 3.0 USERS 
-------------------------------

 For best performance with CorelSCSI, use standard or enhanced mode.
 If you use Microsoft Windows in real mode while running CDAUDIO or
 the installation, you may experience problems caused by insufficient 
 memory.

 If you experience memory problems

 1. Copy the !WIN_UTL.LZH and LHARC.EXE from the installation diskette
    to your hard disk.

 2. From the hard disk sub-directory, type LHARC X !WIN_UTL.LZH
    (This will extract CDINST.EXE & CDINST.INF from the archive).

 3. Run CDINST from your hard disk instead of typing A:SETUP.
