* :title.IBM LAN Server 3.0 ServicePak - IP07045 U.S.  
*************************************************************************
*  The files contained in this package are for use only by licensed     *
*  users of LAN Server 3.0 and may be applied only to machines for      *
*  which a LAN Server 3.0 Entry Server, LAN Server 3.0 Advanced Server, *
*  or a LAN Server Distributed Client Feature license is held.  Using   *
*  the files for any purpose other than providing service to LAN Server *
*  3.0 is unlawful.                                                     *
*************************************************************************
* This ServicePak is cumulative and will bring LS 3.0 users that
* are at Golden code IP07000, or at a service level of IP07001, IP07003,
* or IP07005, to the same level of fixes and enhancements as the refresh
* of LS 3.0.1.  It also includes fixes for RIPL past the refresh level.
* The LAN Server, LAN Requester, UPM, RIPL, Fault Tolerance, and the
* DOS LAN Requester (DLR) components of LS 3.0 are serviced as well as
* Providing service for the LAN Support Program v1.35 (LSP).
* (CAUTION; THE LSP IMAGE - Image numbers 7 and 8 of the 5.25" images should
* be created on 5.25 - inch low capacity diskettes 360KB).
* (CAUTION; THE LSP IMAGE - Image number 6 of the 3.5" images should be
* created on 3.50-inch low capacity diskettes 720KB).
* The WR07045 ServicePak/Refresh for NTS/2 is required for this package,
* and may be requested from this BBS.
* A list of the APAR's fixed may be viewed in the IP07045.INF, as well
* as interesting information regarding the ServicePak, and installation.
* Read LSESSERV.TXT for information on current, or upcoming service for
* LAN Server, Extended Services, and other PSP products.
****************************************************************************
