InS_StArT
TCE16ATW.COM
1.0
^Thomas-Conrad TC5045 Ethernet adapter,TCE16ATW.COM,IE0
?Select the options that match your adapter's settings.
!RIE0(PORT) Base I/O Address
?If an address is not selected, the driver will load the default address of 300h.
100
120
140
160
@300
320
340
*OIE0(FRAME) Frame Type
?If a frame type is not selected, the driver defaults to Ethernet 802.2. Ethernet_II, Ethernet_802.3, and Ethernet_SNAP are also available.
@Ethernet_802.2
Ethernet_II
Ethernet_802.3
Ethernet_SNAP
$OIE0(NODE ADDRESS) Node Address
?Select "None" unless you want to set a locally administered node ID in the range shown below.
008013000000
008013FFFFFF
InS_EnD
