InS_StArT
TRXNET.COM
1.0
^Novell RX-Net & RX-Net II,TRXNET.COM,IE0
^Novell RX-Net/2,TRXNET.COM,00M,6014
?Microchannel machines with a \"Preempt\" option should have the option set to DISABLED; otherwise, the system bus may hang.
!RIE0(INT)Hardware Interrupt
3
4
5
7
@2
10
!RIE0(PORT)Base I/O Port
?The default I/O port setting 2E0 may conflict with some VGA cards.
@2E0
2F0
300
310
350
200
250
2A0
3E0
!RIE0(MEM)Base Memory Address
@D0000
C0000
E0000
CC000
DC000
C4000
C8000
D4000
D8000
!R00M(SLOT)Slot
1
2
3
4
5
6
7
8
*RIEM(FRAME)Frame Type
?For IP, need to select NOVELL_RX-NET frame type.  IPX requires none.
@NOVELL_RX-NET
InS_EnD
