InS_StArT
SMC8100.COM
1.0
^SMC Token Ring EliteFamily Adapter,SMC8100.COM,IEM
?Select the options that match your board's settings.
!RIE0(PORT) I/O Base Port
200
220
240
260
@280
2A0
2C0
2E0
300
320
340
360
380
3A0
3C0
3E0
!R00M(SLOT) Microchannel Slot
1
2
3
4
5
6
7
8
!OIE0(INT) Hardware Interrupt
2
@3
4
5
7
10
11
14
15
!OIE0(MEM) Memory Base
c0000
c4000
c8000
cc000
@d0000
d4000
d8000
dc000
e0000
e4000
e8000
ec000
!OIEM(NODE ADDRESS) Override Node Address
0
7FFFFFFFFFFF
*RIEM(FRAME)Frame Type
@TOKEN-RING
TOKEN-RING_SNAP
InS_EnD

