InS_StArT
UBODI.COM
1.0
^Ungermann-Bass NIUpc/EOTP,UBODI.COM,IE0
^Ungermann-Bass NIUps,UBODI.COM,00M,7012
^Ungermann-Bass NIUpc,UBODI.COM,IE0
^Ungermann-Bass Personal NIU/ex,UBODI.COM,IE0
^Ungermann-Bass Personal NIU,UBODI.COM,IE0
!RIE0(ADAPTERTYPE) Adapter Type
?Specify the type of Ungermann-Bass adapter you have installed.
@NIUpc/EOTP
NIUpc
Personal NIU/ex
Personal NIU
!RIE0(INT) Interrupt Request Level
?Specify the IRQ level corresponding to the jumper settings. NIUpc/EOTP: IRQ 3,12. NIUpc & Personal NIU/ex: IRQ 2,3,4,5. Personal NIU: IRQ 2,5.
2
@3
4
5
12
!RIE0(PORT) I/O Base Address
?Specify the I/O base address corresponding to the jumper settings.  NIUpc/EOTP & NIUpc: 350,358,360,368. Personal NIU & Personal NIU/ex: 360,368.
@350
358
360
368
!RIE0(MEM) Memory Base Address
?Specify the memory base address corresponding to the jumper settings.
C0000
C8000
D0000
@D8000
B0000
B8000
!O00M(SLOT) PS/2 Card Slot
1
2
3
4
5
6
7
8
*RIEM(FRAME) Frame type
?Note: Ethernet_802.2 is now the default frame type for ODI drivers. If you use a NetWare v2.2, select the 802.3 frame type.
ETHERNET_802.3
@ETHERNET_802.2
ETHERNET_SNAP
ETHERNET_II
InS_EnD
