InS_StArT
T30ODI.COM
1.0
^Cabletron Systems Token-Ring T30,T30ODI.COM,00M,0050
?Select the options you will use.
!R00M(SLOT) Slot Number
?Note: If you don't select a slot number, the first T3015 board found will be used.
1
2
3
4
5
6
7
8
!O00M(SOURCE ROUTING) Source Routing
?The Cabletron token-ring drivers have built-in source routing abilities.  Use either the built-in source routing abilities or ROUTE.COM.
@OFF
ON
$O00M(NODE ADDRESS) Node Address
400000000000
7FFFFFFFFFFF
*R00M(FRAME) Frame Type
@TOKEN-RING
TOKEN-RING_SNAP
InS_EnD
