InS_StArT
TCE16MCW.COM
1.0
^Thomas-Conrad TC5046 Ethernet adapter,TCE16MCW.COM,00M
?Select the options that match your adapter's settings.
!R00M(SLOT) Slot
?If a slot is not selected, the driver will check the configuration for a slot number.
1
2
3
4
5
6
7
8
*O00M(FRAME) Frame Type
?If a frame type is not selected, the driver defaults to Ethernet 802.2. Ethernet_II, Ethernet_802.3, and Ethernet_SNAP are also available.
@Ethernet_802.2
Ethernet_II
Ethernet_802.3
Ethernet_SNAP
$OIE0(NODE ADDRESS) Node Address
?Select "None" unless you want to set a locally administered node ID in the range shown below.
008013000000
008013FFFFFF
InS_EnD
