You have just installed PowerChute Plus for OS/2. 
The following items have been changed on your OS/2 
system:

	All the PowerChute files have been copied to 
	your hard drive in the specified directory.

	The CONFIG.SYS was modified to add the Pwrchute 
	directory to the LIBPATH line.

	The variable PWRCHUTE=DRIVE:\PATH was also 
	added to the CONFIG.SYS.

	The file STARTUP.CMD was modified/created 
	to auto start UPSD.EXE.


In LAN installations:

	PowerChute modified the LAN.INI file to 
	comment out the UPS section.

The UPS service routine path was modified to point to 
the PowerChute install path.


Stand Alone OS/2:

	Ensure that UPSD is the first command in 
	the STARTUP.CMD file.

	Reboot the OS/2 system. 

	When the system restarts, ensure UPSD.EXE is 
	started and communication is established.

LAN Installations:

	Ensure that UPSD is in the STARTUP.CMD BEFORE 
	the NET START REQ/SERVER lines. UPSD must 
	be started before the REQ and UPS service.

	If you are running PowerChute on more than 
	one server in your network, refer to the 
	PowerChute manual to add a PWRCHUTE account, 
	and Named pipe to your domain.

	When starting the PowerChute interface screen 
	in a Domain with other PowerChute servers, not 
	all system may appear in the "Select  Server" dialog
	upon startup.
	If the server you wish to connect to is not in 
	the list, ensure that UPSD is running on that system. 
	If so, simply cancel out of the "Select Sever" box, and 
	choose "MONITOR DIFFERENT SERVER". This 
	will give the LAN enough time to gather all the 
	available servers.

APC 24 HOUR TECH SUPPORT 
1-800-800-4272
