      -----------------------------------------------------------------
      STACKER NOTE                                         STACKER NOTE
                         PKZIP 2.04 AND STACKER 4.0
                          (Applies to Stacker 4.0)
      STAC FAX  4510 (03-03-1994)
      -----------------------------------------------------------------
                                      
                                      
      BACKGROUND
      
      You may experience difficulty using PKZIP 2.04 and Stacker 4.0 if
      you have a '386 or better computer, have at least 1MB of RAM, and
      are using pre-loaded compression (DOS 6 or higher). The
      difficulty is caused by the way in which PKZIP uses DPMI
      services. Use the -) option on the command line when using PKZIP.
      If you wish to permanently disable PKZIP's use of DPMI, use this
      option in your PKZIP.CFG file. See your PKZIP documentation
      regarding making changes to the PKZIP.CFG file.
      -----------------------------------------------------------------
      Copyright 1994 Stac Electronics
