; Megahertz 2400-9600 (assorted internal and external models)

;=============================================================
; Last revision date: 02/18/93 (update this date
; each time you edit; it is also advisable to rename
; your edited file [use Save As, rather than Save 
; option] to avoid later confusion and to keep the 
; original .MDM file intact).

; NOTE: Refer to the file TEMPLATE.MDM (A Sample Modem 
; Command File) for a description of modem command 
; files and how they work. "A Sample Modem Command 
; File" is user selectable within the Lotus Notes 
; Setup dialog "Modem Type" listbox in which you found 
; this modem command file (see end of listings, 
; beginning with a period) and is a printable ASCII 
; text file (approximately 15 pages). 

; Additional information may be obtained from either of 
; the two so-called "generic" modem command files 
; (alphabetically listed under letter G, designed for 
; use with Notes Releases 2.x and 3.x, 9600 bps and 
; 14400 bps maximum, respectively), each of which may 
; first be tried as-is with unlisted modems, then edited 
; if required (within the Notes edit box, or outside of 
; Notes, with any text editor) according to the printed 
; instructions within each file, and in compliance with 
; the vendor's command set, result codes, DIP switch 
; settings, and technical specifications as listed in 
; the equipment's users manual.

; For the specific modem(s) listed under this heading:
;===============================================================

; NOTE: This modem accepts command strings of 60 or fewer 
; characters.  After an "AT," commands must be continuous, 
; not separated by spaces.

[attributes]

MODELS=Megahertz 2400-9600 (assorted models)
NULL MODEM =0
MAXIMUM SPEED=38400
DEFAULT SPEED=38400

[commands]

ESCAPE=+++
ATTENTION=ATE0V1
HANGUP=ATH0
SETUP=AT&F
SETUP=ATE0V1
SETUP=AT&C1&D2\\G0\\N7S0=0S7=60X4\\V2\\J0
RTS/CTS ENABLED=AT\\Q3
RTS/CTS IGNORED=AT\\Q0
VOLUME OFF=ATM0
VOLUME LOW=ATM1L1
VOLUME MEDIUM=ATM1L2
VOLUME HIGH=ATM1L3
ANSWER=ATA
MANUAL DIAL=ATX3S9=1D
AUTO DIAL SETUP=ATS9=6
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,

[responses]

OK=OK

RING=RING

NO CARRIER=NO CARRIER

ERROR=ERROR

NO DIALTONE=NO DIALTONE
NO DIALTONE=NO DIAL TONE

BUSY=BUSY

NO ANSWER=NO ANSWER

CONNECT,38400,9600=CONNECT 9600
CONNECT,38400,9600=CONNECT 9600/REL
CONNECT,38400,9600=CONNECT 9600/REL-MNP
CONNECT,38400,9600=CONNECT 9600/REL-MNP-COMP
CONNECT,38400,9600=CONNECT 9600/REL-LAPM
CONNECT,38400,9600=CONNECT 9600/REL-LAPM-COMP
CONNECT,38400,9600=CONNECT 9600/REL-V.42
CONNECT,38400,9600=CONNECT 9600/REL-V.42-COMP

CONNECT,38400,4800=CONNECT 4800
CONNECT,38400,4800=CONNECT 4800/REL
CONNECT,38400,4800=CONNECT 4800/REL-MNP
CONNECT,38400,4800=CONNECT 4800/REL-MNP-COMP
CONNECT,38400,4800=CONNECT 4800/REL-LAPM
CONNECT,38400,4800=CONNECT 4800/REL-LAPM-COMP
CONNECT,38400,4800=CONNECT 4800/REL-V.42
CONNECT,38400,4800=CONNECT 4800/REL-V.42-COMP

CONNECT,38400,2400=CONNECT 2400
CONNECT,38400,2400=CONNECT 2400/REL
CONNECT,38400,2400=CONNECT 2400/REL-MNP
CONNECT,38400,2400=CONNECT 2400/REL-MNP-COMP
CONNECT,38400,2400=CONNECT 2400/REL-LAPM
CONNECT,38400,2400=CONNECT 2400/REL-LAPM-COMP
CONNECT,38400,2400=CONNECT 2400/REL-V.42
CONNECT,38400,2400=CONNECT 2400/REL-V.42-COMP

CONNECT,38400,1200=CONNECT 1200
CONNECT,38400,1200=CONNECT 1200/REL
CONNECT,38400,1200=CONNECT 1200/REL-MNP
CONNECT,38400,1200=CONNECT 1200/REL-MNP-COMP
CONNECT,38400,1200=CONNECT 1200/REL-LAPM
CONNECT,38400,1200=CONNECT 1200/REL-LAPM-COMP
CONNECT,38400,1200=CONNECT 1200/REL-V.42
CONNECT,38400,1200=CONNECT 1200/REL-V.42-COMP
