; Generic 9600 bps Modem File 
; (Intended for use with Notes Ver. 2 and 2.1)

;=============================================================
; Last revision date: 03/23/93 (update this date
; each time you edit; it is also advisable to rename
; your edited file [use Save As, rather than Save 
; option] to avoid later confusion and to keep the 
; original .MDM file intact).

; NOTE: Refer to the file TEMPLATE.MDM (A Sample Modem 
; Command File) for a description of modem command 
; files and how they work. "A Sample Modem Command 
; File" is user selectable within the Lotus Notes 
; Setup dialog "Modem Type" listbox in which you found 
; this modem command file (see end of listings, 
; beginning with a period) and is a printable ASCII 
; text file (approximately 15 pages). 
;===============================================================

; HOW TO USE THIS FILE: The Generic 9600 bps Modem Command File is
; intended to be used when no command file currently exists for the available
; modem, and a reliable connection cannot be obtained with command files
; for modems which seem closest to the model in question.  It is possible this
; file will work as-is, with no editing required from the user.  Should initial
; attempts fail, turn on LOG I/O and try to determine the problem's source.
; The paragraphs below describe how to deal, in order of likelihood with the
; three most common reasons for command file failure.

; 1. This file contains CONNECT responses phrased in the widest possible 
; variety of ways in an endeavor to match the exact syntax utilized by many 
; currently manufactured modems.  As the CONNECT response syntax may
; vary significantly from modem to modem there is no guarantee that the 
; result codes listed here will enable Notes to properly initialize an 
; unsupported modem.  If the result codes which your modem "speaks" 
; aren't listed, it will be necessary for you to consult the manual or the 
; manufacturer for the proper phrasing.

; 2.  The next thing you'll need to do will be to determine the proper commands
; for activating RTS/CTS ENABLED or IGNORED (assuming your modem
; supports hardware flow control).  Again a wide variety of possible
; commands have been listed, but all have been remmed out (see the
; section headed "[commands]" below--the disabled lines have semicolons 
; in front of them, which will need to be removed to make the commands active).
; It will be necessary for you to consult your user's manual to determine which 
; set (if any) are correct for your modem.  

; 3.  Lastly, the main setup strings, SETUP=AT&F, SETUP=ATE0V1, and
; SETUP=AT&C1&D2S0=0X4, allow the modem to operate using factory
; default settings (&F), with the certain necessary exceptions.  Echo is 
; turned off, and Verbose mode is turned on (English responses rather than 
; numeric).  The main string instructs the modem to track carrier, hang up if
; DTR (Data Terminal Ready signal) drops, to not auto-answer, and to enable
; a broad variety of result codes.  The chances are good that the factory
; defaults, combined with these required settings, will permit reliable
; connections to be obtained.  But here again, there are no guarantees,
; and further study of the manual, or a call to the vendor, may be required
; for use of your unsupported modem with Notes. 

; A special note concerning setup and CONNECT responses (section 1, above): 
; it is necessary that, if your modem employs an Auto-Reliable mode, the 
; command which turns this mode on be included in the main setup string,
; unless Auto-Reliable happens to be the factory default (as is the case with
; many modern modems).  The command (and any other deemed necessary)
; may simply be appended after the X4 command.  If you are not sure whether a
; failure to establish dialog is due to a missing Auto-Reliable command, try
; lowering the Maximum Speed via the user interface to the maximum rate the
; modem is rated for.  If the connection now succeeds, it usually means that the
; factory default is set to Normal or Direct mode, and that you are not getting the
; benefit of whatever compression the modem is capable of.  You should still,
; however be able to use the modem for Notes dialup.
;------------------------------------------------------------------------------------------------------------------------

[attributes]

MODELS=Generic V2 9600 bps Modem File (with instructions)
NULL MODEM=0
MAXIMUM SPEED=19200
DEFAULT SPEED=19200

[commands]

ESCAPE=+++
ATTENTION=ATE0V1
HANGUP=ATH0

;--------------------SETUP STRINGS (max. lines=15)---------------------------

SETUP=AT&F
SETUP=ATE0V1
SETUP=AT&C1&D2S0=0X4

;------RTS/CTS ENABLED or IGNORED (max. lines=2, min.=0)--------

; NOTE: If the computer and modem refuse to communicate with no
; flow control specified in the command file, either refer to the manual
; to determine if one of the following sets of commands is correct for
; your modem (or if yet another set is needed), or select one set at a
; time till you activate one which works.  The semicolons at the start
; of each line cause Notes to ignore the line, removing them
; causes Notes to utilize them in initializing the modem.

;RTS/CTS ENABLED=AT&K3
;RTS/CTS IGNORED=AT&K0

;RTS/CTS ENABLED=AT&K3&R0
;RTS/CTS IGNORED=AT&K3&R1

;RTS/CTS ENABLED=AT&K2&U3
;RTS/CTS IGNORED=AT&K0&U0

;RTS/CTS ENABLED=AT&H3
;RTS/CTS IGNORED=AT&H0

;RTS/CTS ENABLED=AT&H1&R2&K2
;RTS/CTS IGNORED=AT&H0&R1&K0

;RTS/CTS ENABLED=AT&E13
;RTS/CTS IGNORED=AT&E12

;RTS/CTS ENABLED=AT&R0S58=2S68=255
;RTS/CTS IGNORED=AT&R3S58=0S68=255

;RTS/CTS ENABLED=ATS58=2S66=1
;RTS/CTS IGNORED=ATS58=0S66=0

;RTS/CTS ENABLED=AT*F3
;RTS/CTS IGNORED=AT*F0

;RTS/CTS ENABLED=AT*FL3
;RTS/CTS IGNORED=AT*FL0

;RTS/CTS ENABLED=AT%F1
;RTS/CTS IGNORED=AT%F0

;RTS/CTS ENABLED=AT\\Q1
;RTS/CTS IGNORED=AT\\Q0

;RTS/CTS ENABLED=AT\\Q2
;RTS/CTS IGNORED=AT\\Q0

;RTS/CTS ENABLED=AT\\Q3
;RTS/CTS IGNORED=AT\\Q0

;RTS/CTS ENABLED=AT\\Q3&R0
;RTS/CTS IGNORED=AT\\Q0&R1

;-----------------------------------------------------

VOLUME OFF=ATM0
VOLUME LOW=ATM1L1
VOLUME MEDIUM=ATM1L2
VOLUME HIGH=ATM1L3
ANSWER=ATA
MANUAL DIAL=ATX3D
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,

[responses]

OK=OK

BUSY=BUSY

NO ANSWER=NO ANSWER

NO CARRIER=NO CARRIER

NO DIALTONE=NO DIALTONE
NO DIALTONE=NO DIAL TONE

ERROR=ERROR

RING=RING

;------------CONNECT RESPONSES (max. lines=150)----------

CONNECT, 19200, 9600=CONNECT 9600
CONNECT, 19200, 9600=CONNECT 9600 EC
CONNECT, 19200, 9600=CONNECT 9600/EC
CONNECT, 19200, 9600=CONNECT 9600/ECL
CONNECT, 19200, 9600=CONNECT 9600/NoEC
CONNECT, 19200, 9600=CONNECT 9600/REL
CONNECT, 19200, 9600=CONNECT 9600/REL 4
CONNECT, 19200, 9600=CONNECT 9600/REL 5
CONNECT, 19200, 9600=CONNECT 9600/ARQ
CONNECT, 19200, 9600=CONNECT 9600/V.42
CONNECT, 19200, 9600=CONNECT 9600/V42
CONNECT, 19200, 9600=CONNECT 9600/V42b
CONNECT, 19200, 9600=CONNECT 9600/V.42BIS
CONNECT, 19200, 9600=CONNECT 9600/V42BIS
CONNECT, 19200, 9600=CONNECT 9600/V.42bis
CONNECT, 19200, 9600=CONNECT 9600/V42bis
CONNECT, 19200, 9600=CONNECT 9600 V42
CONNECT, 19200, 9600=CONNECT 9600 V42bis
CONNECT, 19200, 9600=CONNECT 9600 MNP
CONNECT, 19200, 9600=CONNECT 9600 BUFFER
CONNECT, 19200, 9600=CONNECT 9600/V32
CONNECT, 19200, 9600=CONNECT 9600/ARQ/V32
CONNECT, 19200, 9600=CONNECT 9600/MNP5
CONNECT, 19200, 9600=CONNECT 9600/MNP4
CONNECT, 19200, 9600=CONNECT 9600/MNP3
CONNECT, 19200, 9600=CONNECT 9600/MNP2
CONNECT, 19200, 9600=CONNECT 9600/REL - MNP
CONNECT, 19200, 9600=CONNECT 9600/REL - LAPM
CONNECT, 19200, 9600=CONNECT 9600 RELIABLE
CONNECT, 19200, 9600=CONNECT 9600 RELIABLE COMPRESSED
CONNECT, 19200, 9600=CONNECT 9600/REC
CONNECT, 19200, 9600=CONNECT 9600/LAPM
CONNECT, 19200, 9600=CONNECT 9600 LAP-M
CONNECT, 19200, 9600=CONNECT 9600/COMP
CONNECT, 19200, 9600=CONNECT 9600/LAPM/COMP
CONNECT, 19200, 9600=CONNECT 9600/LAP-M ACTIVE
CONNECT, 19200, 9600=CONNECT 9600 TRELLIS
CONNECT, 19200, 9600=CONNECT 9600 TRELLIS/REL
CONNECT, 19200, 9600=CONNECT 9600 TRELLIS/LAPM
CONNECT, 19200, 9600=CONNECT 9600 TRELLIS/REL/COMP
CONNECT, 19200, 9600=CONNECT 9600 TRELLIS/LAPM/COMP

CONNECT, 19200, 4800=CONNECT 4800
CONNECT, 19200, 4800=CONNECT 4800 EC
CONNECT, 19200, 4800=CONNECT 4800/EC
CONNECT, 19200, 4800=CONNECT 4800/ECL
CONNECT, 19200, 4800=CONNECT 4800/NoEC
CONNECT, 19200, 4800=CONNECT 4800/REL
CONNECT, 19200, 4800=CONNECT 4800/REL 4
CONNECT, 19200, 4800=CONNECT 4800/REL 5
CONNECT, 19200, 4800=CONNECT 4800/ARQ
CONNECT, 19200, 4800=CONNECT 4800/V.42
CONNECT, 19200, 4800=CONNECT 4800/V42
CONNECT, 19200, 4800=CONNECT 4800/V42b
CONNECT, 19200, 4800=CONNECT 9600/V.42BIS
CONNECT, 19200, 4800=CONNECT 4800/V42BIS
CONNECT, 19200, 4800=CONNECT 4800/V.42bis
CONNECT, 19200, 4800=CONNECT 4800/V42bis
CONNECT, 19200, 4800=CONNECT 4800 V42
CONNECT, 19200, 4800=CONNECT 4800 V42bis
CONNECT, 19200, 4800=CONNECT 9600 MNP
CONNECT, 19200, 4800=CONNECT 4800 BUFFER
CONNECT, 19200, 4800=CONNECT 4800/V32
CONNECT, 19200, 4800=CONNECT 4800/ARQ/V32
CONNECT, 19200, 4800=CONNECT 4800/MNP5
CONNECT, 19200, 4800=CONNECT 4800/MNP4
CONNECT, 19200, 4800=CONNECT 4800/MNP3
CONNECT, 19200, 4800=CONNECT 4800/MNP2
CONNECT, 19200, 4800=CONNECT 4800/REL - MNP
CONNECT, 19200, 4800=CONNECT 4800/REL - LAPM
CONNECT, 19200, 4800=CONNECT 4800 RELIABLE
CONNECT, 19200, 4800=CONNECT 4800 RELIABLE COMPRESSED
CONNECT, 19200, 4800=CONNECT 4800/REC
CONNECT, 19200, 4800=CONNECT 4800/LAPM
CONNECT, 19200, 4800=CONNECT 4800 LAP-M
CONNECT, 19200, 4800=CONNECT 4800/COMP
CONNECT, 19200, 4800=CONNECT 4800/LAPM/COMP
CONNECT, 19200, 4800=CONNECT 4800/LAP-M ACTIVE
CONNECT, 19200, 4800=CONNECT 4800 TRELLIS
CONNECT, 19200, 4800=CONNECT 4800 TRELLIS/REL
CONNECT, 19200, 4800=CONNECT 4800 TRELLIS/LAPM
CONNECT, 19200, 4800=CONNECT 4800 TRELLIS/REL/COMP
CONNECT, 19200, 4800=CONNECT 4800 TRELLIS/LAPM/COMP

CONNECT, 19200, 2400=CONNECT 2400
CONNECT, 19200, 2400=CONNECT 2400 EC
CONNECT, 19200, 2400=CONNECT 2400/EC
CONNECT, 19200, 2400=CONNECT 2400/ECL
CONNECT, 19200, 2400=CONNECT 2400/NoEC
CONNECT, 19200, 2400=CONNECT 2400/REL
CONNECT, 19200, 2400=CONNECT 2400/REL 4
CONNECT, 19200, 2400=CONNECT 2400/REL 5
CONNECT, 19200, 2400=CONNECT 2400/ARQ
CONNECT, 19200, 2400=CONNECT 2400/V.42
CONNECT, 19200, 2400=CONNECT 2400/V42
CONNECT, 19200, 2400=CONNECT 2400/V42b
CONNECT, 19200, 2400=CONNECT 2400/V.42BIS
CONNECT, 19200, 2400=CONNECT 2400/V42BIS
CONNECT, 19200, 2400=CONNECT 2400/V.42bis
CONNECT, 19200, 2400=CONNECT 2400/V42bis
CONNECT, 19200, 2400=CONNECT 2400 V42
CONNECT, 19200, 2400=CONNECT 2400 V42bis
CONNECT, 19200, 2400=CONNECT 2400 MNP
CONNECT, 19200, 2400=CONNECT 2400 BUFFER
CONNECT, 19200, 2400=CONNECT 2400/MNP5
CONNECT, 19200, 2400=CONNECT 2400/MNP4
CONNECT, 19200, 2400=CONNECT 2400/MNP3
CONNECT, 19200, 2400=CONNECT 2400/MNP2
CONNECT, 19200, 2400=CONNECT 2400/REL - MNP
CONNECT, 19200, 2400=CONNECT 2400/REL - LAPM
CONNECT, 19200, 2400=CONNECT 2400 RELIABLE
CONNECT, 19200, 2400=CONNECT 2400 RELIABLE COMPRESSED
CONNECT, 19200, 2400=CONNECT 2400/REC
CONNECT, 19200, 2400=CONNECT 2400/LAPM
CONNECT, 19200, 2400=CONNECT 2400 LAP-M
CONNECT, 19200, 2400=CONNECT 2400/COMP
CONNECT, 19200, 2400=CONNECT 2400/LAPM/COMP
CONNECT, 19200, 2400=CONNECT 2400/LAP-M ACTIVE

CONNECT, 19200, 1200=CONNECT 1200
CONNECT, 19200, 1200=CONNECT 1200 EC
CONNECT, 19200, 1200=CONNECT 1200/EC
CONNECT, 19200, 1200=CONNECT 1200/ECL
CONNECT, 19200, 1200=CONNECT 1200/NoEC
CONNECT, 19200, 1200=CONNECT 1200/REL
CONNECT, 19200, 1200=CONNECT 1200/REL 4
CONNECT, 19200, 1200=CONNECT 1200/REL 5
CONNECT, 19200, 1200=CONNECT 1200/ARQ
CONNECT, 19200, 1200=CONNECT 1200/V.42
CONNECT, 19200, 1200=CONNECT 1200/V42
CONNECT, 19200, 1200=CONNECT 1200/V42b
CONNECT, 19200, 1200=CONNECT 1200/V.42BIS
CONNECT, 19200, 1200=CONNECT 1200/V42BIS
CONNECT, 19200, 1200=CONNECT 1200/V.42bis
CONNECT, 19200, 1200=CONNECT 1200/V42bis
CONNECT, 19200, 1200=CONNECT 1200 V42
CONNECT, 19200, 1200=CONNECT 1200 V42bis
CONNECT, 19200, 1200=CONNECT 1200 MNP
CONNECT, 19200, 1200=CONNECT 1200 BUFFER
CONNECT, 19200, 1200=CONNECT 1200 V.22
CONNECT, 19200, 1200=CONNECT 1200/MNP5
CONNECT, 19200, 1200=CONNECT 1200/MNP4
CONNECT, 19200, 1200=CONNECT 1200/MNP3
CONNECT, 19200, 1200=CONNECT 1200/MNP2
CONNECT, 19200, 1200=CONNECT 1200/REL - MNP
CONNECT, 19200, 1200=CONNECT 1200/REL - LAPM
CONNECT, 19200, 1200=CONNECT 1200 RELIABLE
CONNECT, 19200, 1200=CONNECT 1200 RELIABLE COMPRESSED
CONNECT, 19200, 1200=CONNECT 1200/REC
CONNECT, 19200, 1200=CONNECT 1200/LAPM
CONNECT, 19200, 1200=CONNECT 1200/COMP
CONNECT, 19200, 1200=CONNECT 1200/LAPM/COMP
CONNECT, 19200, 1200=CONNECT 1200/LAP-M ACTIVE

CARRIER,,9600=CARRIER 9600

CARRIER,,4800=CARRIER 4800

CARRIER,,2400=CARRIER 2400

CARRIER,,1200=CARRIER 1200

