; Motorola Codex 3220 Series

;===============================================
; Last revision date: 11/18/94 (update this date
; each time you edit; it is also advisable to rename
; your edited file [use Save As, rather than Save 
; option] to avoid later confusion and to keep the 
; original .MDM file intact).

; NOTE: Refer to the file TEMPLATE.MDM (A Sample Modem 
; Command File) for a description of modem command 
; files and how they work. "A Sample Modem Command 
; File" is user selectable within the Lotus Notes 
; Setup dialog "Modem Type" listbox in which you found 
; this modem command file (see end of listings, 
; beginning with a period) and is a printable ASCII 
; text file (approximately 14 pages). 

; Additional information may be obtained from either of 
; the two so-called "generic" modem command files 
; (alphabetically listed under letter G, designed for 
; use with Notes Releases 2.x and 3.x, 9600 bps and 
; 14400 bps maximum, respectively), each of which may 
; first be tried as-is with unlisted modems, then edited 
; if required (within the Notes edit box, or outside of 
; Notes, with any text editor) according to the printed 
; instructions within each file, and in compliance with 
; the vendor's command set, result codes, DIP switch 
; settings, and technical specifications as listed in 
; the equipment's users manual.

; For the specific modem(s) listed under this heading:
;=====================================================
[attributes]

MODELS=Motorola Codex 3220 Series
NULL MODEM=0
MAXIMUM SPEED=38400
DEFAULT SPEED=38400

[commands]

ESCAPE=+++
ATTENTION=ATE0V1
HANGUP=ATH0
SETUP=AT&F
SETUP=ATE0V1
SETUP=AT&C1&D3X4
SETUP=AT*XC1*RS0*SM1S0=0
; NOTE: The command *SMn, above, can be set
; to 3 to enable Auto Reliable mode (i.e. *SM3).
; It may also be set to 1, to force it into Normal
; mode, which turns off all protocols and error
; correction, allowing the modem a wider range of
; compatibility with other modems.
RTS/CTS ENABLED=AT*FL3
RTS/CTS IGNORED=AT*FL0
VOLUME OFF=ATM0
VOLUME LOW=ATM1L1
VOLUME MEDIUM=ATM1L2
VOLUME HIGH=ATM1L3
ANSWER=ATA
MANUAL DIAL=ATX1S9=1D
AUTO DIAL SETUP=ATS9=6
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,

[responses]

OK=OK

BUSY=BUSY

NO ANSWER=NO ANSWER

NO CARRIER=NO CARRIER

NO DIALTONE=NO DIALTONE

ERROR=ERROR

RING=RING

CONNECT,  38400,38400=CONNECT 38400 RELIABLE
CONNECT,  38400,38400=CONNECT 38400

CONNECT,  38400,19200=CONNECT 19200 RELIABLE
CONNECT,  38400,19200=CONNECT 19200

CONNECT,  38400,14400=CONNECT 14400 RELIABLE
CONNECT,  38400,14400=CONNECT 14400

CONNECT,  38400,12000=CONNECT 12000 RELIABLE
CONNECT,  38400,12000=CONNECT 12000

CONNECT,  38400,9600=CONNECT 9600 RELIABLE
CONNECT,  38400,9600=CONNECT 9600

CONNECT,  38400,7200=CONNECT 7200 RELIABLE
CONNECT,  38400,7200=CONNECT 7200

CONNECT,  38400,4800=CONNECT 4800 RELIABLE
CONNECT,  38400,4800=CONNECT 4800

CONNECT,  38400,2400=CONNECT 2400 RELIABLE
CONNECT,  38400,2400=CONNECT 2400

CONNECT,  38400,1200=CONNECT 1200 RELIABLE
CONNECT,  38400,1200=CONNECT 1200

