; USRobotics Sportster 14400 V.32bis/V.42bis 

;===============================================
; Last revision date: 07/13/93 (update this date
; each time you edit; it is also advisable to rename
; your edited file [use Save As, rather than Save 
; option] to avoid later confusion and to keep the 
; original .MDM file intact).

; NOTE: Refer to the file TEMPLATE.MDM (A Sample Modem 
; Command File) for a description of modem command 
; files and how they work. "A Sample Modem Command 
; File" is user selectable within the Lotus Notes 
; Setup dialog "Modem Type" listbox in which you found 
; this modem command file (see end of listings, 
; beginning with a period) and is a printable ASCII 
; text file (approximately 15 pages). 

; Additional information may be obtained from either of 
; the two so-called "generic" modem command files 
; (alphabetically listed under letter G, designed for 
; use with Notes Releases 2.x and 3.x, 9600 bps and 
; 14400 bps maximum, respectively), each of which may 
; first be tried as-is with unlisted modems, then edited 
; if required (within the Notes edit box, or outside of 
; Notes, with any text editor) according to the printed 
; instructions within each file, and in compliance with 
; the vendor's command set, result codes, DIP switch 
; settings, and technical specifications as listed in 
; the equipment's users manual.

; For the specific modem(s) listed under this heading:
;======================================================

; Switch settings:  
;        8 Pos switch: 1,2,6 = UP, all others DOWN 
  
[attributes]

MODELS=USRobotics Sportster 14400 V.32bis/V.42bis
DEFAULT SPEED=38400
MAXIMUM SPEED=38400
NULL MODEM=0

[commands]

ESCAPE=+++
ATTENTION=ATE0V1
HANGUP=ATH0
SETUP=AT&F
SETUP=ATE0&A2B0&N0S10=15&B1
SETUP=ATV1Q0S0=0S7=60X4
RTS/CTS ENABLED=AT&H1&R2&K2
RTS/CTS IGNORED=AT&H0&R1&K0
VOLUME OFF=ATM0
VOLUME LOW=ATM1
VOLUME MEDIUM=ATM1
VOLUME HIGH=ATM1
ANSWER=ATA
MANUAL DIAL=ATX3S9=1D,
AUTO DIAL SETUP=ATS9=6
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,

[responses]

OK=OK

RING=RING

BUSY=BUSY

NO DIALTONE=NO DIAL TONE

NO ANSWER=NO ANSWER

NO CARRIER=NO CARRIER

ERROR=ERROR

CONNECT, 38400,14400=CONNECT 14400
CONNECT, 38400,14400=CONNECT 14400/ARQ
CONNECT, 38400,14400=CONNECT 14400/V32
CONNECT, 38400,14400=CONNECT 14400/ARQ/V32

CONNECT, 38400,12000=CONNECT 12000
CONNECT, 38400,12000=CONNECT 12000/ARQ
CONNECT, 38400,12000=CONNECT 12000/V32
CONNECT, 38400,12000=CONNECT 12000/ARQ/V32

CONNECT, 38400,9600=CONNECT 9600
CONNECT, 38400,9600=CONNECT 9600/ARQ
CONNECT, 38400,9600=CONNECT 9600/V32
CONNECT, 38400,9600=CONNECT 9600/ARQ/V32

CONNECT, 38400,7200=CONNECT 7200
CONNECT, 38400,7200=CONNECT 7200/ARQ
CONNECT, 38400,7200=CONNECT 7200/V32
CONNECT, 38400,7200=CONNECT 7200/ARQ/V32

CONNECT, 38400,4800=CONNECT 4800
CONNECT, 38400,4800=CONNECT 4800/ARQ
CONNECT, 38400,4800=CONNECT 4800/V32
CONNECT, 38400,4800=CONNECT 4800/ARQ/V32

CONNECT, 38400,2400=CONNECT 2400
CONNECT, 38400,2400=CONNECT 2400/ARQ

CONNECT, 38400,1200=CONNECT 1200
CONNECT, 38400,1200=CONNECT 1200/ARQ
