; Multitech V.32/V.32bis w/V.42bis
; Models MT932BA (9600 bps) and 1432BA (14400 bps) modems.

;=============================================================
; Last revision date: 02/18/93 (update this date
; each time you edit; it is also advisable to rename
; your edited file [use Save As, rather than Save 
; option] to avoid later confusion and to keep the 
; original .MDM file intact).

; NOTE: Refer to the file TEMPLATE.MDM (A Sample Modem 
; Command File) for a description of modem command 
; files and how they work. "A Sample Modem Command 
; File" is user selectable within the Lotus Notes 
; Setup dialog "Modem Type" listbox in which you found 
; this modem command file (see end of listings, 
; beginning with a period) and is a printable ASCII 
; text file (approximately 15 pages). 

; Additional information may be obtained from either of 
; the two so-called "generic" modem command files 
; (alphabetically listed under letter G, designed for 
; use with Notes Releases 2.x and 3.x, 9600 bps and 
; 14400 bps maximum, respectively), each of which may 
; first be tried as-is with unlisted modems, then edited 
; if required (within the Notes edit box, or outside of 
; Notes, with any text editor) according to the printed 
; instructions within each file, and in compliance with 
; the vendor's command set, result codes, DIP switch 
; settings, and technical specifications as listed in 
; the equipment's users manual.

; For the specific modem(s) listed under this heading:
;===============================================================

; Switch settings:
;
;  1  2  3  4  5  6  7  8  9  10  11  12      13   14   15   16 
;  U U  D U  U  U D  D D   U   D   D       U    U    U    U

[attributes]

MODELS=MultiTech 932BA & 1432BA (AT Responses)
NULL MODEM=0
MAXIMUM SPEED=38400 
; 38400 for the 932BA, 57600 for the 1432BA
DEFAULT SPEED=38400

[commands]

ESCAPE=+++

ATTENTION=ATE0V1

HANGUP=ATH0

SETUP=AT&F

SETUP=ATE0V1

SETUP=AT$SB38400

;  .. SETS SERIAL BPS RATE FROM DTE TO DCE AT 38400 
; (UI WILL OVERRIDE AS REQUIRED BY OS LIMIT)

SETUP=AT&E1&E4&E13&E15$BA0&D2&C1#A0
; &E1     .. AUTO-RELIABLE ERROR CORRECTION
; &E4     .. CTS MODEM-INITIATED FLOW CONTROL
; &E13    .. PACING ENABLED (FLOW CONTROL, MODEM - SOFTWARE)
; &E15    .. DATA COMPRESSION ENABLED
; $BA0    .. ALLOWS SERIAL BAUD AND MODEM BAUD TO BE INPEPENDANT
; &D2     .. MODEM REACTS TO DTR NORMALLY (GOES ON HOOK WHEN DTR LOST)
; &C1     .. ALLOWS CARRIER DETECT TO ACT NORMALLY
; #A0     .. ENABLES AUTO-SPEED DETECT (14400) TO (12000) TO 9600 TO 4800 
             TO 2400 TO 1200 TO 300 BAUD

SETUP=AT&Q1Q0V1X4S0=0
; &Q1     .. SELECTS STANDARD AT COMMAND SET
; Q0      .. RESULT CODES SENT
; V1      .. RESULT CODES SENT AS WORDS
; X4      .. SELECTS STANDARD AT COMMAND SET WITH "NO DIAL TONE" AND "BUSY"
; S0=0    .. SETS RINGS UNTIL ANSWER TO 0  (WILL NOT AUTO-ANSWER)

VOLUME OFF=ATM0
; SPEAKER ALWAYS OFF

VOLUME LOW=ATM1
VOLUME MEDIUM=ATM1
VOLUME HIGH=ATM1
;VOLUME ON UNTIL CARRIER DETECT=ATM1

RTS/CTS ENABLED=AT&E13 
; (PACING ON, FLOW CONTROL ENABLED)
RTS/CTS IGNORED=AT&E12 
; (PACING OFF, FLOW CONTROL DISABLED)

ANSWER=ATA

MANUAL DIAL=ATB0S9=1D
; B0     .. NO WAIT FOR TONE DIALING

AUTO DIAL SETUP=ATS9=6 
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,
; ,      .. COMMA IN DIALING STRING = DEFAULT 2 SECOND PAUSE PER COMMA

[responses]

OK=OK

BUSY=BUSY

NO ANSWER=NO ANSWER

NO CARRIER=NO CARRIER

NO DIALTONE=NO DIAL TONE

ERROR=ERROR

RING=RING

CONNECT, 38400,14400=CONNECT 14400 LAPM COMPRESSED
CONNECT, 38400,14400=CONNECT 14400 LAPM
CONNECT, 38400,14400=CONNECT 14400 RELIABLE COMPRESSED
CONNECT, 38400,14400=CONNECT 14400 RELIABLE 
CONNECT, 38400,14400=CONNECT 14400  

CONNECT, 38400,12000=CONNECT 12000 LAPM COMPRESSED
CONNECT, 38400,12000=CONNECT 12000 LAPM
CONNECT, 38400,12000=CONNECT 12000 RELIABLE COMPRESSED
CONNECT, 38400,12000=CONNECT 12000 RELIABLE
CONNECT, 38400,12000=CONNECT 12000

CONNECT, 38400,9600=CONNECT 9600 LAPM COMPRESSED
CONNECT, 38400,9600=CONNECT 9600 LAPM
CONNECT, 38400,9600=CONNECT 9600 RELIABLE COMPRESSED
CONNECT, 38400,9600=CONNECT 9600 RELIABLE
CONNECT, 38400,9600=CONNECT 9600

CONNECT, 38400,7200=CONNECT 7200 LAPM COMPRESSED
CONNECT, 38400,7200=CONNECT 7200 LAPM
CONNECT, 38400,7200=CONNECT 7200 RELIABLE COMPRESSED
CONNECT, 38400,7200=CONNECT 7200 RELIABLE
CONNECT, 38400,7200=CONNECT 7200

CONNECT, 38400,4800=CONNECT 4800 LAPM COMPRESSED
CONNECT, 38400,4800=CONNECT 4800 LAPM
CONNECT, 38400,4800=CONNECT 4800 RELIABLE COMPRESSED
CONNECT, 38400,4800=CONNECT 4800 RELIABLE
CONNECT, 38400,4800=CONNECT 4800

CONNECT, 38400,2400=CONNECT 2400 LAPM COMPRESSED
CONNECT, 38400,2400=CONNECT 2400 LAPM
CONNECT, 38400,2400=CONNECT 2400 RELIABLE COMPRESSED
CONNECT, 38400,2400=CONNECT 2400 RELIABLE
CONNECT, 38400,2400=CONNECT 2400

CONNECT, 38400,1200=CONNECT 1200 LAPM COMPRESSED
CONNECT, 38400,1200=CONNECT 1200 LAPM
CONNECT, 38400,1200=CONNECT 1200 RELIABLE COMPRESSED
CONNECT, 38400,1200=CONNECT 1200 RELIABLE
CONNECT, 38400,1200=CONNECT 1200





