+=====================================================================+
|           FixPax for IBM OS/2 WARP 3.0 SYSLEVEL XR03000             |
+=====================================================================+

                              IMPORTANT

  DOWNLOADING THE SERVICE FIX THAT FOLLOWS, INDICATES YOUR ACCEPTANCE OF
  THE FOLLOWING TERMS AND CONDITIONS:

  - YOU MUST BE, AND YOU AGREE THAT YOU ARE, A PRIOR LICENSEE
    OF OS/2 VERSION 3.0
  - YOU MAY MAKE COPIES OF THE OS/2 VERSION 3.0 SERVICE FIX
    EQUAL TO THE NUMBER OF LICENSED COPIES OF OS/2 VERSION
    3.0 YOU POSSESS
  - YOU MAY ONLY USE THIS SERVICE FIX FOR MAINTENANCE PURPOSES
  - ALL OTHER TERMS AND CONDITIONS OF YOUR OS/2 VERSION 3.0
    LICENSE AGREEMENT APPLY TO THIS SERVICE FIX; HOWEVER,
    THIS DOES NOT EXTEND ANY WARRANTY OUTLINED IN SUCH
    AGREEMENT.

+=====================================================================+
|                        Installation Notes                           |
+=====================================================================+
1) You will need the OS/2 Warp 3.0 Corrective Service Facility boot
   disks to install this FixPak. These files should be available from
   the same place you got this FixPak from as

   WARPBDSK.1DK - Corrective Service Facility disk 1 (SP DISK 1)
   WARPBDSK.2DK - Corrective Service Facility disk 2 (SP DISK 2)

      - or -

   WKICKR.ZIP   - File compressed with PKZIP. Contains both of the
                  above disk images. Requires PKUNZIP or UNZIP to
                  extract original files from compressed file.

   To create diskettes from the disk image files you need LOADDSKF.EXE.
   This is also available from the same place you got this FixPak from
   as

   LDF.COM      - Self extracting file that will create LOADDSKF.EXE.
                  Place in a separate directory on your harddisk then
                  enter LDF.

      - or -

   LOADDSKF.ZIP - File compressed with PKZIP, contains LOADDSKF.EXE.
                  Requires PKUNZIP or UNZIP to extract original files
                  from compressed file.

   Use LOADDSKF.EXE to create the diskettes. For each disk image place
   a 2MB HD (1.44MB formatted) diskette in A:

   a. Enter LOADDSKF WARPBDSK.1DK A: /F
        Label as Corrective Service Facility disk 1
   b. Enter LOADDSKF WARPBDSK.2DK A: /F
        Label as Corrective Service Facility disk 2
   c. Enter LOADDSKF XR0W005.1DK A: /F
        Label as FixPak XR0W005 Corrective Service disk 1 (CSF DISK 1)
   d. Enter LOADDSKF XR0W005.2DK A: /F
        Label as FixPak XR0W005 Corrective Service disk 2 (CSF DISK 2)
   e. Enter LOADDSKF XR0W005.3DK A: /F
        Label as FixPak XR0W005 Corrective Service disk 3 (CSF DISK 3)

2) This FixPak will be a prerequisite too all future OS/2 Warp 3.0 FixPaks.

3) If you installed OS/2 Warp 3.0 from a CD-ROM some files being updated
   will have the Read Only attribute set. This will cause the update
   program to ask you if you want them replaced. Answer OK.

4) If the following files are not updated on your system after this
   FixPak has been applied then you must install this FixPak a second
   time without backing out the first install. This will correctly update
   these files:

          USERS.SCR
          WINOS2.COM
          WINSMSG.DLL

   To check if the files were updated look at the SERVICE.LOG in the
   \OS2\INSTALL directory. There should be two entries for each file.
   The entries should look (for example) like one of the following:

         Archiving for x:\WINDOWS\SYSTEM\USERS.SCR.
         Updating x:\WINDOWS\SYSTEM\USERS.SCR

                         or

         Archiving for x:\WINDOWS\SYSTEM\USERS.SCR.
         Deferring service of x:\WINDOWS\SYSTEM\USERS.SCR

     (x: is the drive where Microsoft Windows is installed.)

   If the entries are not there then you need to repeat the install of
   this FixPak as mentioned above. Do not back out the first install
   of this fixpak. Just repeat the install a second time.

5) The Current CSD level for the "IBM OS/2 Base Operating System" will
   not be changed by installation of this FixPak. Look at the file

         \OS2\INSTALL\SERVICE.LOG

   for information relating to the installation of this (or any) FixPak
   on your system. To see the CSD level and other related information
   use the SYSLEVEL command.

6) If you get a "No files to service" message while applying this FixPak
   then the Current CSD level or Component ID of the "IBM OS/2 Base
   Operating System" is incorrect. Correct values must be:

         Current CSD level: XR03000
              Component Id: 562260100

7) See the README2 file on this same disk for a list of APARs fixed.

+=====================================================================+
|                        Installation Process                         |
+=====================================================================+
To INSTALL this fix perform the following steps:

1. Insert Corrective Service Facility disk 1 in A:.

2. Open an OS/2 window or Full Screen.

3. Enter a:\service and press the ENTER key.

   Note: DO NOT boot CSF disk 1. This method is only for use with
         CID install and requires a response file tailored to your
         system.

4. Follow displayed instructions. When prompted to insert Corrective
   Service disk 1 (not Corrective Service Facility disk 1) place
   FixPak XR0W005 disk 1 in a:. Repeat for disk 2 and disk 3.

5. If this is the first OS/2 v3.0 Warp FixPak you have applied to
   this system then enter the path where a copy of replaced file(s)
   will be stored in the ARCHIVE directory, Ex. D:\ARCHIVE.

   Note: This ARCHIVE directory is not related to the ARCHIVES directory
         built into OS/2 Warp 3.0. Please specify a different path.

   If this is not the first OS/2 Warp v3.0 FixPak then enter the path
   where a copy of replaced file(s) will be stored in the BACKUP directory,
   EX. D:\BACKUP.

   For either case make sure there is a sufficient space available. Even
   though these files are kept in compressed (PACK2) format they will
   require 4.5MB of disk space.

6. Click on "OK".

7. Select NO for redisplay of "Product List" when displayed (after
   the first part of the FixPak apply process has completed).

8. Close the Corrective Service Facility window.

9. Shut down and reboot your system.

+=====================================================================+
|                  FixPak Corrective Service Notes                    |
+=====================================================================+
OS/2 Warp 3.0 FixPak          = XR0W005
CORRECTIVE SERVICE LEVEL(CSD) = XR_3000

BUILD LEVEL 8.213B

Product name:  "IBM OS/2 Base Operating System"
Standard Edition  3.00
New CSD Level:  XR0W005_   (Country = United States)
Pre-requisite CSD Level:  XR03000_
System Id:  1000
Component Id:  562260100
Archive is ON for this product.

Files contained in CSD for product:

Filename      Name on CSD   Disk#  Date      Time   Size
------------  ------------  -----  --------  -----  -------
AHA152X.ADD   AHA152X.AD_     2    12/12/94  15:36    38044
AHA164X.ADD   AHA164X.AD_     3    12/12/94  15:36    19716
AIC7870.ADD   AIC7870.AD_     1    12/15/94  16:01    34092
ARCINST.EXE   ARCINST.EX_     3    12/12/94  20:48    21774
ARCRECOV.EXE  ARCRECOV.EX_    2    12/12/94  20:50    24635
BTSCSI.ADD    BTSCSI.AD_      3    12/12/94  15:40    22737
CHKDSK.COM    CHKDSK.CO_      2    01/09/95  07:58    68656
COM.SYS       COM.SY_         3    12/12/94  15:46    16888
CS4231.SYS    CS4231.SY_      3    01/04/95  15:33    33145
DOSCALL1.DLL  DOSCALL1.DL_    1    01/09/95  08:09   137082
E.EXE         E.EX_           2    01/06/95  23:56    70917
FD16-700.ADD  FD16-700.AD_    3    01/10/95  15:17    31258
FD7000EX.ADD  FD7000EX.AD_    3    12/12/94  15:38    20848
FD8XX.ADD     FD8XX.AD_       2    12/12/94  15:39    30030
HPFS.IFS      HPFS.IF_        2    01/31/95  19:54   135746
IBM1FLPY.ADD  IBM1FLPY.AD_    2    12/15/94  15:57    31058
IBM1S506.ADD  IBM1S506.AD_    3    01/15/95  21:21    28328
IBM2AMB1.SYS  IBM2AMB1.SY_    3    12/12/94  17:01    13708
IBM2AST1.SYS  IBM2AST1.SY_    3    12/12/94  17:00    11201
IBM2CAD1.SYS  IBM2CAD1.SY_    3    12/12/94  17:04    13743
IBM2CMQ1.SYS  IBM2CMQ1.SY_    3    12/12/94  17:01    11240
IBM2FLPY.ADD  IBM2FLPY.AD_    3    01/06/95  19:17    13754
IBM2MAT1.SYS  IBM2MAT1.SY_    3    12/12/94  17:03    11201
IBM2NCR1.SYS  IBM2NCR1.SY_    3    12/12/94  17:02    11201
IBM2NEC1.SYS  IBM2NEC1.SY_    3    12/12/94  17:02    11201
IBM2SCSI.ADD  IBM2SCSI.AD_    3    12/01/94  11:39    32629
IBM2SS01.SYS  IBM2SS01.SY_    3    12/12/94  16:59    14367
IBM2SS02.SYS  IBM2SS02.SY_    3    12/12/94  17:00    11576
IBM2TOS1.SYS  IBM2TOS1.SY_    3    12/12/94  16:59    11217
IBM2ZEN1.SYS  IBM2ZEN1.SY_    3    12/12/94  16:58    11201
IBM2ZOS1.SYS  IBM2ZOS1.SY_    3    12/12/94  17:03    11217
IBMIDECD.FLT  IBMIDECD.FL_    3    01/10/95  20:47    20490
IBMKBD.SYS    IBMKBD.SY_      3    01/06/95  20:05     5572
MITFX001.ADD  MITFX001.AD_    3    01/24/95  20:15    20482
MVPRODD.SYS   MVPRODD.SY_     2    01/10/95  19:44    52074
OS2DASD.DMD   OS2DASD.DM_     2    01/04/95  20:52    33578
OS2DUMP       OS2DUMP.___     3    01/10/95  17:24    12251
OS2KRNL       OS2KRNL.___     1    02/02/95  21:23   556026
OS2LDR        OS2LDR.___      3    01/10/95  17:23    30208
OS2MM.DLL     OS2MM.DL_       2    01/31/95  17:02   366710
PCMCIA.SYS    PCMCIA.SY_      3    01/24/95  20:20    41990
PCMCIA.TBL    PCMCIA.TB_      3    12/12/94  15:21     1681
PMGRE.DLL     PMGRE.DL_       3    12/12/94  18:58     2216
PMMERGE.DLL   PMMERGE.DL_     1    02/02/95  20:57   873096
PMSHAPI.DLL   PMSHAPI.DL_     3    11/10/94  01:03     4549
PMWP.DLL      PMWP.DL_        2    12/12/94  22:57   933881
PRINT01.SYS   PRINT01.SY_     3    01/04/95  21:23    11038
PRINT02.SYS   PRINT02.SY_     3    01/04/95  21:23    10166
RESERVE.SYS   RESERVE.SY_     3    12/12/94  15:31     5686
SBCD2.ADD     SBCD2.AD_       3    12/12/94  15:42    18834
SESMGR.DLL    SESMGR.DL_      3    11/10/94  16:08     1536
SONY31A.ADD   SONY31A.AD_     3    12/15/94  16:06    32480
SYSTEM.TDF    SYSTEM.TD_      3    02/02/95  22:14    71980
SYSTEM.TFF    SYSTEM.TF_      2    02/02/95  22:14   183417
UHPFS.DLL     UHPFS.DL_       2    01/31/95  20:02   181968
USERS.SCR     USERS.SC_       3    01/18/95  15:27    16896
VCOM.SYS      VCOM.SY_        3    02/14/95  14:56    12384
VWIN.SYS      VWIN.SY_        3    12/12/94  21:46    24560
WINOS2.COM    WINOS2.CO_      2    01/31/95  08:43    31502
WINSMSG.DLL   WINSMSG.DL_     3    01/18/95  15:29    28672
WPPRINT.DLL   WPPRINT.DL_     2    01/24/95  20:08   369285

+=====================================================================+
|                           Additional Notes                          |
+=====================================================================+

1: To view the Corrective Service Facility documentation:

   A. Insert Corrective Service Facility disk 1 in A:

   B. Enter view a:readme.inf and press the ENTER key
