
Before loading ISDNAPI.SOL to SoLIS change the parameter
"Protocol" in the file SOLIS.INI to one of the following list:


RTT         Belgium
VN          France
1TR6        Germany
ETSI-CH     Swiss
ETSI-DK     Denmark
ETSI-GB     Great Britain
ETSI-I      Italy
ETSI-N      Norway
ETSI        various other European countries with E-DSS1 protocol

To load the card and load the resident PC driver simply type
"CAPI" at the DOS command prompt.
