WiscWorld for Windows - Version 2.0
Packet Driver Installation Notes
August 15, 1994

Please READ this file before continuing with the installation.

The Network Detective has determined that a packet driver is
loaded into the memory of your machine.  

To continue installation, you will have to provide some information
about your network configuration.  Please be prepared to answer the 
following questions or click the 'Exit Install' button in the next 
dialog screen.

    IP Address:
    Netmask:
    Gateway:

    DNS:		128.104.30.38
    Domain:	nn.wisc.edu
    MTU:		1500
    TCP RWIN:	4096
    TCP MSS:	1460

WiscWorld offers suitable default values are offered for the last five
items, but you should consult your local network (LAN) administrator.

The installation program will try to automatically install and
configure your system to run the WiscWorld package; however, 
the installer will not be able to handle a few situations.

       If you are not loading Windows from your AUTOEXEC.BAT file, the
       installer will not insert the command to load the WINPKT file.
       You will be warned at the end of the installation that you
       must edit AUTOEXEC.BAT.  We recommend that you place the WINPKT 
       command just before you execute the WIN command and after your
       packet driver is loaded.

If you haveproblems during installation or when using WiscWorld please 
call the DoIT Help Desk at 264-HELP (264-4357).


