

3/10/95


Auto Token-Ring 16/4 Adapter diskettes, version 1.30.

     DRIVERS.DSK    3-04-95
     LANAID.DSK     3-06-95
     NOVELCLI.DSK   3-06-94
     LSPBOOK.DSK   10-14-94 (unchanged)

LANAID has been fixed to properly disable Plug And Play so the
user can specify adapter settings on a machine with a Plug And Play
BIOS.

====================================================================

Use the LOADDSKF.EXE program to create the diskette(s)
from the diskette image(s) ending in DSK, for example:


     LOADDSKF DRIVERS.DSK A:


The diskette's format must match that of the image file.
Most are 3.5-inch 1.44MB diskette images. If you try to
use a diskette with the wrong density LOADDSKF will report
error "Target disk is wrong format". If you wish to reformat
the diskette to match the image you can add parameter /F
to the command line.

====================================================================
