* Title
"Cirrus Logic 542x Blitter Driver"

* Action routine DLL
"SVGAINST.DLL"

* Type key
"SVGA"

* # additional parameters specific to SVGA
"1"

* Additional parameter (Chipset manufacturer = 4 for Western digital)
"7"

* # of chain elements
"4"

* chain element = key, general prompt, diskette prompt, vol label, resolution

* Configuration chain element - key set set by SVGA.DLL (eg, CXXXxYYYxCCC)
""
* General prompt
"Cirrus Logic"
* diskette prompt
"Display Driver Diskette 1"
* volume label
"DISP 1"
* no resolution for configuration
""

* 3 more resolution chain elements follow

* resolution 640x480x256
* DSP key
"CL640x480x256B"
""
"Display Driver Diskette 1"
"DISP 1"
"640x480x256 blitter driver"

* resolution 800x600x256
"CL800x600x256"
""
"Display Driver Diskette 1"
"DISP 1"
"800x600x256 blitter driver"

* resolution 1024x768x256
"CL1024x768x256"
""
"Display Driver Diskette 1"
"DISP 1"
"1024x768x256 blitter driver"


