IMPORTANT INSTALLATION PROCEDURES AND LATEST INFORMATION 
_________________________________________________________

PLEASE READ THESE INSTRUCTIONS BEFORE YOU BEGIN INSTALLATION.


To Install Cirrus Logic Drivers for OS\2 2.0 read User Manual or
clinst20.txt for instructions.

To install Cirrus Logic Drivers for OS\2 2.1 read User Manual or
clinst21.txt for instructions.


Note:

If you downloaded these files from the BBS, unzip the file to a disk
and label the disk DISP 1 before installation.





Problems running SVGA.EXE in DOS
_________________________________


If you encounter problems using SVGA.EXE in Windowed DOS or Full 
Screen DOS, follow the procedures below:

1. Have a DOS Boot Disk Available and boot with the DOS operating 
   system in drive A.
   If you are running an older BIOS prior to v1.30 and you need to run 
   the new BIOS TSR, load the TSR at this time.
   ex: VGA22.EXE

2. Run CLMODE.EXE to set monitor type.
   ex: CLMODE M5

3. Insert the CIRRUS OS/2 INSTALLATION DISK in Drive A.

4. Run SVGA.EXE
   ex: SVGA ON DOS
   This will create an SVGADATA.DOS file on your diskette.

5. Copy this file to your OS/2 subdirectory in your hard drive.
   ex: copy a:\SVGADATA.DOS c:\os2\SVGADATA.PMI

6. Remove disk from drive A and reboot OS/2 operating system.
   
Anytime SVGA.EXE will not run in WINDOWED DOS OR FULL SCREEN DOS, 
repeat this procedure.

