
			  Little Big Adventure (LBA)
			    Twinsen's Adventure

			     March 13, 1995

    Copyright 1994-1995 Adeline Software International. All Rights Reserved.



REQUIREMENTS:

Little Big Adventure (LBA) requires:

A 486 IBM PC or 100% compatible
4 MB of memory
A VESA compliant SVGA card with 512 KB of RAM


The Recommended Configuration is:

486DX2 - 66 Mhz with local bus (VESA or PCI for example)
Local bus SVGA card with 1 MB of RAM
8 MB of memory
Sound Blaster 16 (Stereo 16 bits Sound FX + FM Music)


The current "Dream" configuration would be:

Pentium 100 Mhz
PCI Local bus SVGA card with 2 MB of RAM
17 inch monitor
8 MB of memory
Sound Blaster AWE32 (Stereo 16 bits Sound FX + Midi Music)
Hi-Fi Power Stereo Amplifier + Speakers



1. Installation

For now, make sure that you have at least 13 MBytes free on your Hard Disk
before installing.

2. Configuration

To configure LBA (Language, SVGA, Music card, Sound Card)
type SETUP in the LBA directory. Make sure to address every option
and save your configuration before returning to DOS.


LBA provides SPECIFIC support for each of the following sound cards:

100% compatible SoundBlaster
Sound Blaster Pro
Sound Blaster 16
Sound Blaster AWE32
ProAudio Spectrum
ProAudio Spectrum Plus
ProAudio Spectrum 16
Gravis UltraSound
Adlib Gold
Microsoft Windows Sound System
MT32 compatible midi cards such as the RAP-10 for MUSIC ONLY
Adlib compatible cards for MUSIC ONLY
OPL3 compatible cards for MUSIC ONLY


LBA currently supports all VESA compliant video cards.


Some specific cards and chipsets are also directly supported.
Those include:

Ati Chipset
Ati Mach32
Ati Ultra Pro
Ati VGA Wonder
Cirrus Logic Chipset
CL-GD 542X Chipset
Compaq AVGA Chipset
Compaq QVision
Diamond Speedstar (Tseng)
Diamond Stealth (S3)
Genoa Chipset
HP Ultra (S3)
NCR
NCR 77C22 Chipset
OAK OTI 067/077 Chipset
Orchid Designer VGA (Tseng)
Orchid Pro Designer VGA (Tseng)
Orchid Fahrenheit (S3)
Paradise
Quadram VGA Spectra (Tseng)
Realtek PT-505
Realtek RTG 3105 Chipset
STB Lightspeed (Tseng)
STB VGA EM-16 Plus (Tseng)
STB VGA Extra/EM (Tseng)
S3 Incorporated Chipset
Tecmar VGA/AD (Tseng)
Tseng 3000 Chipset
Tseng 4000 Chipset
Trident VGA
T8800/T9400 Chipset
Western Digital Chipset
WD90CXX Chipset

If any of those specific supports did not work we STRONGLY encourage you
to try the standard VESA driver.



3. Playing LBA

Type LBA in the LBA directory to run game.

Control keys are :

- During normal gameplaying :

UP              - Forward
DOWN            - Backward
RIGHT           - Turn Right
LEFT            - Turn Left
SPACEBAR        - Action corresponding to the current behaviour
		  * NORMAL: Talk / Read / Search / Use
		  * SPORTY: Jump
		  * AGGRESSIVE:
			Auto mode   : Fight
			Manual mode : While holding the spacebar down
				      UP / RIGHT / LEFT will manually select
				      different punch/kick options
		  * DISCREET: Kneel down to hide
ALT             - Throw the magic ball (when you've found it) in any
		  behaviour
		- Wield the sword after you have found it in any
		  behaviour
RETURN          - Recenter screen on Twinsen
CONTROL         - Behaviour menu
SHIFT           - Inventory
ESC             - Quit Game
F6              - Options menu


- Behavior menu :

To keep this menu active hold the CONTROL key down.
*  LEFT, RIGHT  - Change behavior

Behavioral Change - Quick Keys:
F1(Normal)
F2(Sporty)
F3(Aggressive)
F4(Discreet)

Behavior Menu Item Information:

Red bar         - Life points
Blue bar        - Magic power
		  Each level of magic you reach potentially gives you more
		  power
Coin            - Amount of money you have
Key             - Number of keys you have (open any normally locked door)
		- They are used automatically when needed
Four-Leaf Clover- Number of lives left
		  Can eventually be used through the inventory to reload
		  your Life points and Magic power


- Inventory menu :

Activate by pressing SHIFT key (don't need to hold it down).

LEFT, RIGHT,
UP, DOWN        - Move selection box.
		  An explanation about each object you own is displayed
		  at the bottom of the screen.
SPACEBAR        - go to the next page of explanation about the selected
		  object.
RETURN          - Use selected object if possible in current context.
ESC, SHIFT      - Exit Inventory menu

- Options Menu :

Activated through the F6 key or through the main menu



4. Tips and Tricks :

- When a character is hit by someone or something a little star indicates
  the loss of lifepoints. If there is no star when you hit someone, it
  means you are not strong enough (magic level) or your weapon is not
  appropriate.
- Don't forget to speak (SPACE BAR in Normal behaviour) to people before
  kicking (or even killing) them (if possible).
- Search in all the closets, trash-cans, chests, and flowers pots to find
  coins, life, magic, or keys. For example, at one particular stage you will
  need a rather large amount of money to progress.
- When you touch a door without a lock, it will be opened automatically. If
  the door has a lock you need to use a key. If you don't have a key you
  must adventure until you find one. (You can see the number of keys you
  possess in the behavior menu - (By using the CTRL key).
- Keys can be found in closets, flowers pots... or by killing a
  "monster" (Even doctors!).
- If you know a key was discovered but you can't see it, throw your magic
  ball. It will bring back any key that could be in the general area.
- Switches can be activated by the magic ball.



5. Troubleshooting


Step A. Configuration

If you are having problems launching the game, make sure that LBA is
configured properly.
If the problem remains, select VESA and no music and no sound FX and retry.
If the program gives you an error about VESA support, load the VESA driver
provided with your SVGA card (see SVGA card manual).
If the problem is solved go to step F, if not, go to Step B with this
minimal configuration.


Step B. EMS/UMB provider programs (memory managers)

Try setting up a DOS Boot Disk.  Refer to the DOS Boot Disk section of your
manual. If the problem is solved go to Step F, if not, go to the next step.


Step C. Caching programs

Try reducing the size of any disk cache such as SMARTDRV.EXE (leave some
cache if possible, even 256 KB or less) in your CONFIG.SYS or AUTOEXEC.BAT.
Eventually try removing any reference to those programs in your CONFIG.SYS
or AUTOEXEC.BAT. If the problem is solved go to Step F, if not, go to the
next step.


Step D. HIMEM.SYS

Try removing HIMEM.SYS from your Boot Disk CONFIG.SYS. If the problem is
solved go to Step F, if not, go to the next step.


Step E. Reinstall LBA

Put the Boot Disk in drive A and reboot using this floppy disk. Then
re-install LBA from floppy. If the problem is solved go to step F,
if not, your computer does not have enough memory to run LBA.


Step F. Reconfiguration

You can now try to reconfigure your SVGA, Music, and Sound FX cards with the
LBA setup program.
Enjoy LBA.



6. Technical information

The best configuration for LBA would be a machine with HIMEM.SYS
loaded, no memory manager such as EMM386 or QEMM386, and a disk
caching program.
It is best not have anything loaded high since LBA will make better use
of extended memory than of DOS memory. Therefore, try leaving resident
programs in DOS memory.

LBA does not use EMS.
