/*****/This is for the minimum amount of disk space needed.
#disk
5000000
/*****/This is for the Minimum EMS memory needed to play the game
#ems
0
#xms
0
#addtime
10
#base
100
#adds
6
#pcxnames
new6.pcx
new2b.pcx
alsoavlb.pcx
sc_ed_ad.pcx
alsoavlb.pcx
bs4_3ow.pcx
END
#defaultpath
HARPOON2
#vesa
0x101
#arcnum
2
#disknum
2
#arcsize
1153379
1289757
#cpu
3
#filenum
24
25
#filenames
DISK1
coldwar.000
DISK2
coldwar.001
END
#dosver
5.0
#readme
readme.cw
#checkfile
harpoon2.exe
#wel
ColdWar Installation
#pre
Available Drives
#main
Installing ColdWar
#close
Installation Complete
#autoti
Auto Configuration
#prob
 Your System Configuration Needs an Adjustment
\
#driveinfo
The ColdWar needs to be installed under the
same directory as Harpoon II, please enter the
full path below.\
#mousep
  A mouse driver was not found!\
#mousea
 The solution to this problem is to
install a mouse driver of the make
Logitech(c) or Microsoft(c).  The
current versions are 6.0 and up for
Logitech(c) and 8.0 and up for
Microsoft(c).  If you don't have a
mouse you will not be able to play
Harpoon II.  You will, however,
be able to continue installation
by pressing <ENTER> when prompted
to continue.  You may quit now or
continue the installation.  Hit any
key to continue installing or hit
'Esc' to exit.\

#vesap
  You have a VESA driver installed
into memory, but your video card is
unable to support VESA mode 0x101.
Harpoon II requires support of
this extended video mode to play as
it displays graphics in 640x480
resolution with 256 colors.  Most
likely your video card does not
have the minimum 512k memory on
board to support this display
mode.\
#vesaa
    If this is indeed the case,
then the solution is to upgrade
the memory on your video card so
that it has a minimum video memory
of 512k.  Another option would be
to acquire a video card that has at
least 512k video memory and is VESA
compliant.  Press the right mouse
button to Exit.\

#suitp
   There is no drive with enough
free space on it to install Cold War.
The total amount of free drive space
needed to install is 5,000,000 bytes,
plus 3,000,000 bytes for temporary
swap space during the installation
process.\
#suita
    The solution to this is to
free some space on a fixed drive
and attempt to re-install Cold War.
You may press the 'Esc' key or
the right mouse button to exit.\
#noemsp
    The problem is that you do not
have enough EMS ram available to
run the game.\
#noemsa
    One solution to this problem is
to remove any programs that might
already be using EMS Memory.
You may continue with the install
or press the right mouse button or
'Esc' to exit.\
#noacp
    Your computer does not have
sufficient system memory (RAM) to
play H2.  Please note that the
minimum memory requirement to play
Harpoon II is 4MB RAM.\
#noaca
    The only way to solve this
problem is to install more memory
(RAM) onto your system.  You may
press the 'Esc' key or the right
mouse button to exit.\
#noinstp
    The problem is that there is
no Memory Manager installed.\
#noinsta
    This can be solved by using
the EMM386.exe driver that comes
with DOS 5.0 or Windows 3.x.
    Consult your DOS or Windows
Manual on installing these drivers.\
#noxmsp
    The problem is that there is
not enough XMS memory available for
Harpoon II to use.\
#noxmsa
    The solution is to increase the
number of handles of your XMS Memory
Manger to raise the memory.  You
may continue with the install by
pressing the continue button or by
pressing any key.  If you would
like to quit at this time, press
the right mouse button or the 'Esc'
key.\

#noconp
    The problem is that with
your current system configuration
there isn't enough conventional
memory available to play Harpoon2.\
#nocona
    To solve this problem, you
will either need to remove some
device drivers and TSR's from your
CONFIG.SYS and AUTOEXEC.BAT files,
or load these drivers into upper
memory.  Menu programs such as DOS
Shell and virus scanners are good
examples of these programs which
use valuable memory.  Please refer
to the section in your H2
Installation and Information Guide
entitled, "Freeing More Memory -
Modifying CONFIG.SYS"\

#nocpup
   There is a problem in that
your CPU is unable to support
Harpoon II. Please note that
the minimum system requirements
for Harpoon II include a 386sx
based processor or better, 4MB of
RAM, DOS version 5.0 or later,
and a 512K Video Card which is
VESA compatible.\
#nocpua
   The only solution to this
problem is to acquire a 386sx based
processor or better.  Press the
right mouse button or the 'Esc' key
to exit.\

#nodosp
   The problem is that your current
DOS Version will not support
Harpoon II.
If you are installing under OS/2,
this may cause problems.  Please try
to install under DOS.\
#nodosa
   The only way to solve this
problem is to install DOS version
5.0 or later to your system.  If
you are running OS/2, try rebooting
to a DOS system.\

#welt
                   Welcome to the Harpoon II Cold War
                         Installation Program!

This program will install Cold War, as well as check your system
for any possible configuration problems.  If the installation program
detects any such problems, you will be given the opportunity to correct
them at the end of the installation process.

Please note that at any time during the installation of Cold War, you
may press the 'Esc' key or press the right mouse button to abort the
installation process.\

#clost
                        Installation Complete!
      You may now press any key to begin the Cold War Patch program.




               Thank You For Your Support of Three-Sixty




                          Installation Program
                      Published By Three-Sixty (c) 1995
         Three-Sixty is a registered Trademark of IntraCorp, Inc.\


#autot
During the installation of Cold War, our auto-detection program noted
some changes which need to be made to your CONFIG.SYS and AUTOEXEC.BAT
files before playing the Game.  If you would like us to automatically
make these changes to your CONIFG.SYS and AUTOEXEC.BAT files, please choose
Option 1.  Option 2 allows you to preview the changes before they are made.
Option 3 creates a boot diskette including AUTOEXEC.BAT and CONFIG.SYS
files that have the proper configuration to run Harpoon II. Please note
that your current CONFIG.SYS and AUTOEXEC.BAT files will be saved as
CONFIG.360 and AUTOEXEC.360 before any changes are made.\

#auto1
Press here to commence automatic configuration of your CONFIG.SYS
and AUTOEXEC.BAT files.\
#auto2
Press here to receive suggested changes only.\
#auto3
Press here to create a Boot Disk.\
#auto4
Press here to continue with no changes or recommendations.\
#endtext
Please remember to reboot your computer if you affected any changes to your
CONFIG.SYS or AUTOEXEC.BAT file via the Auto-Configure menu.

Harpoon II must be configured before playing.
Please run H2SETUP now.\
#success
Cold War has been successfully installed.

If there have been any recommended changes listed above, please make
them prior to running Harpoon II.


To begin playing, simply type: HARPOON2 from the HARPOON2 subdirectory.\
#updatetext

Press any key to integrate battleset data.

\
#updateerror
The battleset integration list was not found.
Don't Panic! Please contact tech support for assistance.\
#vesaerror
The installation program could not find a VESA driver for
your video card.  You will need to consult your video card
documentation and/or the manufacturer to learn how to load
the proper VESA driver.  The card's documentation should
contain the manufacturer's phone number and address.  If not
consult the retailer that sold you the card.

\
#memmngr
Your system configuration includes a memory manager such as EMM386,
QEMM, or 386MAX. These programs are not required and may affect the
performance of Harpoon II. If you have 4 megabytes of RAM, it is advised
that you disable your memory manager, since it will interfere with the
virtual memory system Harpoon II uses.  Prior to running, you will need
to alter your CONFIG.SYS removing the memory manager, and then reboot
your system.  Please consult your DOS manual for more information on
memory managers, and editing the CONFIG.SYS files if you are uncertain
how to make the changes.  Remember to reboot your machine prior to running
Harpoon II so the changes will take effect.
\

