***********************************************************************

                        IMPORTANT INFORMATION
                                 for
                        GRAPHICS WONDER Users
***********************************************************************
Release Notes                                            April 21, 1995
***********************************************************************

READ THIS FILE COMPLETELY BEFORE ATTEMPTING TO USE THIS PRODUCT !

ATI Technologies Inc.
33 Commerce Valley Drive East
Thornhill, Ontario
Canada L3T 7N6

Head Office, Sales and Marketing ....... (905) 882-2600
Corporate FAX .......................... (905) 882-2620

Customer Support (VOICE)................ (905) 882-2626
Customer Support FAX ................... (905) 882-0546

ATI DOWNLOAD BBS ....................... (905) 764-9404
                14400 bps, 9600 bps, 2400 bps, 1200 bps
                        (8 Data, 1 Stop Bit, No parity)
CompuServe ............................. GO ATITECH
      General Inquiries                  76004,3656
      Technical Support Inquiries        74740,667

****************************

Contents

1.0     Introduction
2.0     Adapter Installation
3.0     Contents of Distribution Diskette
4.0     Installation Notes for Windows 3.1
  4.1     Multimedia Video Acceleration
5.0     Installation Notes for AutoDesk products
6.0     Installation Notes for OS/2
7.0     Installation Notes for WordPerfect 
8.0     Installation Notes for Microsoft Word
9.0     Installation Notes for Lotus 1-2-3/Symphony
10.0     Installation Notes for MicroStation 
11.0     Driver Compatibility
12.0     Turbo Application Interface
13.0     Feature Changes
14.0    Reporting Problems

****************************

1.0     Introduction

This file contains last-minute updates that are not found in the User's
Guide or in any addendum accompanying the display adapter.  Please read
this file before proceeding with the installation.

For information on running the INSTALL program please refer to the following
sections in your User's Guide:

"CONFIGURING YOUR CARD"
"RUNNING THE INSTALL PROGRAM"

GENERAL INFO for NEW INSTALLATIONS:

- In order to match the card to your monitor and to your system
  configuration you must run "SET POWER UP CONFIGURATION" before installing
  any drivers
- Please refer to "MAIN SELECTION MENU" in your User's Manual.
- After running "SET POWER UP CONFIGURATION", run Install Device Drivers
  and EXIT back to DOS.


GENERAL INFO FOR UPDATE INSTALLATIONS:

If you are updating from a previous version of the mach32 Windows Driver
we suggest that:

A) You make a backup of you current WIN.INI and SYSTEM.INI prior to
   installation

B) You use the UNINSTALL WINDOWS DRIVER Option before installing the
   the new drivers. The UNINSTALL will remove any previous mach32 settings.

UNINSTALL PROCESS:

   a) Run the "INSTALL" program by inserting Disk #1 of the supplied mach32
      disks into the appropriate disk drive and run the INSTALL program.

   b) On the Main Menu Screen select the "INSTALL DEVICE DRIVER" and press
      ENTER.

   c) From the "Install Device Drivers" pop-up menu select
      "Microsoft Windows"

   d) After confirmation of directory and paths you will be presented with
      the "Windows Enhanced" pop-up menu. From this menu, select the
      appropriate "Uninstall" option and follow the directions on the Screen.

****************************

2.0     Adapter Installation

Adapter installation, while greatly simplified through the mach32 INSTALL
utility, requires a step by step methodical approach to ensure that the
adapter does not conflict with other system resources and that it will
provide optimal performance.

The following technical information is a basic outline of the steps required
to install a mach32 graphics adapter.

1)  The mach32 requires port addresses 2E0-2EF and 3A0-3DF.  It also uses
    C0000-C7FFF for VGA BIOS.

    Check the system hardware for internal modems, FAX cards or LAN cards
    which may be using addresses at COM4 (2E8) or addresses between the
    range of 2E0 to 2EF.

    Also ensure that LAN cards, scanner cards and other peripheral adapters
    are not using upper memory addresses between C000 and C7FF.

    If you have a system containing an on-board graphics controller, consult
    your owners manual on how to disable it.

    Check and record how much system memory is installed on the system
    motherboard.

2)  Review your CONFIG.SYS file to determine if a Memory Manager device
    driver is being loaded.

    Memory Manager device drivers, such as EMM386, QEMM and 386MAX, may
    interfere with the installation software and should not be loaded
    until the mach32 graphics adapter has been completely installed

3)  After powering down your system, remove your old graphics adapter (or
    disable the on-board graphics controller) and plug-in the mach32.

    Connect the monitor cable and mouse cable (if applicable) to the
    mach32 card and power-up the system.

    NOTE: Not all mach32 cards have built-in Mouse ports.

    If the system fails to produce text on the monitor, return to Step 1
    and re-check the installed hardware for address conflicts.

    If no obvious conflicts are present, carefully remove all non-
    essential peripheral adapters (scanner, FAX/modem, audio, CD ROM cards,
    etc.) to determine the nature of the conflict.

    As a last resort, if possible, see if the card works in a different
    system.

4)  Once the system has properly booted, place Disk #1 of the supplied mach32
    disks into the appropriate disk drive and run the INSTALL program.

    The INSTALL program may report that it has found the graphics card to
    be in a "new or changed configuration".  If this message appears, press
    any key to have the INSTALL program update the mach32 EEPROM.

    NOTE: The screen will flicker for a few seconds during a configuration
          change.

    If the INSTALL program returns to DOS and states that it could not find
    a mach32 based graphics card in the system, return to Step 3 to remove
    any memory manager device driver from your CONFIG.SYS file.


****************************

3.0     Contents of Distribution Diskette

The following files are on the distribution diskettes. The files are
decompressed into the appropriate directories by the INSTALL utility.

Disk #1
    README              This file
    README.COM          Utility to read the README file
    INSTALL.EXE         Main install program
    INSTALL.HLP         Help file for INSTALL.EXE
    INSTALL.VSF         Control file for INSTALL.EXE
    MONITOR.DAT         Control file for INSTALL.EXE
    SCRN_ADJ.EXE        Part of install.  Do not run.
    !ATI4421.CFG        EISA configuration file for ISA boards
    !ATI4431.CFG        EISA configuration file for VLB boards
    C-INFO.EXE          Video Technical Information Program
    LHARC.EXE           Disk archiving tool
    TEST.EXE            Video Accelerator Diagnostics Program
    UTILITY.LZH         Video Adapter Utilities archive
    ACAD
        ACADINST.EXE    Part of install.  Do not run.
        ACADINST.HLP    Help file for ACADINST.EXE
        DLXPRESS.LZH    AutoCAD drivers archive
    LOTUS
        INST123.EXE     Part of install.  Do not run.
        INST123.HLP     Help file for INST123.EXE
        LOTUSDRV.LZH    Lotus 1-2-3 drivers archive
    USTATION
        USINST.EXE      Part of install.  Do not run.
        USINST.HLP      Help file for USINST.EXE
        USDRIVER.LZH    Microstation drivers archive

Disk #2
    LHARC.EXE           Disk archiving tool
    VIDEO
        TIMEWARP.LZH    Multimedia Video Acceleration drivers archive
        WINVIDS.LZH     Multimedia Video Acceleration drivers archive
        WINVIDW.LZH     Multimedia Video Acceleration drivers archive
    WINDOWS
        WININST.EXE     Part of install.  Do not run.
        WININST.HLP     Help file for WININST.EXE
        MACHW.LZH       Windows drivers archive
        MACHE.LZH       Windows drivers archive
        MACHS.LZH       Windows drivers archive

Disk #3
    LHARC.EXE           Disk archiving tool
    FONTS
        GSFONTS.LZH     Crystal Fonts archive
    HDIPCDOS
        AI.LZH          Application Interface archive
    PM
        PMINST.EXE      Part of install.  Do not run.
        PMINST.HLP      Help file for PMINST.EXE
        OS2DRV.LZH      OS/2 drivers archive
    WORD
        WORDINST.EXE    Part of install.  Do not run.
        WORDINST.HLP    Help file for WORDINST.EXE
        WORDRVRS.LZH    Word for DOS drivers archive

****************************

4.0     Installation Notes for Windows 3.1

1) Run INSTALL from Disk #1 of the mach32 diskettes.

2) Select Install Device Drivers from the Main Selection Menu.

3) From the Install Device Drivers menu select Microsoft Windows.

4) Select INSTALL Windows 3.1 driver:

    a) Select Display Drivers only
       - if you have NOT installed Windows based multimedia applications
         (e.g. Multimedia CD-ROMS, Video editing packages)

    b) Select Display Drivers + Video drivers
       - if you have installed Windows based multimedia applications
         (e.g. Multimedia CD-ROMS, Video editing packages)
       - Note:  INSTALL will not successfully install the Video drivers
         unless it detects that Video for Windows has already been installed.

5) Follow the screen instructions to completion.

6) When INSTALL reports that the driver has been successfully installed,
   exit the INSTALL program using the <escape> key.

7) Start Windows, use the mach FlexDesk Control Panel icon to configure
   Windows for the desired resolution and color depth.

Note:  If you wish to change the Windows' display driver, to a different
       driver (i.e. VGA or 8514a), do not use the Windows' Setup icon within
       Windows.  To change the display, exit Windows and change directory
       to the Windows subdirectory.  When at the Windows prompt type SETUP
       and select the desired display driver.

For further information regarding the mach32 Windows functions please use
MS Write to read the MACH.WRI file.  This Write file is copied to the
ATI\ATIDESK (default) directory specified during install.

4.1     Multimedia Video Acceleration

In order to take advantage of ATI's Multimedia Video Acceleration, you will
require one of the following:

- Microsoft Video for Windows 1.0 or 1.1
- Microsoft Video for Windows 1.1 run-time

Microsoft Video for Windows 1.1 run-time is available from the following
sources as a self-extracting file called VFW11A.EXE:

- On CompuServe, GEnie, and Microsoft OnLine.  VFW11A.EXE is located in the
  Microsoft Software Library.  You can find VFW11A.EXE in the Software
  Library by searching on the word VFW11A.EXE.  On CompuServe, you can also
  get VFW11A.EXE through the Video for Windows library (use "GO WINMM").
- By Modem.  Use the Microsoft Download Service which you can reach by
  calling (206) 936-6735.  The highest download speed available is 14,400
  bits per second.
- On the Internet.  VFW11A.EXE is located on the Microsoft anonymous ftp
  server, which you can reach by typing "ftp ftp.microsoft.com" (without
  the quotation marks) at the ">" command prompt.

Once you obtain VFW11A.EXE, perform the following steps:

1. Copy VFW11A.EXE to an empty directory and expand it by typing "VFW11A.EXE"
   (without quotation marks) at the DOS prompt.  You will now have a file
   called SETUP.EXE.
2. Start Windows.
3. In Program Manager, choose Run from the File menu.
4. In the Command Line box, type the path to the SETUP.EXE file you expanded
   from VFW11A.EXE.  For example:
       c:\download\setup.exe
5. Setup will install the Video for Windows run-time.

Follow the Installation Notes for Windows 3.1 and select Display Drivers 
+ Video driver to enable Multimedia Video Acceleration.

****************************

5.0     Installation Notes for AutoDesk products

Note:   The following applications are supported:
        AutoCAD R10, R11, R12 (Protected Mode only); 3D Studio R2 and
        AutoShade 386 with Renderman.

1) Run INSTALL from Disk #1 of the mach32 diskettes.

2) Select Install Device Drivers from the Main Selection Menu.

3) From the Install Device Drivers menu select one of the following:

        AutoCAD
        AutoDesk 3D Studio
        AutoShade

4) Follow the screen instructions to completion.

5) When the INSTALL reports that the driver has been successfully installed,
   hit <escape> to exit the INSTALL program.

6) All the AutoDesk products require environment variables to be loaded
   prior to starting the application.  The INSTALL program creates
   batch files that contain all the necessary SET statements.  These
   batch files will be located in the directory specified during the
   driver installation. The following are the default batch file names:

        AutoCAD R10, R11 and R12        ADIACAD.BAT
        AutoDesk 3D Studio R2           ADI3DS.BAT
        AutoShade with Renderman        ADISHADE.BAT

7) After running the appropriate batch file, refer to your AutoDesk
   documentation for information on how to select and reconfigure the
   display driver.

For further details, please see README.DLX after installing the drivers.

****************************

6.0     Installation Notes for OS/2

1) Insert disk #1 and run INSTALL from within a full screen DOS session
   (under OS/2) and check "Set Power-up Configuration", to ensure that you
   have selected an appropriate monitor type:

    a) OS/2 requires that the 640x480 resolution be configured for the IBM
       default 60Hz vertical refresh rate.
    b) You must configure the card for all resolutions that your monitor
       can support in order to have them functioning correctly under OS/2.
       Only those resolutions that you have configured will display
       correctly.

2) Check The Minimized Window Viewer to see if you have any WIN-OS/2 or
   DOS sessions iconized. Close them all as the INSTALL may not work
   if a WIN-OS/2 session is running.

Note: Do not task switch while running the INSTALL program.

3) From the INSTALL Main Selection Menu, select Drivers Installation and
   pick Presentation Manager.  Then follow the instructions given on the
   screen.

Note:  If PM Desktop does not reappear after exiting from the full screen
       DOS session, pressing <Enter> will bring you back to full screen.
       You must reboot to get back to the PM Desktop.


4) Run DSPINSTL from within an OS/2 window.

5) When the Display Driver Install panel appears, select Primary Display
   and click OK to bring up a list of choices.  You should see an option for
   ATI mach32.

7) Select 'ATI Technologies mach32' from the list and click OK. Ignore the
   error message pop-up which says "The installed adapter does not support
   the selected display driver.  Do you wish to continue?" and click OK.

8) When the source directory panel appears, select 'Change' and enter:
   C:\MACH_OS2 (replace c: with your boot drive letter if you don't use c)
   Click 'Set' and then 'Install'. After the files are copied, exit the OS/2
   window or full screen session. Shut down and restart your system.

9) The PM driver will first come up in 640x480, 256 colors mode.  Use the
   following steps to change the screen resolutions or number of colors:

   a) Open 'OS/2 System' icon.
   b) Open 'System Setup' icon.
   c) Open 'System' icon.
   b) Select the 'Screen' tab.
   e) Select the desired resolution and number of colors from the list.
   f) Double click on the system menu icon or select close from the system
      menu to close the window.
   g) Shut down and restart your system.

NOTE:    Changing Refresh Rates

When changing refresh rates of 640x480 resolution using the mach32
installation diskettes from a DOS full screen window, the computer freezes
up.  IBM OS/2 must use 60 Hz VGA frequency since it sets the registers
directly.  This is a design limitation of OS/2 and only applies to the
640x480 resolution. Other resolutions may be configured at any vertical
refresh rate.

****************************

7.0     Installation Notes for WordPerfect 

WordPerfect drivers support 800x600 and 1024x768 resolutions in 16 colors,
VGA mode for Print Preview.

1) Make sure that WordPerfect has already been installed on your hard drive.

2) To complete the install successfully, you will require the following
   information:

   a) The full path name of the WordPerfect directory.

3) From the Install Device Drivers menu select WORDPERFECT.

4) Select WordPerfect and follow the screen instructions to completion.

5) When the INSTALL reports that the driver has been successfully installed, 
   exit the program.

6) Change directory to the WordPerfect subdirectory and run WordPerfect.

7) Select display driver in Setup option <shift><F1>.

8) Press <D> for Display.

9) Press <G> for Graphics Screen Type.

10) Select the desired resolution.

****************************

8.0     Installation Notes for Microsoft Word

Microsoft Word drivers support 800x600 and 1024x768 resolutions in 16 
colors, VGA mode for Print Preview.

1) Make sure that Word has already been installed on your hard drive.

2) To complete the install successfully, you will require the following
   information:

   a) The full path name of the Word for DOS directory.

3) From the Install Device Drivers menu select MICROSOFT WORD.  

4) Select Microsoft Word from the menu and follow the screen instructions 
   to completion.

5) When INSTALL reports that the driver has been successfully installed, 
   exit the program.

6) Change to your Word directory and start Word.

7) Word's print preview function will automatically use the highest 
   resolution installed. 

Note: If the high resolution page preview mode is not available, (i.e.
      the mach32 has not been configured to support high resolutions)
      the VGA 640x480 16 color mode will be used.

****************************

9.0     Installation Notes for Lotus 1-2-3/Symphony

The Lotus driver supports:

Lotus 1-2-3 version 2.0, 2.01, 2.1 and 2.2;
Symphony version 1.1 to 2.x

For VGA text modes:     132x25 and 132x44 in 16 colors;
                        132x44 in 2 colors

1) Make sure that Lotus has already been installed on your hard drive.

2) To complete the install successfully, you will require the following
   information:

   a) The full path name of the Lotus directory.

3) From the Install Device Drivers menu select Lotus 1-2-3.  

4) Select a program version, , for example, Lotus 1-2-3 version 2.2.

5) Follow the on screen instructions to completion.

6) When INSTALL reports that the driver has been successfully installed, 
   exit the program.

7) The driver installation is now complete. Remember to run the Lotus 1-2-3/
   Symphony setup program to update the configuration files; only then can 
   you use the driver you just installed.

****************************

10.0     Installation Notes for MicroStation 
 
1) Make sure MicroStation has already been installed on your hard drive.

2) To complete the install successfully, you will require the following
   information:

    a) The full path name of the MicroStation directory.
    
3) From the Install Device Drivers menu select MicroStation.

4) When INSTALL has completed copying all necessary files, exit the 
   program.  

5) Reboot the system (if you allowed INSTALL to modify autoexec.bat).  If
   you have created a batch file for the set environment, run the .BAT file.

6) Change directory to the MicroStation subdirectory and run USCONFIG.EXE.

7) Refer to the README.USD file for further information regarding how to 
   use the enhanced features.  This readme file is copied to the 
   MicroStation DRIVERS subdirectory during the drivers install.

****************************

11.0     Driver Compatibility

The mach32 accelerator supports more software drivers than any other 
graphics card. This flexibility means that the mach32 accelerator is 
compatible with virtually any software application right out-of-the-box. 
The supported drivers are:

*       mach32
*       VGAWONDER+
*       IBM VGA
*       VESA Super VGA

These drivers differ by the degree of acceleration, resolution and colors 
supported.


****************************

12.0     Turbo Application Interface

The mach32 Turbo Adapter Interface (Turbo AI) is a programming interface 
written exclusively for the mach32 accelerator chip. This AI provides 
access to the mach32 graphics controller by providing a "call interface" 
to programs performing display functions in the 8514/A-compatible part 
of the graphics card. This Turbo AI is 100% compatible with the IBM 8514/A 
adapter interface.

The Turbo AI is only supported on 2MB Graphics Wonder product. Attempting 
to use the Turbo AI on a 1MB card may result in displays problems.

Any application that needs an AI will ask for a TSR (Terminate-and-Stay-
Resident) program called HDILOAD.EXE. This TSR is supplied on a diskette 
that comes with your mach32 accelerator. Install this TSR only if you use 
applications that specifically use an 8514/A adapter interface.

There are two categories of software drivers that support the IBM 8514/A 
graphics adapter -- Direct-to-Registers and Adapter Interface. They are 
described as follows:

Direct-to-Registers:
The direct-to-registers driver writes directly to the registers of the 
graphics controller. Examples of such applications are MS Windows and 
IBM OS/2 Presentation.

Adapter Interface
Many applications access the 8514/A graphics controller using a software 
interface called the 8514 Adapter Interface (AI). Examples are Lotus 1-2-3, 
WordPerfect, and Turbo Pascal. These and many other applications use the AI 
to eliminate the need for separate graphics drivers for different 
applications. Contact your application program vendor for information on 
AI support.


Installing the Turbo AI:
1.      Run the mach32 INSTALL program to bring up the Main Selection Menu.
2.      Select Install Adapter Interface from the menu.
3.      Although the AI files can be copied to any directory on the hard 
        drive, certain applications require that the AI must be in a 
        directory called \HDIPCDOS. We recommend that you accept \HDIPCDOS 
        as prompted by the installation program. If this directory does not 
        exist on the drive, one will be created. Press<Enter> to continue.
4.      Accept the Source (drive and directory) as prompted, or type in 
        the location where these files can be found. Insert the appropriate 
        disk and press <Enter> to start copying.
5.      The installation program attempts to modify your PATH statement to 
        include the AI directory. It also attempts to add a line in the 
        AUTOEXEC.BAT file so that the AI is loaded automatically on every 
        power-up. Press <Y> if you want the AI in the PATH and automatic
        loading.
6.      When the AI installation is complete, press <Esc> to exit.

Using the Turbo AI:
If you prefer to load the Turbo AI manually, type:
C:\HDIPCDOS\HDILOAD\<Enter>
To unload the Turbo AI, type:
C:\HDIPCDOS\HDILOAD\UNLOAD<Enter>

Note
-  Application programs that use "AI" will display an error message if the 
   AI is not present prior to starting the application.
-  The order of TSR program unloading (if you have more than one) from DOS 
   memory is important. The last TSR loaded must be the first one you unload. 
   Therefore, HDILOAD must be the last TSR loaded in order for you to unload 
   it successfully.


****************************

13.0     Features Changes

- New VESA 75Hz Refresh Modes:

    ATI has adopted the 75Hz vertical refresh rate modes which have been
    recently standardized by the Video Electronics Standards Association
    (VESA).  Where applicable, these new modes will replace the previous
    76Hz modes at 640x480, 800x600 and 1024x768 and the 74Hz mode at
    1280x1024.

    To access any of these modes, use the following steps:

    1.  Run the "INSTALL" program by inserting Disk #1 of the supplied mach32
        disks into the appropriate disk drive and run the INSTALL program.
    2.  From the Main Selection Menu, select Set Power-Up Configuration
    3.  Under the Set Power-Up Configuration menu, select Monitor Type
    4.  Under the Monitor Type menu, select either:
            VESA standard 75Hz
    5.  Save your monitor selection by pressing <F10>
    6.  From the Main Selection Menu, re-select Set Power-Up Configuration
    7.  Under the Set Power-Up Configuration menu, select Monitor Type
    8.  Under the Monitor Type menu, select the Custom... option
    9.  For each resolution, you must specify the vertical refresh rate.
        You will notice that the refresh rate which you have specified in
        step 4 will now be listed as an option, if it is available at that
        resolution.

WARNING!
If the box outline in the Adjustment Screen becomes scrambled, press 
< Esc > immediately to exit, then try a lower refresh rate.

For further information on using the Custom option, refer to the Monitor 
and Video Modes chapter of your User's Guide. 

    Note:  Your existing refresh rates will remain unchanged (i.e. may
           continue to use 74 or 76Hz refresh) until you re-run INSTALL
           (version 1.1) and select and save a new Monitor Type under
           Set Power-Up Configuration.


- VDIF.EXE Utility:

    VDIF files are monitor definition files which conform to the VESA Display
    Information Format.  They define parameters which provide optimal
    resolution and refresh rate for the specified monitor.  If your monitor
    type is not already defined in the monitor list of the mach32 INSTALL
    program, having the VDIF file for your monitor will save you time.
    Please note that VDIF files are provided by your monitor manufacturer and
    they may not be available for all makes and models.

    VDIF.EXE is a mach32 software utility which takes a VDIF monitor
    definition file and converts it into an entry in the monitor list
    of the mach32 INSTALL program.  For complete instructions on using
    VDIF.EXE, consult README.VDI in your mach32 Utilities subdirectory
    (default is C:\MACH32).

- Memory Aperture:

    The Memory Aperture is not user configurable on ISA GRAPHICS WONDER 
    product.

- Accelerated Video Playback:

    ATI Multimedia Video Acceleration now supports the accelerated
    playback of video clips based on the following compression schemes:

        Intel Indeo 2.1
        Intel Indeo 3.1
        Microsoft Video 1
        Microsoft RLE
        Cinepak


****************************

14.0     Reporting Problems

TECHNICAL SUPPORT

If you experience any problems, please report them to ATI Customer Support
by fax (using the attached form) or by CompuServe.

Make multiple photocopies of the form and use a separate form for each
problem being reported. Please mail or fax your completed forms to us
as soon as possible.

PROBLEM REPORT FORM

Please complete this form and return it to ATI Technologies Inc. at the
address or fax number listed below, or return via CompuServe. Make multiple
copies of this form.

Please attach C-INFO output to all problem reports submitted. Use a
separate form for each problem being reported.

ATI Technologies Inc.
33 Commerce Valley Drive East
Thornhill, Ontario
CANADA. L3T 7N6

FAX:  (905) 882-0546

Product Name:
Bios P/N #:
Customer Name:
CompuServe Address:
Fax Number:
Address:

My Hardware is Configured as follows:
CPU/Speed:
Memory:
Video Capture Adapter (Make and Model):
Audio Adapter (Make and Model):
CD-ROM Drive (Make and Model):
Software:


Other system/software Information:


Problem description:





If you are sending any dumps, test cases or documentation associated
with this problem, list them here:






