uP = 8088
input filename = testyn
header = TESTYN with sample2.def file
xref = on

none

sega:0028 loc  begin_program
sega:0043 loc  exit
segc:0000 sub  beeper         Beep the speaker once    
segc:002C da, R 0C  yes_no_message        ;(note: "R 0C" is for 12 characters)
segc:0038 dw  speaker_port    I/O port for the speaker
segc:003A dw  on_off_time     Duration of speaker on/off
segc:003C dw  beep_cycles     Number of on/off cycles

