> # SANE-umax backend

- Index
- Frontend options:
  - Standard options
  - Advanced options
- Supported scanners:
  - Power Look series
  - Mirage series
  - Astra series
  - Vista series
  - UC series
  - others
  - Not listed scanners
  - UMAX scanner clones
- UMAX parallel port scanners
- Configuration
- Speed of UMAX scanners
- SANE-umax homepage
- SANE homepage
- XSane homepage

> Used System:
> CPU | AMD K6-III/400
> RAM | 128MB
> SCSI-Controller | NCR/Symbios logic 53C810
> Scanner | UMAX Supervista S12

> RGB scan 24 bits/pixel
> Resolution/dpi | Size(h x v)/cm | size/MB | time/min:sec | remark
> |  |  | 0:13 | calibration
> 100 | 21.6 x 29.7 | 2.8 | 0:30 |
> 200 | 21.6 x 29.7 | 11.3 | 0:30 |
> 300 | 21.6 x 29.7 | 25.5 | 0:35 |
> 400 | 21.6 x 29.7 | 45.5 | 1:00 | some backtracks
> >=500 | 21.6 x 29.7 |  | too long | not usable
> 500 | 9.0 x 13.0 | 12.9 | 0:30 |
> 600 | 9.0 x 13.0 | 18.6 | 0:30 |
> 700 | 9.0 x 13.0 | 25.4 | 0:55 |
> 1200 | 9.0 x 13.0 | 74.4 | 5:20 | lots of backtracks

> Grayscale scan 8 bits/pixel
> Resolution/dpi | Size(h x v)/cm | size/MB | time/min:sec | remark
> |  |  | 0:10 | calibration
> 100 | 21.6 x 29.7 | 1.0 | 0:25 |
> 200 | 21.6 x 29.7 | 3.7 | 0:30 |
> 300 | 21.6 x 29.7 | 8.5 | 0:30 |
> 400 | 21.6 x 29.7 | 15.0 | 0:30 |
> 500 | 21.6 x 29.7 | 23.7 | 0:35 |
> 600 | 21.6 x 29.7 | 34.1 | 0:45 | some backtracks
> 700 | 21.6 x 29.7 | 46.4 | 0:50 | some backtracks
> 800 | 21.6 x 29.7 | 60.6 | 1:20 | some backtracks
> 900 | 21.6 x 29.7 | 76.8 | 1:35 | some backtracks
> 1000 | 21.6 x 29.7 | 94.8 | 1:40 | some backtracks
> 1100 | 21.6 x 29.7 | 114.7 | 1:40 | some backtracks
> 1200 | 21.6 x 29.7 | 136.5 | 1:40 | some backtracks

> Lineart scan 1 bit/pixel
> Resolution/dpi | Size(h x v)/cm | size/MB | time/min:sec | remark
> |  |  | 0:07 | calibration
> 100 | 21.6 x 29.7 | 0.122 | 0:20 |
> 1200 | 21.6 x 29.7 | 17.0 | 0:40 |

This page has been changed on 12th. february 2001

> Author: Oliver Rauch