> # SANE-umax advanced options

- Index
- Frontend options:
  - Standard options
  - Advanced options
- Supported scanners:
  - Power Look series
  - Mirage series
  - Astra series
  - Vista series
  - UC series
  - others
  - Not listed scanners
  - UMAX scanner clones
- UMAX parallel port scanners
- Configuration
- Speed of UMAX scanners
- SANE-umax homepage
- SANE homepage
- XSane homepage

> This backend dynamically enabeles the options that are supported by the scanner in dependence of the scanning-mode and other options. Here is an example of the frontend XSane:

> Advanced options | Remark
> Set exposure time | Enable selection of exposure time, if not enabled, scanner uses default values. *
> Cal. exposure time | Define exposure time for calibration. *
> Scan exposure time | Define exposure time for scan. *
> Set lamp density | Enable selection of lamp density, if not enabled, scanner automatically selects a value. *
> Cal. lamp density | Define lamp density for calibration. *
> Set scan lamp density | Enable selection of lamp density for scan, if not enabled scanner uses the value that was used for calibration. *
> Scan lamp density | Define lamp density for scan. *
> lamp on | Turn on scanner lamp. *
> lamp off | Turn off scanner lamp. *
> lamp off at exit | Turn off scanner lamp when program exits (when sane_close is called) *

> * only available for some scanners

This page has been changed on 5th. february 2001

> Author: Oliver Rauch