sane-lexmark(5)

NAME
sane-lexmark - SANE backend for Lexmark X1100/X1200 Series scanners

DESCRIPTION
The sane-lexmark library implements a SANE (Scanner Access Now Easy) backend that provides access to the scanner part of Lexmark X1100/X1200 AIOs. This backend should be considered beta-quality software!

The scanners that should work with this backend are:

       Vendor Model           status
    ----------------------  -----------
      Lexmark X74             good
      Lexmark X1110           untested
      Lexmark X1140           untested
      Lexmark X1150           good
      Lexmark X1170           good
      Lexmark X1180           good
      Lexmark X1185           complete
      Lexmark X12xx           good in USB1.1,
      			  not fully tested in USB2.0
      Dell    A920            good
The options the backend supports can either be selected through command line options to programs like scanimage or through GUI elements in xscanimage or xsane.
If you have any strange behavior, please report to the backend maintainer or to the SANE mailing list. Valid command line options and their syntax can be listed by using
    scanimage --help -d lexmark:usb:<usb port>

Scan Mode Options

--mode
    selects the basic mode of operation of the scanner valid choices are Color, Gray and Lineart The default mode is Color. The Lineart mode is black and white only (1 bit). Grayscale will produce 256 levels of gray (8 bits). Color mode allows for over 16 million different colors produced from 24 bits of color information.

--resolution
    selects the resolution for a scan. The horizontal and vertical resolutions are set by the value of this option. The scanner is capable of the following resolutions for the specified option value:

      Value   Hor. Resolution  Vert. Resolution
      -----   ---------------  -------------------
      75      75dpi            75dpi
      150     150dpi           150dpi
      300     300dpi           300dpi
      600     600dpi           600dpi
      1200    600dpi           1200dpi  (only for X11xx models with 'B2' sensor)

--preview
    requests a preview scan. The resolution used for that scan is 75 dpi and the scan area and the scan mode are as specified through their options, or the default if not specified. The default value for preview mode is "no".

--threshold
    selects the minimum-brightness to get a white point. The threshold is only used with Lineart mode scans. It is specified as a percentage in the range 0..100% (in steps of 1). The default value of the threshold option is 50.

CONFIGURATION FILE
The configuration file /sane/etc/sane.d/lexmark.conf contains only the usb device id (eg usb 0x043d 0x007c).

FILES

/sane/lib/sane/libsane-lexmark.a
    The static library implementing this backend.

/sane/lib/sane/libsane-lexmark.so
    The shared library implementing this backend (present on systems that support dynamic loading).

ENVIRONMENT

SANE_DEBUG_LEXMARK
    SANE_DEBUG_LEXMARK_LOW If the library was compiled with debug support enabled, this environment variable controls the debug level for this backend. E.g., a value of 255 requests all debug output to be printed. Smaller levels reduce verbosity.

LIMITATIONS
The windows TWAIN driver has many more options than this SANE backend. However they are only software adjustments. This backend only implements what the scanner can support. For instance, shading correction (vertical stripes due to sensor variation across its width) is done in software. Head park position is also detected by software. The data compression isn't supported for the X1200 serie on USB 1.1, leading to slow scans.

BUGS
No bugs currently known.

SEE ALSO
sane-scsi(5), scanimage(1), xscanimage(1), xsane(1), sane(7)

AUTHOR

The backend was originaly written by Fred Odendaal.
    http://ca.geocities.com/freshshelf@rogers.com/

The new version is currently developped by Stéphane Voltz.
    http://stef.dev.free.fr/sane/lexmark

X74 support was written by Torsten Houwaart (<ToHo@gmx.de>)

CREDITS

Many thanks go to:
    Julien Furgerot who lend me a Dell A920. Robert Price, Dani Ele and Dalai Felinto for the time they spent recording USB activity and testing the experimental version.