sane-s9036(5)

NAME
sane-s9036 - SANE backend for Siemens 9036 flatbed scanners

DESCRIPTION
The sane-s9036 library implements a SANE (Scanner Access Now Easy) backend that provides access to Siemens 9036 flatbed scanners.

DEVICE NAMES
This backend expects device names of the form:

    special

Where special is the path-name for the special device that corresponds to a SCSI scanner. The special device name must be a generic SCSI device or a symlink to such a device. The program sane-find-scanner helps to find out the correct device. Under Linux, such a device name could be /dev/sga or /dev/sge, for example. See sane-scsi(5) for details.

FILES

/sane/etc/sane.d/s9036.conf
    The backend configuration file (see also description of SANE_CONFIG_DIR below).

/sane/lib/sane/libsane-s9036.a
    The static library implementing this backend.

/sane/lib/sane/libsane-s9036.so
    The shared library implementing this backend (present on systems that support dynamic loading).

ENVIRONMENT

SANE_CONFIG_DIR
    This environment variable specifies the list of directories that may contain the configuration file. Under UNIX, the directories are separated by a colon (`:'), under OS/2, they are separated by a semi-colon (`;'). If this variable is not set, the configuration file is searched in two default directories: first, the current working directory (".") and then in /sane/etc/sane.d. If the value of the environment variable ends with the directory separator character, then the default directories are searched after the explicitly specified directories. For example, setting SANE_CONFIG_DIR to "/tmp/config:" would result in directories "tmp/config", ".", and "/sane/etc/sane.d" being searched (in this order).

SANE_DEBUG_S9036
    If the library was compiled with debug support enabled, this environment variable controls the debug level for this backend. Higher debug levels increase the verbosity of the output. Example: export SANE_DEBUG_S9036=4

SEE ALSO
sane(7), sane-scsi(5)

AUTHOR
Ingo Schneider