> # UMAX Mirage scanners

- Index
- Frontend options:
  - Standard options
  - Advanced options
- Supported scanners:
  - Power Look series
  - Mirage series
  - Astra series
  - Vista series
  - UC series
  - others
  - Not listed scanners
  - UMAX scanner clones
- UMAX parallel port scanners
- Configuration
- Speed of UMAX scanners
- SANE-umax homepage
- SANE homepage
- XSane homepage

UMAX scanners
Mirage series:
Name | SCSI-ID | Versions | UTA | ADF | B/W | Gray | Color | Bits/pixel | Resolution
Mirage | Mirage D-16L | all (2.7) | incl |  | ok | ok | ok | 1,8,10,24,30 | 400 x 800 800 x 1600*
Mirage II | Mirage II | all (1.6) | incl |  | ok | ok | ok | 1,8,12,24,36 | 700 x 1400 1400 x 2800
Mirage IIse | Mirage IIse | ? | incl |  | ? | ? | ? | 1,8,12,24,36 | 700 x 1400

* Mirage D-16L scanners allow scanning up to 800x800 / 1600x1600 dpi.

UTA = Umax Transparancy Adapter, ADF = Automatic Document Feeder
(X = supported by scanner, incl = is included)

This page has been changed on 12th. february 2001

> Author: Oliver Rauch