sane-umax1220u(5)

NAME
sane-umax1220u - SANE backend for the UMAX Astra 1220U and similar scanners

DESCRIPTION
The sane-umax1220 library implements a SANE (Scanner Access Now Easy) backend for the the UMAX Astra 1220U and similar scanners. For more information on this backend, please visit http://umax1220u-sane.sourceforge.net/.

UMAX ASTRA 1600U/2000U/2100U SUPPORT
This backend is also able to drive the UMAX Astra 1600U/2000U/2100U. The 2100U is confirmed to work. For the other scanners no reports have been received yet. Please contact us and tell us if your scanner works (sane-devel@lists.alioth.debian.org).

CONFIGURATION
Usually, no manual configuration is necessary. The configuration file for this backend resides in /sane/etc/sane.d/umax1220u.conf. Its contents is a list of device names that correspond to UMAX Astra scanners. Empty lines and lines starting with a hash mark (#) are ignored. A sample configuration file is shown below:
 #usb vendor product
 usb 0x1606 0x0010
 # Device list for non-linux systems
 /dev/scanner
 /dev/usb/scanner0
See sane-usb(5) for information on how to set the access permissions on the usb device files.

FILES

The backend configuration file:
    /sane/etc/sane.d/umax1220u.conf

The static library implementing this backend:
    /sane/lib/sane/libsane-umax1220u.a

The shared library implementing this backend:
    /sane/lib/sane/libsane-umax1220u.so (present on systems that support dynamic loading)

ENVIRONMENT

SANE_DEBUG_UMAX1220U
    If the library was compiled with debug support enabled, this environment variable controls the debug level for this backend. E.g., a value of 128 requests all debug output to be printed. Smaller levels reduce verbosity: SANE_DEBUG_UMAX1220U values
    Number  Remark

     1       print failures
     2       print information
     3       print high-level function calls
     4       print high-level function checkpoints
     9       print mid-level function calls
     10      print mid-level function checkpoints
     80      print protocol-level function entry
     90      print protocol-level function exit

Example:
    export SANE_DEBUG_UMAX1220U=10

KNOWN BUGS
600 dpi scanning may fail for large image sizes. If you keep getting I/O errors, try cycling the power on your scanner to reset it. There is no way to cancel a scan, since the driver ignores sane_cancel(). If you try scanning an image which is too small, you will get I/O errors. Be sure to adjust the scan area before doing a scan, since by default, the scan area is zero.

SEE ALSO
sane(7), sane-usb(5)

(Old) homepage:
    http://umax1220u-sane.sourceforge.net/

AUTHOR
Marcio Luis Teixeira <marciot@users.sourceforge.net>

EMAIL-CONTACT
sane-devel@lists.alioth.debian.org

REPORTING BUGS
This backend isn't actively maintained. Nevertheless, bug reports and comments should be sent to the sane-devel mailing list. When reporting bugs, please run the backend with SANE_DEBUG_UMAX1220U set to 10 and attach a copy of the log messages.