
OVERVIEW:
SP31728
HP ProLiant NC10XX/67XX/77XX/150X/320X Gigabit Server Adapter Firmware Upgrade Utility for MS-DOS
This utility (NICFWUPG.BAT) will upgrade NIC firmware as follows:

NC1020 Boot code version 3.18 and PXE code version 7.7.8.
NC6770 Boot Code version 2.19 and PXE code version 3.2.2.
NC7760 Boot Code version 2.37.
NC7761 Boot Code version 3.18.
NC7770 Boot Code version 2.19 and PXE code version 3.2.2.
NC7771 Boot Code version 2.35 and PXE code version 7.7.8.
NC7780 Boot Code version 2.19.
NC7781 Boot Code version 2.35 and IPMI code version 3.26.
NC7782 Boot Code version 3.27b and IPMI code version 3.26.
NC 150T Boot Code version 3.18
NC 320T Boot Code version 3.55a and PXE code version 8.3.9


INSTALLATION:

1) Copy these files to a bootable DOS diskette.

7781V235 BIN         8,192 03-02-04   9:48a
150TV318 BIN         8,192 07-28-04   9:38a
6770V219 BIN         8,192 11-23-03   4:57p
7760V237 BIN         8,192 03-02-04  10:19a
7761V318 BIN         8,192 03-02-04  10:55a
7770V219 BIN         8,192 11-23-03   4:57p
7771V235 BIN         8,192 03-02-04  10:08a
7780V219 BIN         4,096 03-02-04   9:54a
1020V318 BIN         8,192 01-22-04   5:34p
7782327B BIN         8,192 08-03-04  11:42a
NICFWUPG BAT         5,401 12-01-05   1:00p
PT5704C2 36         29,896 11-24-04   5:46p
PXE_V322 BIN        57,244 01-22-04   2:38p
Q57UDIAG EXE       260,559 12-09-04   4:42p
SP29044  TXT         3,424 02-15-05   9:47a
PXE_V778 BIN        65,212 02-07-05   7:37p
PXE_V839 BIN        56,100 11-29-05   7:39p
320TV355 BIN         8,080 11-29-05   7:09p         
 
2) Boot the system using the DOS diskette.

3) Run NICFWUPG.BAT from the command prompt. 


NOTES:

	o Before updating NC7770 or NC6770 NICs, Be sure to move jumper J1 to the Enable position.

	o This utility does NOT make a backup of your current firmware version.

	o This utility will update your firmware version if your current version of 
	  firmware is less than or equal to the most recent firmware version.

	o After updating NC7770 or NC6770 NICS, Be sure to move jumper J1 to the Disable position.



Here is a sample CONFIG.SYS 

dos=high
dos=umb                         
device=a:\himem.sys /verbose /testmem:off 
files=30
lastdrive=z
Stacks=40,512
Files=50
Buffers=50
fcbs=16,4



(c)Copyright 2001, 2005 Hewlett-Packard Development Company, L.P.

Hewlett-Packard Company shall not be liable for technical or editorial errors or omissions contained herein. The information in this document is provided "as is" without warranty of any kind and is subject to change without notice. The warranties for HP products are set forth in the express limited warranty statements accompanying such products. Nothing herein should be construed as constituting an additional warranty.
