/*  @(#)43    1.3  framer/os2/irda_phy.msg, framer, tor_irda_v1b, v2r2_648 10/31/96 15:08:06 */
^

<=== OS/2 IrDA Physical Driver ^ ===>
Copyright (C) IBM Corp. ^
Invalid command line option ^
Invalid prameter value ^

   IrDA_PHY Critical Error: Initialization failed
            The IrDA Physical driver did not load.

^   Phy driver UART Base:  ^
   Phy driver UART IRQ:   ^
   Phy driver SDLC Base:  ^
   Phy driver SDLC IRQ:   ^
   Phy driver Ram Base:   ^
   Phy driver RX Buffers: ^
Rx Buffer Size must be between 1 and 7 inclusive^
   Trace Buffer Size:   ^
The trace buffer size must either be 0 or > 16 and smaller than 20k.
^
   Data buffers moved to DMAable region
   Memory image increased by ^
   Phy driver Rx DMA:     ^
   Phy driver Tx DMA:     ^
Only DMA channels 0 and 3 are available for use by the IrDA driver.^
IR Subsystem is disabled.^
Low Speed IR is enabled.^
   IRDA_PHY Critical Error: Driver already installed.
            Remove multiple lines in CONFIG.SYS that load the IRDA_PHY driver.
            The second IrDA Physical driver did not load.

^
